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Status of this Memo
   By submitting this Internet-Draft, each author represents that any
   applicable patent or other IPR claims of which he or she is aware
   have been or will be disclosed, and any of which he or she becomes
   aware will be disclosed, in accordance with Section 6 of BCP 79.
   Internet-Drafts are working documents of the Internet Engineering
   Task Force (IETF), its areas, and its working groups.  Note that
   other groups may also distribute working documents as Internet-
   Drafts.
   Internet-Drafts are draft documents valid for a maximum of six months
   and may be updated, replaced, or obsoleted by other documents at any
   time.  It is inappropriate to use Internet-Drafts as reference
   material or to cite them other than as "work in progress."
   The list of current Internet-Drafts can be accessed at
   http://www.ietf.org/ietf/1id-abstracts.txt.
   The list of Internet-Draft Shadow Directories can be accessed at
   http://www.ietf.org/shadow.html.
   This Internet-Draft will expire on January 8, 2009.
Abstract
   This document defines a Management Information Base (MIB) module for
   use with network management protocols in the Internet community.  In
   particular, it describes objects used for managing parameters of the
   "Very High Speed Digital Subscriber Line 2 (VDSL2)" interface type,
   which are also applicable for managing ADSL, ADSL2, and ADSL2+
   interfaces.
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1.  The Internet-Standard Management Framework
   For a detailed overview of the documents that describe the current
   Internet-Standard Management Framework, please refer to Section 7 of
   RFC 3410 [RFC3410].
   Managed objects are accessed via a virtual information store, termed
   the Management Information Base or MIB.  MIB objects are generally
   accessed through the Simple Network Management Protocol (SNMP).
   Objects in the MIB are defined using the mechanisms defined in the
   Structure of Management Information (SMI).  This memo specifies a MIB
   module that is compliant to the SMIv2, which is described in STD 58,
   RFC 2578 [RFC2578], STD 58, RFC 2579 [RFC2579] and STD 58, RFC 2580
   [RFC2580].
   The key words "MUST", "MUST NOT", "REQUIRED", "SHALL", "SHALL NOT",
   "SHOULD", "SHOULD NOT", "RECOMMENDED", "MAY", and "OPTIONAL" in this
   document are to be interpreted as described in RFC 2119 [RFC2119].
2.  Overview
   This document defines a Management Information Base (MIB) module for
   use with network management protocols in the Internet community for
   the purpose of managing VDSL2, ADSL, ADSL2, and ADSL2+ lines.
   The MIB module described in RFC 2662 [RFC2662] describes objects used
   for managing Asymmetric Bit-Rate DSL (ADSL) interfaces per
   [T1E1.413], [G.992.1], and [G.992.2].  These object descriptions are
   based upon the specifications for the ADSL Embedded Operations
   Channel (EOC) as defined in American National Standards Institute
   (ANSI) T1E1.413/1995 [T1E1.413] and International Telecommunication
   Union (ITU-T) G.992.1 [G.992.1] and G.992.2 [G.992.2].
   The MIB module described in RFC 4706 [RFC4706] is a wider management
   model that includes, in addition to ADSL technology, the ADSL2 and
   ADSL2+ technologies per G.992.3, G.992.4, and G.992.5 ([G.992.3],
   [G.992.4], and [G.992.5] respectively).
   This document does not obsolete RFC 2662 [RFC2662], or RFC 4706
   [RFC4706] but rather provides a more comprehensive management model
   that addresses the VDSL2 technology per G.993.2 ([G.993.2]) as well
   as ADSL, ADSL2 and ADSL2+ technologies.
   Additionally, the management framework for VDSL2 lines [TR-129]
   specified by the Digital Subscriber Line Forum (DSLF) has been taken
   into consideration.  That framework is based on ITU-T G.997.1
   standard [G.997.1] and its amendment 1 [G.997.1-Am1].
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   Note that the management model, according to this document, does not
   allow managing VDSL technology per G.993.1 ([G.993.1]).  VDSL lines
   MUST be managed by RFC 3728 [RFC3728].
   The MIB module is located in the MIB tree under MIB 2 transmission,
   as discussed in the MIB-2 Integration (RFC 2863 [RFC2863]) section of
   this document.
2.1.  Relationship to other MIBs
   This section outlines the relationship of this MIB module with other
   MIB modules described in RFCs.  Specifically, IF-MIB as presented in
   RFC 2863 [RFC2863] is discussed.
2.1.1.  General IF-MIB Integration (RFC 2863)
   The VDSL2 Line MIB specifies the detailed attributes of a data
   interface.  As such, it needs to integrate with RFC 2863 [RFC2863].
   The IANA has assigned the following ifTypes, which may be applicable
   for VDSL2 lines as well as for ADSL, ADSL2 and ADSL2+ lines:
   IANAifType ::= TEXTUAL-CONVENTION
       ...
   SYNTAX INTEGER {
       ...
       channel(70),     -- Channel
       adsl(94),        -- Asymmetric Digital Subscriber Loop
       ...
       interleave(124), -- Interleaved Channel
       fast(125),       -- Fast Channel
       ...
       adsl2plus(238),  -- Asymmetric Digital Subscriber Loop Version 2,
                           Version 2 Plus, and all variants
       vdsl2(xxx),      -- Very High Speed Digital Subscriber Loop 2
       ...
       }
   ADSL lines that are identified with ifType=adsl(94) MUST be managed
   with the MIB specified by RFC2662.  ADSL, ADSL2, and ADSL2+ lines
   identified with ifType=adsl2plus(238) MUST be managed with the MIB
   specified by RFC 4706 [RFC4706].  VDSL2, ADSL, ADSL2, and ADSL2+
   lines identified with ifType=vdsl2(xxx) MUST be managed with the MIB
   specified by this document.
   In any case, the SNMP agent may use either ifType=interleave(124) or
   fast(125) for each channel, e.g., depending on whether or not it is
   capable of using an interleaver on that channel.  It may use the
   ifType=channel (70) when all channels are capable of using an
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   interleaver (e.g., for ADSL2 xTUs).
   Note that the ifFixedLengthGroup from RFC 2863 [RFC2863] MUST be
   supported and that the ifRcvAddressGroup does not apply to this MIB
   module.
2.1.2.  Usage of ifTable
   The MIB branch identified by ifType contains tables appropriate for
   the interface types described above.  Most such tables extend the
   ifEntry table, and are indexed by ifIndex.  For interfaces in systems
   implementing this MIB module, those table entries indexed by ifIndex
   MUST be persistent.
   The following attributes are part of the mandatory
   ifGeneralInformationGroup in the Interfaces MIB [RFC2863], and are
   not duplicated in the VDSL2 Line MIB.
      ifIndex                  Interface index.
      ifDescr                  See interfaces MIB.
      ifType                   vdsl2(xxx), channel(70),
                               interleave(124), or fast(125)
      ifSpeed                  Set as appropriate.
      ifPhysAddress            This object MUST have an octet
                               string with zero length.
      ifAdminStatus            See interfaces MIB.
      ifOperStatus             See interfaces MIB.
      ifLastChange             See interfaces MIB.
      ifName                   See interfaces MIB.
      ifAlias                  See interfaces MIB.
      ifLinkUpDownTrapEnable   Default to enabled(1).
      ifHighSpeed              Set as appropriate.
      ifConnectorPresent       Set as appropriate.
   -------------------------------------------------------------------
                     Figure 1: Use of ifTable Objects
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2.1.3.  Usage of ifStackTable
   Use of the ifStackTable to associate the entries for physical, fast,
   interleaved channels, and higher layers (e.g., ATM) is shown below.
   Use of ifStackTable is necessary, because configuration information
   is stored in profile tables associated with the physical-layer
   ifEntry only.  The channels' ifEntrys need the ifStackTable to find
   their associated physical-layer entry and thus their configuration
   parameters.  The following example shows the ifStackTable entries for
   an xDSL line with a single channel that uses an ATM data path.
                       HigherLayer      LowerLayer
                       -----------------------------
                            0               ATM
                           ATM           XdslChannel
                        XdslChannel      XdslPhysical
                        XdslPhysical         0
   Figure 2: ifStackTable entries for ATM path over a single xDSL
   channel
2.2.  IANA Considerations
   The VDSL2-LINE-MIB module requires the allocation of a new ifType
   value for Very High Speed Digital Subscriber Loop Version 2, to
   distinguish between ADSL lines that are managed with the RFC2662
   management model, ADSL/ADSL2 and ADSL2+ lines that are managed with
   the RFC 4706 [RFC4706] management model, and VDSL2/ADSL/ADSL2 and
   ADSL2+ lines that are managed with the model defined in this
   document.
   Also, the VDSL2-LINE-MIB module requires the allocation of a single
   object identifier for its MODULE-IDENTITY.  The IANA should allocate
   this object identifier in the transmission subtree.
   As performed in the past for the ADSL2-LINE-MIB module, the IANA is
   kindly requested to ensure that the allocated ifType value is the
   same as the allocated branch number in the transmission subtree.
2.3.  Conventions Used in the MIB Module
2.3.1.  Naming Conventions
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      atuc  ADSL/ADSL2 or ADSL2+ line termination unit -
            Central office
      atur  ADSL/ADSL2 or ADSL2+ line termination unit -
            Remote site
      CRC   Cyclic Redundancy Check
      DELT  Dual Ended Loop Test
      ES    Errored Second
      FEC   Forward Error Correction
      LOF   Loss Of Frame
      LOS   Loss Of Signal
      LOSS  LOS Seconds
      NSC   Highest transmittible subcarriers index
      NSCds NSC for downstream transmission direction
      NSCus NSC for upstream transmission direction
      PTM   Packet Transfer Mode
      SES   Severely-Errored Second
      SNR   Signal-to-Noise Ratio
      UAS   Unavailable Seconds
      US0   Upstream band number 0
      vtuc  VDSL2 line termination unit - Central office
      vtur  VDSL2 line termination unit - Remote site
      xTU-C ADSL/ADSL2/ADSL2+ or VDSL2 line termination unit -
            Central office
      xTU-R ADSL/ADSL2/ADSL2+ or VDSL2 line termination unit -
            Remote site
      xTU   A line termination unit; either an xTU-C or xTU-R
2.3.2.  Textual Conventions
   The following textual conventions are defined to reflect the line
   topology in the MIB module (further discussed in the following
   section), the various transmission modes, power states,
   synchronization states, possible values for various configuration
   parameters, status parameters, and other parameter types.
   o  Xdsl2Unit:
      Attributes with this syntax uniquely identify each unit in the
      VDSL2/ADSL/ADSL2/ADSL2+ link.  This mirrors the EOC addressing
      mechanism:
         xtuc(1)                - Central Office (CO) line termination
         unit.
         xtur(2)                - Remote site line termination unit.
   o  Xdsl2Direction:
      Attributes with this syntax uniquely identify a transmission
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      direction in a VDSL2/ADSL/ADSL2/ADSL2+ link.  The upstream
      direction is a transmission from the remote end (xTU-R) towards
      the central office end (xTU-C).  The upstream direction is
      indicated by upstream(1).  The downstream direction is a
      transmission from the xTU-C towards the xTU-R.  The downstream
      direction is indicated by downstream(2).
         upstream(1)        - Transmission from the xTU-R to the xTU-C.
         downstream(2)      - Transmission from the xTU-C to the xTU-R.
   o  Xdsl2Band:
      Attributes with this syntax uniquely identify a band in an ADSL,
      ADSL2, ADSL2+ or VDSL2 link.  For a band in the upstream
      direction, transmission is from the remote end (xTU-R) towards the
      central office end (xTU-C).  For a band in the downstream
      direction, transmission is from the xTU-C towards the xTU-R.  For
      ADSL, ADSL2 and ADSL2+ which use a single band in the upstream
      direction and a single band in the downstream direction, the only
      relevant values are upstream(1) and downstream(2).  For VDSL2,
      which uses multiple bands in each transmission direction, a band
      in the upstream direction is indicated by any of us0(3), us1(5),
      us2(7), us3(9), or us4(11) and a band in the downstream direction
      is indicated by any of ds1(4), ds2(6), ds3(8), or ds4(10).  For
      VDSL2, the values upstream(1) and downstream(2) may be used when
      there is a need to refer to the whole upstream or whole downstream
      traffic (e.g., report the average signal-to-noise ratio on any
      transmission direction).
       upstream(1)        - Transmission from the xTU-R to the xTU-C
                            (refers to the single upstream band for
                            ADSL/ADSL2/ADSL2+ or to the whole upstream
                            traffic for VDSL2).
       downstream(2)      - Transmission from the xTU-C to the xTU-R
                            (refers to the single downstream band for
                            ADSL/ADSL2/ADSL2+ or to the whole downstream
                            traffic for VDSL2).
       us0(3)             - Upstream band number 0   (US0) (VDSL2).
       ds1(4)             - Downstream band number 1 (DS1) (VDSL2).
       us1(5)             - Upstream band number 1   (US1) (VDSL2).
       ds2(6)             - Downstream band number 2 (DS2) (VDSL2).
       us2(7)             - Upstream band number 2   (US2) (VDSL2).
       ds3(8)             - Downstream band number 3 (DS3) (VDSL2).
       us3(9)             - Upstream band number 3   (US3) (VDSL2).
       ds4(10)            - Downstream band number 4 (DS4) (VDSL2).
       us4(11)            - Upstream band number 4   (US4) (VDSL2).
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   o  Xdsl2TransmissionModeType:
      Attributes with this syntax reference the list of possible
      transmission modes for VDSL2/ADSL/ADSL2 or ADSL2+.
      Specified as a BITS construct, there are currently a few dozen
      transmission modes in the list.
   o  Xdsl2RaMode:
      Attributes with this syntax describe how Rate-Adaptive
      synchronization is being used on the respective VDSL2/ADSL/ADSL2
      or ADSL2+ link:
         manual (1)    - No Rate-Adaptation.  The initialization process
                         attempts to synchronize to a specified rate.
         raInit (2)    - Rate-Adaptation during initialization process
                         only, which attempts to synchronize to a rate
                         between minimum and maximum specified values.
         dynamicRa (3) - Dynamic Rate-Adaptation during initialization
                         process as well as during SHOWTIME.
   o  Xdsl2InitResult:
      Attributes with this syntax report the recent result of a full
      initialization attempt:
         noFail (0)             - Successful initialization.
         configError (1)        - Configuration failure.
         configNotFeasible (2)  - Configuration details not supported.
         commFail (3)           - Communication failure.
         noPeerAtu (4)          - Peer ATU not detected.
         otherCause (5)         - Other initialization failure reason.
   o  Xdsl2OperationModes:
      Attributes with this syntax uniquely identify an xDSL mode, which
      is a category associated with each transmission mode defined for
      the VDSL2/ADSL/ADSL2 or ADSL2+ link.  Part of the line
      configuration profile depends on the xDSL Mode:
      Specified as an enumeration construct, there are currently a few
      dozen transmission modes in the list.
   o  Xdsl2PowerMngState:
      Attributes with this syntax uniquely identify each power
      management state defined for the VDSL2/ADSL/ADSL2 or ADSL2+ link.
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      For VDSL2 links only L0 and L3 states are supported:
         l0(1)       - L0: Full power management state.
         l1(2)       - L1: Low power management state (for G.992.2).
         l2(3)       - L2: Low power management state (for G.992.3,
                           G.992.4, and G.992.5).
         l3(4)       - L3: Idle power management state.
   o  Xdsl2ConfPmsForce:
      Attributes with this syntax are configuration parameters that
      reference the desired power management state for the VDSL2/ADSL/
      ADSL2 or ADSL2+ link.  For VDSL2, only L0 and L3 states are
      supported:
         l3toL0 (0)       - Perform a transition from L3 to L0 (Full
                            power management state).
         l0toL2 (2)       - Perform a transition from L0 to L2 (Low
                            power management state).
         l0orL2toL3 (3)   - Perform a transition into L3 (Idle power
                            management state).
   o  Xdsl2LinePmMode:
      Attributes with this syntax are configuration parameters that
      reference the power modes/states into which the xTU-C or xTU-R may
      autonomously transit.
      This is a BITS structure that allows control of the following
      transit options:
         allowTransitionsToIdle (0)    - xTU may autonomously transit
                                         to idle (L3) state.
         allowTransitionsToLowPower (1)- xTU may autonomously transit
                                         to low-power (L1/L2) state.
   o  Xdsl2LineLdsf:
      Attributes with this syntax are configuration parameters that
      control the Loop Diagnostic mode for the VDSL2/ADSL/ADSL2 or
      ADSL2+ link:
         inhibit (0)       - Inhibit Loop Diagnostic mode.
         force (1)         - Force/Initiate Loop Diagnostic mode.
   o  Xdsl2LdsfResult:
      Attributes with this syntax are status parameters that report the
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      result of the recent Loop Diagnostic mode issued for the VDSL2/
      ADSL/ADSL2 or ADSL2+ link:
        none        (1)   - The default value, in case LDSF was never
                            requested for the associated line.
        success     (2)   - The recent command completed successfully.
        inProgress  (3)   - The Loop Diagnostics process is in progress.
        unsupported (4)   - The NE or the line card doesn't support
                            LDSF.
        cannotRun   (5)   - The NE cannot initiate the command, due to
                            a nonspecific reason.
        aborted     (6)   - The Loop Diagnostics process aborted.
        failed      (7)   - The Loop Diagnostics process failed.
        illegalMode (8)   - The NE cannot initiate the command, due
                            to the specific mode of the relevant line.
        adminUp     (9)   - The NE cannot initiate the command because
                            the relevant line is administratively
                            'Up'.
        tableFull   (10)  - The NE cannot initiate the command, due to
                            reaching the maximum number of rows in the
                            results table.
        noResources (11)  - The NE cannot initiate the command, due to
                            lack of internal memory resources.
   o  Xdsl2LineBpsc:
      Attributes with this syntax are configuration parameters that
      control the bits per subcarrier measurement for the VDSL2/ADSL/
      ADSL2 or ADSL2+ link:
         idle (1)          - Idle state.
         measure (2)       - Measure the bits per subcarrier.
   o  Xdsl2BpscResult:
      Attributes with this syntax are status parameters that report the
      result of the recent bits per subcarrier measurement issued for
      the VDSL2/ADSL/ADSL2 or ADSL2+ link:
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        none        (1)   - The default value, in case a measurement
                            was never requested for the associated line.
        success     (2)   - The recent measurement request completed
                            successfully.
        inProgress  (3)   - The bits per subcarrier measurement is in
                            progress.
        unsupported (4)   - The bits per subcarrier request mechanism
                            is not supported.
        failed      (5)   - The measurement request has failed and no
                            results are available.
        noResources (6)   - The NE cannot initiate the command, due
                            to lack of internal memory resources.
   o  Xdsl2LineReset:
      Attributes with this syntax are configuration parameters that
      control the line reset function.
         idle (1)          - This state indicates that there is
                             currently no request for a line reset.
         reset (2)         - This state indicates that a line reset
                             request has been issued.
   o  Xdsl2LineProfiles:
      Attributes with this syntax reference the list of supported,
      enabled or active ITU-T G.993.2 implementation profiles.  This is
      a BITS structure with the following values:
         profile8a  (0)    - Profile 8a.
         profile8b  (1)    - Profile 8b.
         profile8c  (2)    - Profile 8c.
         profile8d  (3)    - Profile 8d.
         profile12a (4)    - Profile 12a.
         profile12b (5)    - Profile 12b.
         profile17a (6)    - Profile 17a.
         profile30a (7)    - Profile 30a.
   o  Xdsl2LineClassMask:
      Attributes with this syntax are configuration parameters that
      specify the VDSL2 PSD Mask Class for a selected VDSL2 transmission
      mode.  The following classes are defined:
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         none     (1) - VDSL2 PSD Mask Class is unknown/irrelevant.
         a998ORb997M1cORc998B (2)-
                        For ITU-T G.993.2 Annex A this is the
                        only applicable PSD class.
                        ITU-T G.993.2 Annex B: 997-M1c-A-7.
                        ITU-T G.993.2 Annex C: 998-B (POTS-138b,
                        POTS-276b, TCM-ISDN).
         b997M1xOR998co (3) -
                        ITU-T G.993.2 Annex B: 997-M1x-M-8 or
                        997-M1x-M.
                        ITU-T G.993.2 Annex C: 998-CO (POTS-138co,
                        POTS-276co).
         b997M2x  (4) - ITU-T G.993.2 Annex B: 997-M2x-M-8, 997-M2x-A,
                        997-M2x-M, 997E17-M2x-NUS0, 997E30-M2x-NUS0.
         b998M1x  (5) - ITU-T G.993.2 Annex B: 998-M1x-A, 998-M1x-B,
                        998-M1x-NUS0.
         b998M2x  (6) - ITU-T G.993.2 Annex B: 998-M2x-A, 998-M2x-M,
                        998-M2x-B, 998-M2x-NUS0, 998E17-M2x-NUS0,
                        998E17-M2x-NUS0-M, 998E30-M2x-NUS0,
                        998E30-M2x-NUS0-M.
         b998AdeM2x(7)- ITU-T G.993.2 Annex B: 998-M2x-A, 998-M2x-M,
                        998-M2x-B, 998-M2x-NUS0, 998ADE17-M2x-A,
                        998ADE17-M2x-B, 998ADE17-M2x-NUS0-M,
                        998ADE30-M2x-NUS0-A, 998ADE30-M2x-NUS0-M.
         bHpeM1   (8) - ITU-T G.993.2 Annex B: HPE17-M1-NUS0,
                        HPE30-M1-NUS0.
   o  Xdsl2LineLimitMask:
      Attributes with this syntax are configuration parameters that
      specify the VDSL2 PSD Limit Mask for each PSD Mask Class and
      implementation profile.  The VDSL2 implementation profiles are
      grouped into 4 classes and each is allocated 16 PSD Limit Mask
      values in this textual convention.
   o  Xdsl2LineUs0Disable:
      Attributes with this syntax are configuration parameters that
      indicate if US0 (upstream band number 0) is disabled for each
      limit PSD mask.  The VDSL2 implementation profiles are grouped
      into 4 classes and each is allocated 16 values in this textual
      convention.
   o  Xdsl2LineUs0Mask:
      Attributes with this syntax are configuration parameters for ITU-T
      G.993.2 Annex A transmission mode that specify the US0 PSD masks
      to be allowed by the near-end xTU on the line.  This syntax is a
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      bit map that supports 20 possible US0 masks.
   o  Xdsl2SymbolProtection:
      Attributes with this syntax are configuration parameters that
      reference the minimum length impulse noise protection (INP) in
      terms of number of symbols (subcarrier spacing of 4.3125 kHz):
         noProtection (1)    - INP not required
         halfSymbol (2)      - INP length =1/2 symbol.
         singleSymbol (3)    - INP length =  1 symbol.
         twoSymbols (4)      - INP length =  2 symbols.
         threeSymbols (5)    - INP length =  3 symbols.
         fourSymbols (6)     - INP length =  4 symbols.
         fiveSymbols (7)     - INP length =  5 symbols.
         sixSymbols (8)      - INP length =  6 symbols.
         sevenSymbols (9)    - INP length =  7 symbols.
         eightSymbols (10)   - INP length =  8 symbols.
         nineSymbols (11)    - INP length =  9 symbols.
         tenSymbols (12)     - INP length = 10 symbols.
         elevenSymbols (13)  - INP length = 11 symbols.
         twelveSymbols (14)  - INP length = 12 symbols.
         thirteeSymbols (15) - INP length = 13 symbols.
         fourteenSymbols (16)- INP length = 14 symbols.
         fifteenSymbols (17) - INP length = 15 symbols.
         sixteenSymbols (18) - INP length = 16 symbols.
   o  Xdsl2SymbolProtection8:
      Attributes with this syntax are configuration parameters that
      reference the minimum length impulse noise protection (INP) in
      terms of number of symbols (subcarrier spacing of 8.625 kHz):
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         noProtection (1)    - INP not required.
         singleSymbol (2)    - INP length =  1 symbol.
         twoSymbols (3)      - INP length =  2 symbols.
         threeSymbols (4)    - INP length =  3 symbols.
         fourSymbols (5)     - INP length =  4 symbols.
         fiveSymbols (6)     - INP length =  5 symbols.
         sixSymbols (7)      - INP length =  6 symbols.
         sevenSymbols (8)    - INP length =  7 symbols.
         eightSymbols (9)    - INP length =  8 symbols.
         nineSymbols (10)    - INP length =  9 symbols.
         tenSymbols (11)     - INP length = 10 symbols.
         elevenSymbols (12)  - INP length = 11 symbols.
         twelveSymbols (13)  - INP length = 12 symbols.
         thirteeSymbols (14) - INP length = 13 symbols.
         fourteenSymbols (15)- INP length = 14 symbols.
         fifteenSymbols (16) - INP length = 15 symbols.
         sixteenSymbols (17) - INP length = 16 symbols.
   o  Xdsl2MaxBer:
      Attributes with this syntax are configuration parameters that
      reference the maximum Bit Error Rate (BER):
         eminus3 (1)  - Maximum BER=E^-3.
         eminus5 (2)  - Maximum BER=E^-5.
         eminus7 (3)  - Maximum BER=E^-7.
   o  Xdsl2ChInitPolicy:
      This syntax serves for channel configuration parameters that
      reference the channel initialization policy.
         policy0 (1)  - Policy 0 according to the applicable standard.
         policy1 (2)  - Policy 1 according to the applicable standard.
   o  Xdsl2ScMaskDs:
      Attributes with this syntax are configuration parameters that
      reference the downstream subcarrier mask.  This syntax is a bitmap
      of up to 4096 bits.
   o  Xdsl2ScMaskUs:
      Attributes with this syntax are configuration parameters that
      reference the upstream subcarrier mask.  This syntax is a bitmap
      of up to 4096 bits.
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   o  Xdsl2CarMask:
      Attributes with this syntax are configuration parameters for VDSL2
      transmission modes that define an array of up to 32 bands.  Each
      band is represented by a start subcarrier index followed by a stop
      subcarrier index.
   o  Xdsl2RfiBands:
      Attributes with this syntax are configuration parameters that
      define radio frequency interference (RFI) bands.  Each RFI band is
      represented by 4 octets: 16 bit start subcarrier index followed by
      a 16 bit stop subcarrier index.
   o  Xdsl2PsdMaskDs:
      Attributes with this syntax are configuration parameters that
      reference the downstream power spectrum density (PSD) mask.  This
      syntax is a structure of up to 32 breakpoints, where each
      breakpoint occupies 3 octets.
   o  Xdsl2PsdMaskUs:
      Attributes with this syntax are configuration parameters that
      reference the upstream power spectrum density (PSD) mask.  This
      syntax is a structure of up to 16 breakpoints, where each
      breakpoint occupies 3 octets.
   o  Xdsl2Tssi:
      Attributes with this syntax are status parameters that reference
      the transmit spectrum shaping (TSSi).  This syntax is a structure
      of up to 32 breakpoints, where each breakpoint occupies 3 octets.
   o  Xdsl2LastTransmittedState:
      Attributes with this syntax reference the list of initialization
      states for VDSL2/ADSL/ADSL2 or ADSL2+ modems.  The list of states
      for CO side modems is different from the list of states for the
      CPE side modems.  Also, the states for VDSL2 modems are not the
      same as those for the ADSL/ADSL2 and ADSL2+ modems.
      Specified as an enumeration type, there are currently a few dozen
      states in the list per each unit side (i.e., CO and CPE).
   o  Xdsl2LineStatus:
      Attributes with this syntax are status parameters that reflect the
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      failure status for a given end point of a VDSL2/ADSL/ADSL2 or
      ADSL2+ link.
      This is a BITS structure that can report the following failures:
         noDefect (0)      - This bit position positively reports that
                             no defect or failure exist.
         lossOfFraming (1) - Loss of frame synchronization.
         lossOfSignal (2)  - Loss of signal.
         lossOfPower (3)   - Loss of power.  Usually this failure may
                             be reported for CPE units only.
         initFailure (4)   - Recent initialization process failed.
                             Never active on xTU-R.
   o  Xdsl2ChInpReport:
      Attributes with this syntax are status parameters that report the
      method that ACTINP is computed with.
         inpComputedUsingFormula (1) - ACTINP computed using
                                       INP_no_erasure formula.
         inpEstimatedByXtur (2)      - ACTINP estimated by the xTU
         receiver.
   o  Xdsl2ChAtmStatus:
      Attributes with this syntax are status parameters that reflect the
      failure status for Transmission Convergence (TC) layer of a given
      ATM interface (data path over a VDSL2/ADSL/ADSL2 or ADSL2+ link).
      This is a BITS structure that can report the following failures:
      noDefect (0)             - This bit position positively reports
                                 that no defect or failure exists.
      noCellDelineation (1)    - The link was successfully initialized
                                 but cell delineation was never acquired
                                 on the associated ATM data path.
      lossOfCellDelineation (2)- Loss of cell delineation on the
                                 associated ATM data path.
   o  Xdsl2ChPtmStatus:
      Attributes with this syntax are status parameters that reflect the
      failure status for a given PTM interface (i.e., packet data path
      over a VDSL2/ADSL/ADSL2 or ADSL2+ link).
      This is a BITS structure that can report the following failures:
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         noDefect (0)     - This bit position positively reports that no
                            defect or failure exists.
         outOfSync (1)    - Out of synchronization.
   o  Xdsl2UpboKLF:
      Attributes with this syntax are configuration parameters referring
      to whether or not upstream power backoff (UPBO) is enabled and how
      electrical length in the context of UPBO is determined.
      This enumeration type can have the following values:
       auto(1)          - The VTUs autonomously determine the electrical
                          length.
       override(2)      - Forces the VTU-R to use the electrical length,
                          kl0, of the CO-MIB (UPBOKL) to compute the
                          UPBO.
       disableUpbo(3)   - Disables UPBO. I.e., UPBO is not utilized.
   o  Xdsl2BandUs:
      Attributes with this syntax are used as table indexes that refer
      to upstream bands of VDSL2 lines (excluding US0 band).
      This enumeration type can have the following values:
         us1(5)           - Upstream band number 1 (US1).
         us2(7)           - Upstream band number 2 (US2).
         us3(9)           - Upstream band number 3 (US3).
         us4(11)          - Upstream band number 4 (US4).
   o  Xdsl2LinePsdMaskSelectUs:
      Attributes with this syntax are configuration parameters that
      control the upstream PSD mask selection for Annexes J and M of
      G.992.3 and G.992.5.
         adlu32Eu32 (1),   - ADLU-32 / EU-32.
         adlu36Eu36 (2),   - ADLU-36 / EU-36.
         adlu40Eu40 (3),   - ADLU-40 / EU-40.
         adlu44Eu44 (4),   - ADLU-44 / EU-44.
         adlu48Eu48 (5),   - ADLU-48 / EU-48.
         adlu52Eu52 (6),   - ADLU-52 / EU-52.
         adlu56Eu56 (7),   - ADLU-56 / EU-56.
         adlu60Eu60 (8),   - ADLU-60 / EU-60.
         adlu64Eu64 (9)    - ADLU-64 / EU-64.
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   o  Xdsl2LineCeFlag:
      Attributes with this syntax are configuration parameters that
      control the optional cyclic extension values.
         enableCyclicExtension (0) - Enable use of optional
                                     Cyclic Extension values.
   o  Xdsl2LineSnrMode
      Attributes with this syntax are parameters related to the enabling
      and disabling of transmitter referred virtual noise.
         virtualNoiseDisabled (1) - virtual noise is disabled.
         virtualNoiseEnabled (2)  - virtual noise is enabled.
   o  Xdsl2LineTxRefVnDs
      Attributes with this syntax are configuration parameters that
      define the downstream transmitter referred virtual noise, which is
      specified through a set of breakpoints.  Each breakpoint occupies
      3 octets: The first two octets hold the index of the subcarrier
      associated with the breakpoint.  The third octet holds the PSD
      reduction at the breakpoint from 0 (-140 dBm/Hz) to 200 (-40
      dBm/Hz) using units of 0.5dBm/Hz.  A special value of 255
      indicates a noise level of 0 W/Hz.
   o  Xdsl2LineTxRefVnUs:
      Attributes with this syntax are configuration parameters that
      define the upstream transmitter referred virtual noise, which is
      specified through a set of breakpoints.  Each breakpoint occupies
      3 octets: The first two octets hold the index of the subcarrier
      associated with the breakpoint.  The third octet holds the PSD
      reduction at the breakpoint from 0 (-140 dBm/Hz) to 200 (-40
      dBm/Hz) using units of 0.5dBm/Hz.  A special value of 255
      indicates a noise level of 0 W/Hz.
   o  Xdsl2LineForceInp:
      Attributes with this syntax are configuration parameters that
      control the framer of a bearer channel.
         forceFramerForInp (0) -  Select framer setting to satisfy
                                  impulse noise protection requirements.
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   o  Xdsl2BitsAlloc:
      Attributes with this syntax are status parameters that report the
      bits allocation for each subcarrier.  The bits allocation for a
      subcarrier is in the range 0 to 15.
   o  Xdsl2MrefPsdDs:
      Attributes with this syntax are MEDLEY Reference PSD status
      parameters in the downstream direction.  This is expressed as the
      set of breakpoints exchanged at initialization.  The OCTET STRING
      contains up to 48 pairs of values in the following structure:
      Octets 0-1 -- Index of 1st subcarrier used in the context of a
      first breakpoint.  Octets 2-3 -- The PSD level for the subcarrier
      indicated by octets 0-1.  Octets 4-7 -- Same, for a 2nd breakpoint
      Octets 8-11 -- Same, for a 3rd breakpoint And so on until Octets
      188-191 -- Same, for a 48th breakpoint.  Each subcarrier index is
      an unsigned number in the range 1 to NSds (i.e., highest supported
      subcarrier index in the downstream direction).  The PSD level is
      an integer value in the 0 to 4095 range.  It is represented in
      units of 0.1 dB offset from -140dBm/Hz.
   o  Xdsl2MrefPsdUs:
      Attributes with this syntax are MEDLEY Reference PSD status
      parameters in the upstream direction.  This is expressed as the
      set of breakpoints exchanged at initialization.  The OCTET STRING
      contains up to 32 pairs of values in the following structure:
      Octets 0-1 -- Index of 1st subcarrier used in the context of a
      first breakpoint.  Octets 2-3 -- The PSD level for the subcarrier
      indicated by octets 0-1.  Octets 4-7 -- Same, for a 2nd breakpoint
      Octets 8-11 -- Same, for a 3rd breakpoint And so on until Octets
      124-127 -- Same, for a 32nd breakpoint.  Each subcarrier index is
      an unsigned number in the range 1 to NSus (i.e., highest supported
      subcarrier index in the upstream direction).  The PSD level is an
      integer value in the 0 to 4095 range.  It is represented in units
      of 0.1 dB offset from -140dBm/Hz.
2.4.  Structure
   The MIB module is structured into the following MIB groups:
   o  Line Configuration, Maintenance, and Status Group:
      This group supports MIB objects for configuring parameters for the
      VDSL2/ADSL/ADSL2 or ADSL2+ line and retrieving line status
      information.  It also supports MIB objects for configuring a
      requested power state or initiating a Dual Ended Loop Test (DELT)
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      process in the VDSL2/ADSL/ADSL2 or ADSL2+ line.  It contains the
      following tables:
         - xdsl2LineTable
         - xdsl2LineSegmentTable
         - xdsl2LineBandTable
   o  Channel Status Group:
      This group supports MIB objects for retrieving channel layer
      status information.  It contains the following table:
         - xdsl2ChannelStatusTable
   o  Subcarrier Status Group:
      This group supports MIB objects for retrieving the subcarrier
      layer status information, mostly collected by a Dual Ended Loop
      Test (DELT) process.  It contains the following tables:
         - xdsl2SCStatusTable
         - xdsl2SCStatusBandTable
         - xdsl2SCStatusSegmentTable
   o  Unit Inventory Group:
      This group supports MIB objects for retrieving Unit inventory
      information about units in VDSL2/ADSL/ADSL2 or ADSL2+ lines via
      the EOC.  It contains the following table:
         - xdsl2LineInventoryTable
   o  Current Performance Group:
      This group supports MIB objects that provide the current
      performance information relating to VDSL2/ADSL/ADSL2 and ADSL2+
      line, unit and channel levels.  It contains the following tables:
         - xdsl2PMLineCurrTable
         - xdsl2PMLineInitCurrTable
         - xdsl2PMChCurrTable
   o  15-Minute Interval Performance Group:
      This group supports MIB objects that provide historic performance
      information relating to VDSL2/ADSL/ADSL2 and ADSL2+ line, unit and
      channel levels in 15- minute intervals.  It contains the following
      tables:
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         - xdsl2PMLineHist15MinTable
         - xdsl2PMLineInitHist15MinTable
         - xdsl2PMChHist15MinTable
   o  1-Day Interval Performance Group:
      This group supports MIB objects that provide historic performance
      information relating to VDSL2/ADSL/ADSL2 and ADSL2+ line, unit and
      channel levels in 1-day intervals.  It contains the following
      tables:
         - xdsl2PMLineHist1DayTable
         - xdsl2PMLineInitHist1DayTable
         - xdsl2PMChHist1DTable
   o  Configuration Template and Profile Group:
      This group supports MIB objects for defining configuration
      profiles for VDSL2/ADSL/ADSL2 and ADSL2+ lines and channels, as
      well as configuration templates.  Each configuration template is
      comprised of one line configuration profile and one or more
      channel configuration profiles.  This group contains the following
      tables:
         - xdsl2LineConfTemplateTable
         - xdsl2LineConfProfTable
         - xdsl2LineConfProfModeSpecTable
         - xdsl2LineConfProfModeSpecBandUsTable
         - xdsl2ChConfProfileTable
   o  Alarm Configuration Template and Profile Group:
      This group supports MIB objects for defining alarm profiles for
      VDSL2/ADSL/ADSL2 and ADSL2+ lines and channels, as well as alarm
      templates.  Each alarm template is comprised of one line alarm
      profile and one or more channel alarm profiles.  This group
      contains the following tables:
         - xdsl2LineAlarmConfTemplateTable
         - xdsl2LineAlarmConfProfileTable
         - xdsl2ChAlarmConfProfileTable
   o  Notifications Group:
      This group defines the notifications supported for VDSL2/ADSL/
      ADSL2 and ADSL2+ lines:
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         - xdsl2LinePerfFECSThreshXtuc
         - xdsl2LinePerfFECSThreshXtur
         - xdsl2LinePerfESThreshXtuc
         - xdsl2LinePerfESThreshXtur
         - xdsl2LinePerfSESThreshXtuc
         - xdsl2LinePerfSESThreshXtur
         - xdsl2LinePerfLOSSThreshXtuc
         - xdsl2LinePerfLOSSThreshXtur
         - xdsl2LinePerfUASThreshXtuc
         - xdsl2LinePerfUASThreshXtur
         - xdsl2LinePerfCodingViolationsThreshXtuc
         - xdsl2LinePerfCodingViolationsThreshXtur
         - xdsl2LinePerfCorrectedThreshXtuc
         - xdsl2LinePerfCorrectedThreshXtur
         - xdsl2LinePerfFailedFullInitThresh
         - xdsl2LinePerfFailedShortInitThresh
         - xdsl2LineStatusChangeXtuc
         - xdsl2LineStatusChangeXtur
2.5.  Persistence
   All read-create objects and most read-write objects defined in this
   MIB module SHOULD be stored persistently.  Following is an exhaustive
   list of these persistent objects:
         xdsl2LineCnfgTemplate
         xdsl2LineAlarmCnfgTemplate
         xdsl2LineCmndConfPmsf
         xdsl2LConfTempTemplateName
         xdsl2LConfTempLineProfile
         xdsl2LConfTempChan1ConfProfile
         xdsl2LConfTempChan1RaRatioDs
         xdsl2LConfTempChan1RaRatioUs
         xdsl2LConfTempChan2ConfProfile
         xdsl2LConfTempChan2RaRatioDs
         xdsl2LConfTempChan2RaRatioUs
         xdsl2LConfTempChan3ConfProfile
         xdsl2LConfTempChan3RaRatioDs
         xdsl2LConfTempChan3RaRatioUs
         xdsl2LConfTempChan4ConfProfile
         xdsl2LConfTempChan4RaRatioDs
         xdsl2LConfTempChan4RaRatioUs
         xdsl2LConfTempRowStatus
         xdsl2LConfProfProfileName
         xdsl2LConfProfScMaskDs
         xdsl2LConfProfScMaskUs
         xdsl2LConfProfVdsl2CarMask
         xdsl2LConfProfRfiBandsDs
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         xdsl2LConfProfRaModeDs
         xdsl2LConfProfRaModeUs
         xdsl2LConfProfRaUsNrmDs
         xdsl2LConfProfRaUsNrmUs
         xdsl2LConfProfRaUsTimeDs
         xdsl2LConfProfRaUsTimeUs
         xdsl2LConfProfRaDsNrmDs
         xdsl2LConfProfRaDsNrmUs
         xdsl2LConfProfRaDsTimeDs
         xdsl2LConfProfRaDsTimeUs
         xdsl2LConfProfTargetSnrmDs
         xdsl2LConfProfTargetSnrmUs
         xdsl2LConfProfMaxSnrmDs
         xdsl2LConfProfMaxSnrmUs
         xdsl2LConfProfMinSnrmDs
         xdsl2LConfProfMinSnrmUs
         xdsl2LConfProfMsgMinUs
         xdsl2LConfProfMsgMinDs
         xdsl2LConfProfXtuTransSysEna
         xdsl2LConfProfPmMode
         xdsl2LConfProfL0Time
         xdsl2LConfProfL2Time
         xdsl2LConfProfL2Atpr
         xdsl2LConfProfL2Atprt
         xdsl2LConfProfProfiles
         xdsl2LConfProfDpboEPsd
         xdsl2LConfProfDpboEsEL
         xdsl2LConfProfDpboEsCableModelA
         xdsl2LConfProfDpboEsCableModelB
         xdsl2LConfProfDpboEsCableModelC
         xdsl2LConfProfDpboMus
         xdsl2LConfProfDpboFMin
         xdsl2LConfProfDpboFMax
         xdsl2LConfProfUpboKL
         xdsl2LConfProfUpboKLF
         xdsl2LConfProfUs0Mask
         xdsl2LConfProfRowStatus
         xdsl2LConfProfXdslMode
         xdsl2LConfProfMaxNomPsdDs
         xdsl2LConfProfMaxNomPsdUs
         xdsl2LConfProfMaxNomAtpDs
         xdsl2LConfProfMaxNomAtpUs
         xdsl2LConfProfMaxAggRxPwrUs
         xdsl2LConfProfPsdMaskDs
         xdsl2LConfProfPsdMaskUs
         xdsl2LConfProfPsdMaskSelectUs
         xdsl2LConfProfClassMask
         xdsl2LConfProfLimitMask
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         xdsl2LConfProfUs0Disabl
         xdsl2LConfProfModeSpecRowStatus
         xdsl2LConfProfXdslBandUs
         xdsl2LConfProfUpboPsdA
         xdsl2LConfProfUpboPsdB
         xdsl2LConfProfModeSpecBandUsRowStatus
         xdsl2ChConfProfProfileName
         xdsl2ChConfProfMinDataRateDs
         xdsl2ChConfProfMinDataRateUs
         xdsl2ChConfProfMinResDataRateDs
         xdsl2ChConfProfMinResDataRateUs
         xdsl2ChConfProfMaxDataRateDs
         xdsl2ChConfProfMaxDataRateUs
         xdsl2ChConfProfMinDataRateLowPwrDs
         xdsl2ChConfProfMaxDelayDs
         xdsl2ChConfProfMaxDelayUs
         xdsl2ChConfProfMinProtectionDs
         xdsl2ChConfProfMinProtectionUs
         xdsl2ChConfProfMaxBerDs
         xdsl2ChConfProfMaxBerUs
         xdsl2ChConfProfUsDataRateDs
         xdsl2ChConfProfDsDataRateDs
         xdsl2ChConfProfUsDataRateUs
         xdsl2ChConfProfDsDataRateUs
         xdsl2ChConfProfImaEnabled
         xdsl2ChConfProfMaxDelayVar
         xdsl2ChConfProfInitPolicy
         xdsl2ChConfProfRowStatus
         xdsl2LAlarmConfTempTemplateName
         xdsl2LAlarmConfTempLineProfile
         xdsl2LAlarmConfTempChan1ConfProfile
         xdsl2LAlarmConfTempChan2ConfProfile
         xdsl2LAlarmConfTempChan3ConfProfile
         xdsl2LAlarmConfTempChan4ConfProfile
         xdsl2LAlarmConfTempRowStatus
         xdsl2LineAlarmConfProfileName
         xdsl2LineAlarmConfProfileXtucThresh15MinFecs
         xdsl2LineAlarmConfProfileXtucThresh15MinEs
         xdsl2LineAlarmConfProfileXtucThresh15MinSes
         xdsl2LineAlarmConfProfileXtucThresh15MinLoss
         xdsl2LineAlarmConfProfileXtucThresh15MinUas
         xdsl2LineAlarmConfProfileXturThresh15MinFecs
         xdsl2LineAlarmConfProfileXturThresh15MinEs
         xdsl2LineAlarmConfProfileXturThresh15MinSes
         xdsl2LineAlarmConfProfileXturThresh15MinLoss
         xdsl2LineAlarmConfProfileXturThresh15MinUas
         xdsl2LineAlarmConfProfileThresh15MinFailedFullInt
         xdsl2LineAlarmConfProfileThresh15MinFailedShrtInt
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         xdsl2LineAlarmConfProfileRowStatus
         xdsl2ChAlarmConfProfileName
         xdsl2ChAlarmConfProfileXtucThresh15MinCodingViolations
         xdsl2ChAlarmConfProfileXtucThresh15MinCorrected
         xdsl2ChAlarmConfProfileXturThresh15MinCodingViolations
         xdsl2ChAlarmConfProfileXturThresh15MinCorrected
         xdsl2ChAlarmConfProfileRowStatus
   Note, also, that the interface indices in this MIB are maintained
   persistently.  View-based Access Control Model (VACM) data relating
   to these SHOULD be stored persistently as well [RFC3410].
2.6.  Line Topology
   A VDSL2/ADSL/ADSL2 and ADSL2+ Line consists of two units: atuc or
   vtuc (a central office termination unit) and atur or vtur (a remote
   termination unit).  There are up to 4 channels (maximum number of
   channels depends on the specific DSL technology), each carrying an
   independent information flow, as shown in the figure below.
       <-- Network Side                            Customer Side -->
       |<///////////// VDSL2/ADSL/ADSL2/ADSL2+ Span //////////////>|
       +-------+                                           +-------+
       |       |<---------------------1------------------->|       |
       | atuc  |<---------------------2------------------->|  atur |
       |  or   |<~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~>|   or  |
       | vtuc  |<---------------------3------------------->|  vtuc |
       |       |<---------------------4------------------->|       |
       +-------+                                           +-------+
       Key:  <////> VDSL2/ADSL/ADSL2/ADSL2+ Span
             <~~~~> VDSL2/ADSL/ADSL2/ADSL2+ twisted-pair
             -1-    Channel #1 carried over the line
             -2-    Optional channel #2 carried over the line
             -3-    Optional channel #3 carried over the line
             -4-    Optional channel #4 carried over the line
   Figure 3: General topology for a VDSL2/ADSL/ADSL2/ADSL2+ Line
2.7.  Counters, Interval Buckets, and Thresholds
2.7.1.  Counters Managed
   There are various types of counters specified in this MIB.  Each
   counter refers either to the whole VDSL2/ADSL/ADSL2/ADSL2+ line, to
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   one of the xTU entities, or to one of the bearer channels.
   o  On the whole line level
      For full initializations, failed full initializations, short
      initializations, and for failed short initializations there are
      event counters, current 15-minute and 0 to 96 15-minute history
      bucket(s) of "interval-counters", as well as current and 0 to 30
      previous 1-day interval-counter(s).  Each current 15-minute
      "failed" event bucket has an associated threshold notification.
   o  On the xTU level
      For the LOS Seconds, ES, SES, FEC seconds, and UAS, there are
      event counters, current 15-minute and 0 to 96 15-minute history
      bucket(s) of "interval-counters", as well as current and 0 to 30
      previous 1-day interval-counter(s).  Each current 15-minute event
      bucket has an associated threshold notification.
   o  On the bearer channel level
      For the coding violations (CRC anomalies) and corrected blocks
      (i.e., FEC events) there are event counters, current 15-minute and
      0 to 96 15-minute history bucket(s) of "interval- counters", as
      well as current and 0 to 30 previous 1-day interval- counter(s).
      Each current 15-minute event bucket has an associated threshold
      notification.
2.7.2.  Minimum Number Of Buckets
   Although it is possible to support up to 96 15-minute history buckets
   of "interval-counters", systems implementing this MIB module SHOULD
   practically support at least 16 buckets, as specified in ITU-T
   G.997.1, paragraph #7.2.7.9.
   Similarly, it is possible to support up to 30 previous 1-day
   "interval-counters", but systems implementing this MIB module SHOULD
   support at least 1 previous day bucket.
2.7.3.  Interval Buckets Initialization
   There is no requirement for an agent to ensure a fixed relationship
   between the start of a 15-minute interval and any wall clock;
   however, some implementations may align the 15-minute intervals with
   quarter hours.  Likewise, an implementation may choose to align one
   day intervals with the start of a day.
   Counters are not reset when an xTU is reinitialized, only when the
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   agent is reset or reinitialized (or under specific request outside
   the scope of this MIB module).
2.7.4.  Interval Buckets Validity
   As in RFC 3593 [RFC3593] and RFC 2662 [RFC2662], in case the data for
   an interval is suspect or known to be invalid, the agent MUST report
   the interval as invalid.  If the current 15-minute event bucket is
   determined to be invalid, the element management system SHOULD ignore
   its content and the agent MUST NOT generate notifications based upon
   the value of the event bucket.
   A valid 15-minute event bucket SHOULD usually count the events for
   exactly 15 minutes.  Similarly, a valid 1-day event bucket SHOULD
   usually count the events for exactly 24 hours.  However, the
   following scenarios are exceptional:
   1) For implementations that align the 15-minute intervals with
      quarter hours, and the 1-day intervals with start of a day, the
      management system may still start the PM process not aligned with
      the wall clock.  Such a management system may wish to retrieve
      even partial information for the first event buckets, rather than
      declaring them all as invalid.
   2) For an event bucket that suffered relatively short outages, the
      management system may wish to retrieve the available PM outcomes,
      rather than declaring the whole event bucket as invalid.  This is
      more important for 1-day event buckets.
   3) An event bucket may be shorter or longer than the formal duration
      if a clock adjustment was performed during the interval.
   This MIB allows supporting the exceptional scenarios described above
   by reporting the actual Monitoring Time of a monitoring interval.
   This parameter is relevant only for Valid intervals, but is useful
   for these exceptional scenarios:
   a) The management system MAY still declare a partial PM interval as
      Valid and report the actual number of seconds the interval lasted.
   b) If the interval was shortened or extended due to clock
      corrections, the management system SHOULD report the actual number
      of seconds the interval lasted, beside reporting that the interval
      is Valid.
2.8.  Profiles
   As a managed node can handle a large number of xTUs, (e.g., hundreds
   or perhaps thousands of lines), provisioning every parameter on every
   xTU may become burdensome.  Moreover, most lines are provisioned
   identically with the same set of parameters.  To simplify the
   provisioning process, this MIB module makes use of profiles and
   templates.
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   A configuration profile is a set of parameters that can be shared by
   multiple entities.  There is a configuration profile to address line-
   level provisioning and another type of profile that addresses
   channel-level provisioning parameters.
   A configuration template is actually a profile-of-profiles.  That is,
   a template is comprised of one line configuration profile and one or
   more channel configuration profiles.  A template provides the
   complete configuration of a line.  The same configuration can be
   shared by multiple lines.
   In a similar manner to the configuration profiles and templates, this
   MIB module makes use of templates and profiles for specifying the
   alarm thresholds associated with performance parameters.  This allows
   provisioning multiple lines with the same criteria for generating
   threshold crossing notifications.
   The following paragraphs describe templates and profiles used in this
   MIB module
2.8.1.  Configuration Profiles And Templates
   o  Line Configuration Profiles - Line configuration profiles contain
      line-level parameters for configuring VDSL2/ADSL/ADSL2 and ADSL2+
      lines.  They are defined in the xdsl2LineConfProfTable.
      The line configuration includes settings such as the specific
      VDSL2/ADSL/ADSL2 or ADSL2+ modes to enable on the respective line,
      power spectrum parameters, rate adaptation criteria, and SNR
      margin-related parameters.  A subset of the line configuration
      parameters depends upon the specific xDSL Mode allowed (i.e., Does
      the profile allow VDSL2, ADSL, ADSL2 and/or ADSL2+?) as well as
      what annex/annexes of the standard are allowed.  This is the
      reason a line profile MUST include one or more mode-specific
      extensions.
   o  Channel Configuration Profiles - Channel configuration profiles
      contain parameters for configuring bearer channels over the VDSL2/
      ADSL/ADSL2 and ADSL2+ lines.  They are sometimes considered as the
      service layer configuration of the VDSL2/ADSL/ADSL2 and ADSL2+
      lines.  They are defined in the xdsl2ChConfProfTable.
      The channel configuration includes issues such as the desired
      minimum and maximum rate on each traffic flow direction and
      impulse noise protection parameters.
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   o  Line Configuration Templates - Line configuration templates allow
      combining line configuration profiles and channel configuration
      profiles into a comprehensive configuration of the VDSL2/ADSL/
      ADSL2 and ADSL2+ line.  They are defined in the
      xdsl2LineConfTemplateTable.
      The line configuration template includes one index of a line
      configuration profile and one to four indexes of channel
      configuration profiles.  The template also addresses the issue of
      distributing the excess available data rate on each traffic flow
      direction (i.e., the data rate left after each channel is
      allocated a data rate to satisfy its minimum requested data rate)
      among the various channels.
2.8.2.  Alarm Configuration Profiles And Templates
   o  Line Alarm Configuration Profiles - Line-level Alarm configuration
      profiles contain the threshold values for Performance Monitoring
      (PM) parameters, counted either on the whole line level or on an
      xTU level.  Thresholds are required only for failures and
      anomalies.  E.g., there are thresholds for failed initializations
      and LOS seconds, but not for the aggregate number of full
      initializations.  These profiles are defined in the
      xdsl2LineAlarmConfProfileTable.
   o  Channel Alarm Configuration Profiles - Channel-level Alarm
      configuration profiles contain the threshold values for PM
      parameters counted on a bearer channel level.  Thresholds are
      defined for two types of anomalies: corrected blocks and coding
      violations.  These profiles are defined in the
      xdsl2ChAlarmConfProfileTable.
   o  Line Alarm Configuration Templates - Line Alarm configuration
      templates allow combining line-level alarm configuration profiles
      and channel-level alarm configuration profiles into a
      comprehensive configuration of the PM thresholds for the VDSL2/
      ADSL/ADSL2 and ADSL2+ line.  They are defined in the
      xdsl2LineAlarmConfTemplateTable.
      The line alarm configuration template includes one index of a
      line-level alarm configuration profile and one to four indexes of
      channel-level alarm configuration profiles.
2.8.3.  Managing Profiles And Templates
   The index value for each profile and template is a locally-unique,
   administratively assigned name having the textual convention
Morgenstern, et al.      Expires January 8, 2009               [Page 30]
Internet-Draft               VDSL2-LINE MIB                    July 2008
   'SnmpAdminString' (RFC 3411 [RFC3411]).
   One or more lines may be configured to share parameters of a single
   configuration template (e.g., xdsl2LConfTempTemplateName = 'silver')
   by setting its xdsl2LineCnfgTemplate object to the value of this
   template.
   One or more lines may be configured to share parameters of a single
   Alarm configuration template (e.g., xdsl2LAlarmConfTempTemplateName =
   'silver') by setting its xdsl2LineAlarmCnfgTemplate object to the
   value of this template.
   Before a template can be deleted or taken out of service, it MUST be
   first unreferenced from all associated lines.  Implementations MAY
   also reject template modification while it is associated with any
   line.
   Before a profile can be deleted or taken out of service, it MUST be
   first unreferenced from all associated templates.  Implementations
   MAY also reject profile modification while it is referenced by any
   template.
   Implementations MUST provide a default profile whose name is 'DEFVAL'
   for each profile and template type.  The values of the associated
   parameters will be vendor-specific unless otherwise indicated in this
   document.  Before a line's templates have been set, these templates
   will be automatically used by setting xdsl2LineCnfgTemplate and
   xdsl2LineAlarmCnfgTemplate to 'DEFVAL' where appropriate.  This
   default profile name, 'DEFVAL', is considered reserved in the context
   of profiles and templates defined in this MIB module.
   Profiles and templates are created, assigned, and deleted dynamically
   using the profile name and profile row status in each of the profile
   tables.
   If the implementation allows modifying a profile or template while it
   is associated with a line, then such changes MUST take effect
   immediately.  These changes MAY result in a restart (hard reset or
   soft restart) of the units on the line.
   Network Elements may optionaly implement a fallback line
   configuration template ( See xdsl2LineCnfgFallbackTemplate ).  The
   fallback template will be tried if the xDSL2 line fails to operate
   using the primary template.  If the xDSL2 line fails to operate using
   the fallback template then the primary template should be retried.
   The xTU-C should continue to alternate between the primary and
   fallback templates until one of them succeeds.
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2.8.4.  Managing Multiple Bearer Channels
   The number of bearer channels is configured by setting the template
   attributes xdsl2LConfTempChan1ConfProfile,
   xdsl2LConfTempChan2ConfProfile, xdsl2LConfTempChan3ConfProfile, and
   xdsl2LConfTempChan4ConfProfile and then assigning that template to a
   DSL line using the xdsl2LineCnfgTemplate attribute.  When the number
   of bearer channels for a DSL line changes, the SNMP agent will
   automatically create or destroy rows in channel-related tables
   associated with that line.  For example, when a DSL line is operating
   with one bearer channel, there will be zero rows in channel-related
   tables for channels two, three, and four.  The SNMP agent MUST create
   and destroy channel-related rows as follows:
   o  When the number of bearer channels for a DSL line changes to a
      higher number, the SNMP agent will automatically create rows in
      the xdsl2ChannelStatusTable, and xdsl2PMChCurrTable tables for
      that line.
   o  When the number of bearer channels for a DSL line changes to a
      lower number, the SNMP agent will automatically destroy rows in
      the xdsl2ChannelStatusTable,
      xdsl2PMChCurrTable,xdsl2PMChHist15MinTable and
      xdsl2PMChHist1DTable tables for that line.
2.9.  Notifications
   The ability to generate the SNMP notifications coldStart/WarmStart
   (per [RFC3418]), which are per agent (e.g., per Digital Subscriber
   Line Access Multiplexer, or DSLAM, in such a device), and linkUp/
   linkDown (per [RFC2863]), which are per interface (i.e., VDSL2/ADSL/
   ADSL2 or ADSL2+ line) is required.
   A linkDown notification MAY be generated whenever any of ES, SES, CRC
   Anomaly, LOS, LOF, or UAS event occurs.  The corresponding linkUp
   notification MAY be sent when all link failure conditions are
   cleared.
   The notifications defined in this MIB module are for status change
   (e.g., initialization failure) and for the threshold crossings
   associated with the following events: Full initialization failures,
   short initialization failures, ES, SES, LOS Seconds, UAS, FEC
   Seconds, FEC events, and CRC anomalies.  Each threshold has its own
   enable/threshold value.  When that value is 0, the notification is
   disabled.
   The xdsl2LineStatusXtur and xdsl2LineStatusXtuc are bitmasks
   representing all outstanding error conditions associated with the
   xTU-R and xTU-C (respectively).  Note that since the xTU-R status is
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   obtained via the EOC, this information may be unavailable in case the
   xTU-R is unreachable via EOC during a line error condition.
   Therefore, not all conditions may always be included in its current
   status.  Notifications corresponding to the bit fields in those two
   status objects are defined.
   Note that there are other status parameters that refer to the xTU-R
   (e.g., downstream line attenuation).  Those parameters also depend on
   the availability of EOC between the central office xTU and the remote
   xTU.
   A threshold notification occurs whenever the corresponding current
   15-minute interval error counter becomes equal to, or exceeds the
   threshold value.  Only one notification SHOULD be sent per interval
   per interface.  Since the current 15-minute counter is reset to 0
   every 15 minutes, and if the condition persists, the notification may
   recur as often as every 15 minutes.  For example, to get a
   notification whenever a "loss of" event occurs (but at most once
   every 15 minutes), set the corresponding threshold to 1.  The agent
   will generate a notification when the event originally occurs.
   Notifications, other than the threshold notifications listed above,
   SHOULD be rate-limited (throttled) such that there is an
   implementation-specific gap between the generation of consecutive
   notifications of the same event.  When notifications are rate-
   limited, they are dropped and not queued for sending at a future
   time.  This is intended to be a general rate-limiting statement for
   notifications that otherwise have no explicit rate limiting
   assertions in this document.
   Note that the Network Management System, or NMS, may receive a
   linkDown notification, as well, if enabled (via
   ifLinkUpDownTrapEnable [RFC2863]).  At the beginning of the next 15
   minute interval, the counter is reset.  When the first second goes by
   and the event occurs, the current interval bucket will be 1, which
   equals the threshold, and the notification will be sent again.
3.  Definitions
VDSL2-LINE-TC-MIB DEFINITIONS ::= BEGIN
IMPORTS
   MODULE-IDENTITY,
   transmission
      FROM SNMPv2-SMI
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   TEXTUAL-CONVENTION
      FROM SNMPv2-TC;
vdsl2TCMIB MODULE-IDENTITY
   LAST-UPDATED "200807010000Z" -- July 1, 2008
   ORGANIZATION "ADSLMIB Working Group"
   CONTACT-INFO "WG-email:  adslmib@ietf.org
   Info:      https://www1.ietf.org/mailman/listinfo/adslmib
             Chair:     Mike Sneed
                        Sand Channel Systems
             Postal:    P.O. Box 37324
                        Raleigh NC 27627-732
             Email:     sneedmike@hotmail.com
             Phone:     +1 206 600 7022
             Co-Chair:  Menachem Dodge
                        ECI Telecom Ltd.
             Postal:    30 Hasivim St.
                        Petach Tikva 49517,
                        Israel.
             Email:     mbdodge@ieee.org
             Phone:     +972 3 926 8421
             Co-editor: Moti Morgenstern
                        ECI Telecom Ltd.
             Postal:    30 Hasivim St.
                        Petach Tikva 49517,
                        Israel.
             Email:     moti.morgenstern@ecitele.com
             Phone:     +972 3 926 6258
             Co-editor: Scott Baillie
                        NEC Australia
             Postal:    649-655 Springvale Road,
                        Mulgrave, Victoria 3170,
                        Australia.
             Email:     scott.baillie@nec.com.au
             Phone:     +61 3 9264 3986
             Co-editor: Umberto Bonollo
                        NEC Australia
             Postal:    649-655 Springvale Road,
                        Mulgrave, Victoria 3170,
                        Australia.
             Email:     umberto.bonollo@nec.com.au
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             Phone:     +61 3 9264 3385
            "
   DESCRIPTION
        "This MIB Module provides Textual Conventions to be
         used by the VDSL2-LINE-MIB module for the purpose of
         managing VDSL2, ADSL, ADSL2 and ADSL2+ lines.
        Copyright (C) The IETF Trust (2008).  This version of
        this MIB module is part of RFC XXXX: see the RFC itself for
        full legal notices."
-- RFC Ed.: replace XXXX with assigned number & remove this note
   REVISION "200807010000Z" -- July 1, 2008
   DESCRIPTION "Initial version, published as RFC XXXX."
-- RFC Ed.: replace XX with assigned number & remove this note
      ::= { transmission xxx 2} -- vdsl2MIB 2
-- IANA, the xxx here must be the same as the one assigned
--       to the vdsl2MIB below.
-- RFC Ed.: Please fill in xxx once assigned by IANA.
------------------------------------------------
--          Textual Conventions               --
------------------------------------------------
Xdsl2Unit ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Identifies a transceiver as being either xTU-C or xTU-R.
       A VDSL2/ADSL/ADSL2 or ADSL2+ line consists of two
       transceivers, an xTU-C and an xTU-R.
       In the case of ADSL/ADSL2 and ADSL2+ those two transceivers are
       also called atuc and atur.
       In the case of VDSL2 those two transceivers are also called
       vtuc and vtur.
       Specified as an INTEGER, the two values are:
        xtuc(1)  -- central office transceiver
        xtur(2)  -- remote site transceiver"
   SYNTAX      INTEGER {
                  xtuc(1),
                  xtur(2)
               }
Xdsl2Direction ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION
        "Identifies the direction of a band in a VDSL2/ADSL/ADSL2/
        ADSL2+ link.
        The upstream direction is a transmission from the remote end
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        (xTU-R) towards the central office end (xTU-C). The downstream
        direction is a transmission from the xTU-C towards the xTU-R.
        Specified as an INTEGER, the values are defined as
        follows:"
     SYNTAX INTEGER {
        upstream(1),   -- Transmission from the xTU-R to the xTU-C.
        downstream(2)  -- Transmission from the xTU-C to the xTU-R.
            }
Xdsl2Band ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION
        "Identifies a band in a VDSL2/ADSL/ADSL2/ADSL2+ link.
        For a band in the upstream direction, transmission is from the
        remote end (xTU-R) towards the central office end (xTU-C).
        For a band in the downstream direction, transmission is from
        the xTU-C towards the xTU-R.
        For ADSL, ADSL2 and ADSL2+, which use a single band in the
        upstream direction and a single band
        in the downstream direction,
        the only relevant values are upstream(1) and downstream(2).
        For VDSL2, which uses multiple bands in each transmission
        direction, a band in the upstream direction is indicated by any
        of us0(3), us1(5), us2(7), us3(9) or us4(11) and a band in the
        downstream direction is indicated by any of ds1(4), ds2(6),
        ds3(8) or ds4(10).
        For VDSL2, the values upstream(1) and downstream(2) may be used
        when there is a need to refer to the whole upstream or
        downstream traffic (e.g., report the average signal-to-noise
        ratio on any transmission direction).
        Specified as an INTEGER, the values are defined as
        follows:"
     SYNTAX INTEGER {
        upstream(1),   -- Transmission from the xTU-R to the xTU-C
                       -- (refers to the single upstream band for
                       -- ADSL/ADSL2/ADSL2+ or to the whole
                       -- upstream traffic for VDSL2).
        downstream(2), -- Transmission from the xTU-C to the xTU-R
                       -- (refers to the single downstream band
                       -- for ADSL/ADSL2/ADSL2+ or to the whole
                       -- downstream traffic for VDSL2).
        us0(3),        -- Upstream band number 0   (US0) (VDSL2).
        ds1(4),        -- Downstream band number 1 (DS1) (VDSL2).
        us1(5),        -- Upstream band number 1   (US1) (VDSL2).
        ds2(6),        -- Downstream band number 2 (DS2) (VDSL2).
        us2(7),        -- Upstream band number 2   (US2) (VDSL2).
        ds3(8),        -- Downstream band number 3 (DS3) (VDSL2).
        us3(9),        -- Upstream band number 3   (US3) (VDSL2).
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        ds4(10),       -- Downstream band number 4 (DS4) (VDSL2).
        us4(11)        -- Upstream band number 4   (US4) (VDSL2).
            }
Xdsl2TransmissionModeType ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "A set of xDSL line transmission modes, with one bit
       per mode.  The notes (F) and (L) denote Full-Rate and
       Lite/splitterless respectively:
          Bit 00 : Regional Std. (ANSI T1.413) (F)
          Bit 01 : Regional Std. (ETSI DTS/TM06006) (F)
          Bit 02 : G.992.1 POTS non-overlapped (F)
          Bit 03 : G.992.1 POTS overlapped (F)
          Bit 04 : G.992.1 ISDN non-overlapped (F)
          Bit 05 : G.992.1 ISDN overlapped (F)
          Bit 06 : G.992.1 TCM-ISDN non-overlapped (F)
          Bit 07 : G.992.1 TCM-ISDN overlapped (F)
          Bit 08 : G.992.2 POTS non-overlapped (L)
          Bit 09 : G.992.2 POTS overlapped (L)
          Bit 10 : G.992.2 with TCM-ISDN non-overlapped (L)
          Bit 11 : G.992.2 with TCM-ISDN overlapped (L)
          Bit 12 : G.992.1 TCM-ISDN symmetric (F) --- not in G.997.1
          Bit 13-17: Reserved
          Bit 18 : G.992.3 POTS non-overlapped (F)
          Bit 19 : G.992.3 POTS overlapped (F)
          Bit 20 : G.992.3 ISDN non-overlapped (F)
          Bit 21 : G.992.3 ISDN overlapped (F)
          Bit 22-23: Reserved
          Bit 24 : G.992.4 POTS non-overlapped (L)
          Bit 25 : G.992.4 POTS overlapped (L)
          Bit 26-27: Reserved
          Bit 28 : G.992.3 Annex I All-Digital non-overlapped (F)
          Bit 29 : G.992.3 Annex I All-Digital overlapped (F)
          Bit 30 : G.992.3 Annex J All-Digital non-overlapped (F)
          Bit 31 : G.992.3 Annex J All-Digital overlapped (F)
          Bit 32 : G.992.4 Annex I All-Digital non-overlapped (L)
          Bit 33 : G.992.4 Annex I All-Digital overlapped (L)
          Bit 34 : G.992.3 Annex L POTS non-overlapped, mode 1,
                                   wide U/S (F)
          Bit 35 : G.992.3 Annex L POTS non-overlapped, mode 2,
                                   narrow U/S(F)
          Bit 36 : G.992.3 Annex L POTS overlapped, mode 3,
                                   wide U/S (F)
          Bit 37 : G.992.3 Annex L POTS overlapped, mode 4,
                                   narrow U/S (F)
          Bit 38 : G.992.3 Annex M POTS non-overlapped (F)
          Bit 39 : G.992.3 Annex M POTS overlapped (F)
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          Bit 40 : G.992.5 POTS non-overlapped (F)
          Bit 41 : G.992.5 POTS overlapped (F)
          Bit 42 : G.992.5 ISDN non-overlapped (F)
          Bit 43 : G.992.5 ISDN overlapped (F)
          Bit 44-45: Reserved
          Bit 46 : G.992.5 Annex I All-Digital non-overlapped (F)
          Bit 47 : G.992.5 Annex I All-Digital overlapped (F)
          Bit 48 : G.992.5 Annex J All-Digital non-overlapped (F)
          Bit 49 : G.992.5 Annex J All-Digital overlapped (F)
          Bit 50 : G.992.5 Annex M POTS non-overlapped (F)
          Bit 51 : G.992.5 Annex M POTS overlapped (F)
          Bit 52-55: Reserved
          Bit 56 : G.993.2 Annex A
          Bit 57 : G.993.2 Annex B
          Bit 58 : G.993.2 Annex C
          Bit 59-63: Reserved"
   SYNTAX      BITS {
                  ansit1413(0),
                  etsi(1),
                  g9921PotsNonOverlapped(2),
                  g9921PotsOverlapped(3),
                  g9921IsdnNonOverlapped(4),
                  g9921isdnOverlapped(5),
                  g9921tcmIsdnNonOverlapped(6),
                  g9921tcmIsdnOverlapped(7),
                  g9922potsNonOverlapped(8),
                  g9922potsOverlapped(9),
                  g9922tcmIsdnNonOverlapped(10),
                  g9922tcmIsdnOverlapped(11),
                  g9921tcmIsdnSymmetric(12),
                  reserved1(13),
                  reserved2(14),
                  reserved3(15),
                  reserved4(16),
                  reserved5(17),
                  g9923PotsNonOverlapped(18),
                  g9923PotsOverlapped(19),
                  g9923IsdnNonOverlapped(20),
                  g9923isdnOverlapped(21),
                  reserved6(22),
                  reserved7(23),
                  g9924potsNonOverlapped(24),
                  g9924potsOverlapped(25),
                  reserved8(26),
                  reserved9(27),
                  g9923AnnexIAllDigNonOverlapped(28),
                  g9923AnnexIAllDigOverlapped(29),
                  g9923AnnexJAllDigNonOverlapped(30),
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                  g9923AnnexJAllDigOverlapped(31),
                  g9924AnnexIAllDigNonOverlapped(32),
                  g9924AnnexIAllDigOverlapped(33),
                  g9923AnnexLMode1NonOverlapped(34),
                  g9923AnnexLMode2NonOverlapped(35),
                  g9923AnnexLMode3Overlapped(36),
                  g9923AnnexLMode4Overlapped(37),
                  g9923AnnexMPotsNonOverlapped(38),
                  g9923AnnexMPotsOverlapped(39),
                  g9925PotsNonOverlapped(40),
                  g9925PotsOverlapped(41),
                  g9925IsdnNonOverlapped(42),
                  g9925isdnOverlapped(43),
                  reserved10(44),
                  reserved11(45),
                  g9925AnnexIAllDigNonOverlapped(46),
                  g9925AnnexIAllDigOverlapped(47),
                  g9925AnnexJAllDigNonOverlapped(48),
                  g9925AnnexJAllDigOverlapped(49),
                  g9925AnnexMPotsNonOverlapped(50),
                  g9925AnnexMPotsOverlapped(51),
                  reserved12(52),
                  reserved13(53),
                  reserved14(54),
                  reserved15(55),
                  g9932AnnexA(56),
                  g9932AnnexB(57),
                  g9932AnnexC(58),
                  reserved16(59),
                  reserved17(60),
                  reserved18(61),
                  reserved19(62),
                  reserved20(63)
               }
Xdsl2RaMode ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Specifies the rate adaptation behavior for the line.
       The three possible behaviors are:
        manual (1)   - No Rate-Adaptation.  The initialization
                       process attempts to synchronize to a
                       specified rate.
        raInit (2)   - Rate-Adaptation during initialization process
                       only, which attempts to synchronize to a rate
                       between minimum and maximum specified values.
        dynamicRa (3)- Dynamic Rate-Adaptation during initialization
                       process as well as during SHOWTIME"
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   SYNTAX      INTEGER {
                  manual(1),
                  raInit(2),
                  dynamicRa(3)
               }
Xdsl2InitResult ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Specifies the result of full initialization attempt; the
       six possible result values are:
        noFail (0)            - Successful initialization
        configError (1)       - Configuration failure
        configNotFeasible (2) - Configuration details not supported
        commFail (3)          - Communication failure
        noPeerAtu (4)         - Peer ATU not detected
        otherCause (5)        - Other initialization failure
        reason"
   SYNTAX      INTEGER {
                  noFail(0),
                  configError(1),
                  configNotFeasible(2),
                  commFail(3),
                  noPeerAtu(4),
                  otherCause(5)
               }
Xdsl2OperationModes ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "The VDSL2 management model specified includes an xDSL Mode
       attribute which identifies an instance of xDSL Mode-Specific
       PSD Configuration object in the xDSL Line Profile.  The
       following classes of xDSL operating mode are defined.
       The notes (F) and (L) denote Full-Rate and Lite/splitterless
       respectively:
       +-------+--------------------------------------------------+
       | Value |         xDSL operation mode description          |
       +-------+--------------------------------------------------+
           1   - The default/generic PSD configuration.  Default
                 configuration will be used when no other matching
                 mode-specific configuration can be found.
           2   - Regional Std. (ANSI T1.413) (F)
           3   - Regional Std. (ETSI DTS/TM06006) (F)
           4   - G.992.1 POTS non-overlapped (F)
           5   - G.992.1 POTS overlapped (F)
           6   - G.992.1 ISDN non-overlapped (F)
           7   - G.992.1 ISDN overlapped (F)
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           8   - G.992.1 TCM-ISDN non-overlapped (F)
           9   - G.992.1 TCM-ISDN overlapped (F)
          10   - G.992.2 POTS non-overlapped (L)
          11   - G.992.2 POTS overlapped (L)
          12   - G.992.2 with TCM-ISDN non-overlapped (L)
          13   - G.992.2 with TCM-ISDN overlapped (L)
          14   - G.992.1 TCM-ISDN symmetric (F) --- not in G.997.1
        15-19  - Unused. Reserved for future ITU-T specification.
          20   - G.992.3 POTS non-overlapped (F)
          21   - G.992.3 POTS overlapped (F)
          22   - G.992.3 ISDN non-overlapped (F)
          23   - G.992.3 ISDN overlapped (F)
        24-25  - Unused. Reserved for future ITU-T specification.
          26   - G.992.4 POTS non-overlapped (L)
          27   - G.992.4 POTS overlapped (L)
        28-29  - Unused. Reserved for future ITU-T specification.
          30   - G.992.3 Annex I All-Digital non-overlapped (F)
          31   - G.992.3 Annex I All-Digital overlapped (F)
          32   - G.992.3 Annex J All-Digital non-overlapped (F)
          33   - G.992.3 Annex J All-Digital overlapped (F)
          34   - G.992.4 Annex I All-Digital non-overlapped (L)
          35   - G.992.4 Annex I All-Digital overlapped (L)
          36   - G.992.3 Annex L POTS non-overlapped, mode 1,
                 wide U/S (F)
          37   - G.992.3 Annex L POTS non-overlapped, mode 2,
                 narrow U/S(F)
          38   - G.992.3 Annex L POTS overlapped, mode 3,
                 wide U/S (F)
          39   - G.992.3 Annex L POTS overlapped, mode 4,
                 narrow U/S (F)
          40   - G.992.3 Annex M POTS non-overlapped (F)
          41   - G.992.3 Annex M POTS overlapped (F)
          42   - G.992.5 POTS non-overlapped (F)
          43   - G.992.5 POTS overlapped (F)
          44   - G.992.5 ISDN non-overlapped (F)
          45   - G.992.5 ISDN overlapped (F)
        46-47  - Unused. Reserved for future ITU-T specification.
          48   - G.992.5 Annex I All-Digital non-overlapped (F)
          49   - G.992.5 Annex I All-Digital overlapped (F)
          50   - G.992.5 Annex J All-Digital non-overlapped (F)
          51   - G.992.5 Annex J All-Digital overlapped (F)
          52   - G.992.5 Annex M POTS non-overlapped (F)
          53   - G.992.5 Annex M POTS overlapped (F)
        54-57  - Unused. Reserved for future ITU-T specification.
          58   - G.993.2 Annex A
          59   - G.993.2 Annex B
          60   - G.993.2 Annex C
      "
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   SYNTAX      INTEGER {
                  defMode(1),
                  ansit1413(2),
                  etsi(3),
                  g9921PotsNonOverlapped(4),
                  g9921PotsOverlapped(5),
                  g9921IsdnNonOverlapped(6),
                  g9921isdnOverlapped(7),
                  g9921tcmIsdnNonOverlapped(8),
                  g9921tcmIsdnOverlapped(9),
                  g9922potsNonOverlapped(10),
                  g9922potsOverlapped(11),
                  g9922tcmIsdnNonOverlapped(12),
                  g9922tcmIsdnOverlapped(13),
                  g9921tcmIsdnSymmetric(14),
                  g9923PotsNonOverlapped(20),
                  g9923PotsOverlapped(21),
                  g9923IsdnNonOverlapped(22),
                  g9923isdnOverlapped(23),
                  g9924potsNonOverlapped(26),
                  g9924potsOverlapped(27),
                  g9923AnnexIAllDigNonOverlapped(30),
                  g9923AnnexIAllDigOverlapped(31),
                  g9923AnnexJAllDigNonOverlapped(32),
                  g9923AnnexJAllDigOverlapped(33),
                  g9924AnnexIAllDigNonOverlapped(34),
                  g9924AnnexIAllDigOverlapped(35),
                  g9923AnnexLMode1NonOverlapped(36),
                  g9923AnnexLMode2NonOverlapped(37),
                  g9923AnnexLMode3Overlapped(38),
                  g9923AnnexLMode4Overlapped(39),
                  g9923AnnexMPotsNonOverlapped(40),
                  g9923AnnexMPotsOverlapped(41),
                  g9925PotsNonOverlapped(42),
                  g9925PotsOverlapped(43),
                  g9925IsdnNonOverlapped(44),
                  g9925isdnOverlapped(45),
                  g9925AnnexIAllDigNonOverlapped(48),
                  g9925AnnexIAllDigOverlapped(49),
                  g9925AnnexJAllDigNonOverlapped(50),
                  g9925AnnexJAllDigOverlapped(51),
                  g9925AnnexMPotsNonOverlapped(52),
                  g9925AnnexMPotsOverlapped(53),
                  g9932AnnexA(58),
                  g9932AnnexB(59),
                  g9932AnnexC(60)
               }
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Xdsl2PowerMngState ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Attributes with this syntax uniquely identify each power
       management state defined for the VDSL2/ADSL/ADSL2 or ADSL2+
       link.
       In VDSL2, only L0 and L3 states are defined.
       The possible values are:
         l0(1)              - (L0): Full power management state
         l1(2)              - (L1): Low power management state
                                    (for G.992.2)
         l2(3)              - (L2): Low power management state
                                    (for G.992.3, G.992.4 and G.992.5)
         l3(4)              - (L3): Idle power management state"
   SYNTAX      INTEGER {
                  l0(1),
                  l1(2),
                  l2(3),
                  l3(4)
               }
Xdsl2ConfPmsForce ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Attributes with this syntax are configuration parameters
       that reference the desired power management state for the
       VDSL2/ADSL/ADSL2 or ADSL2+ link
       In VDSL2, only L0 and L3 states are defined:
         l3toL0 (0)         - Perform a transition from L3 to L0
                              (Full power management state)
         l0toL2 (2)         - Perform a transition from L0 to L2
                              (Low power management state)
         l0orL2toL3 (3)     - Perform a transition into L3 (Idle
                              power management state)"
   SYNTAX      INTEGER {
                  l3toL0 (0),
                  l0toL2 (2),
                  l0orL2toL3 (3)
               }
Xdsl2LinePmMode ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "Attributes with this syntax are configuration parameters
       that reference the power modes/states into which the xTU-C or
       xTU-R may autonomously transit.
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       It is a BITS structure that allows control of the following
       transit options:
        allowTransitionsToIdle (0)    - xTU may autonomously transit
                                        to idle (L3) state.
        allowTransitionsToLowPower (1)- xTU may autonomously transit
                                        to low-power (L1/L2)
                                        state."
   SYNTAX BITS {
       allowTransitionsToIdle(0),
       allowTransitionsToLowPower(1)
     }
Xdsl2LineLdsf ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "Attributes with this syntax are configuration parameters
       that control the Loop Diagnostic mode for a VDSL2/ADSL/ADSL2
       or ADSL2+ link.  The possible values are:
         inhibit (0)  - Inhibit Loop Diagnostic mode
         force   (1)  - Force/Initiate Loop Diagnostic mode"
   SYNTAX INTEGER {
       inhibit(0),
       force(1)
     }
Xdsl2LdsfResult ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION
        "Possible failure reasons associated with performing
         Dual Ended Loop Test (DELT) on a DSL line.
         Possible values are:
          none        (1) - The default value in case LDSF was never
                            requested for the associated line.
          success     (2) - The recent command completed
                            successfully.
          inProgress  (3) - The Loop Diagnostics process is in
                            progress.
          unsupported (4) - The NE or the line card doesn't support
                            LDSF.
          cannotRun   (5) - The NE cannot initiate the command, due
                            to a nonspecific reason.
          aborted     (6) - The Loop Diagnostics process aborted.
          failed      (7) - The Loop Diagnostics process failed.
          illegalMode (8) - The NE cannot initiate the command, due
                            to the specific mode of the relevant
                            line.
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          adminUp     (9) - The NE cannot initiate the command, as
                            the relevant line is administratively
                            'Up'.
          tableFull   (10)- The NE cannot initiate the command, due
                            to reaching the maximum number of rows
                            in the results table.
          noResources (11)- The NE cannot initiate the command, due
                            to lack of internal memory resources."
     SYNTAX INTEGER {
          none (1),
          success (2),
          inProgress (3),
          unsupported (4),
          cannotRun (5),
          aborted (6),
          failed (7),
          illegalMode (8),
          adminUp (9),
          tableFull (10),
          noResources (11)
     }
Xdsl2LineBpsc ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "Attributes with this syntax are configuration parameters
       that control the bits per subcarrier measurement for a
       VDSL2/ADSL/ADSL2 or ADSL2+ link. The possible values are:
         idle    (1)  - Idle state
         measure (2)  - Measure the bits per subcarrier"
   SYNTAX INTEGER {
       idle(1),
       measure(2)
     }
Xdsl2BpscResult ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION
        "Possible failure reasons associated with performing
         a bits per subcarrier measurement on a DSL line.
         Possible values are:
          none        (1) - The default value, in case a measurement
                            was never requested for the associated
                            line.
          success     (2) - The recent measurement request completed
                            successfully.
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          inProgress  (3) - The bits per subcarrier measurement is
                            in progress.
          unsupported (4) - The bits per subcarrier request
                            mechanism is not supported.
          failed      (5) - The measurement request has failed and no
                            results are available.
          noResources (6) - The NE cannot initiate the command, due
                            to lack of internal memory resources."
     SYNTAX INTEGER {
          none(1),
          success(2),
          inProgress(3),
          unsupported(4),
          failed(5),
          noResources(6)
     }
Xdsl2LineReset ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "This type is used to request a line reset to occur.
          idle        (1) - This state indicates that there is
                            currently no request for a line reset.
          reset       (2) - This state indicates that a line reset
                            request has been issued."
   SYNTAX INTEGER {
       idle(1),
       reset(2)
     }
Xdsl2LineProfiles ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "Attributes with this syntax reference the list of
      ITU-T G.993.2 implementation profiles supported by an
      xTU, enabled on the VDSL2 line or active on that line."
      SYNTAX BITS {
          profile8a(0),
          profile8b(1),
          profile8c(2),
          profile8d(3),
          profile12a(4),
          profile12b(5),
          profile17a(6),
          profile30a(7)
     }
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Xdsl2LineClassMask ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "VDSL2 PSD Mask Class.
       The limit Power Spectral Density masks are grouped in
       the following PSD mask classes:
       Class 998     Annex A: D-32, D-48, D-64, D-128.
       Class 997-M1c Annex B: 997-M1c-A-7.
       Class 997-M1x Annex B: 997-M1x-M-8, 997-M1x-M.
       Class 997-M2x Annex B: 997-M2x-M-8, 997-M2x-A, 997-M2x-M,
                              997E17-M2x-NUS0, 997E30-M2x-NUS0.
       Class 998-M1x Annex B: 998-M1x-A, 998-M1x-B, 998-M1x-NUS0.
       Class 998-M2x Annex B: 998-M2x-A, 998-M2x-M, 998-M2x-B,
                              998-M2x-NUS0, 998E17-M2x-NUS0,
                              998E17-M2x-NUS0-M, 998E30-M2x-NUS0,
                              998E30-M2x-NUS0-M.
       Class 998ADE-M2x Annex B: Annex B: 998-M2x-A, 998-M2x-M,
                              998-M2x-B, 998-M2x-NUS0,
                              998ADE17-M2x-A, 998ADE17-M2x-B,
                              998ADE17-M2x-NUS0-M,
                              998ADE30-M2x-NUS0-A,
                              998ADE30-M2x-NUS0-M.
       Class 998-B   Annex C: POTS-138b, POTS-276b per C.2.1.1
                              in G.993.2, TCM-ISDN per C.2.1.2
                              in G.993.2.
       Class 998-CO  Annex C: POTS-138co, POTS-276co per C.2.1.1
                              in G.993.2.
       Class HPE-M1  Annex B: HPE17-M1-NUS0, HPE30-M1-NUS0."
   SYNTAX      INTEGER {
                  none(1),
                  a998ORb997M1cORc998B(2),
                  b997M1xOR998co(3),
                  b997M2x(4),
                  b998M1x(5),
                  b998M2x(6),
                  b998AdeM2x(7),
                  bHpeM1(8)
               }
Xdsl2LineLimitMask ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "The G.993.2 limit PSD mask for each class of profile.
      The profiles are grouped in following profile classes:
      - Class 8: Profiles 8a, 8b, 8c, 8d
      - Class 12: Profiles 12a, 12b
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      - Class 17: Profile 17a
      - Class 30: Profile 30a."
      SYNTAX BITS {
          profile8Limit1(0),
          profile8Limit2(1),
          profile8Limit3(2),
          profile8Limit4(3),
          profile8Limit5(4),
          profile8Limit6(5),
          profile8Limit7(6),
          profile8Limit8(7),
          profile8Limit9(8),
          profile8Limit10(9),
          profile8Limit11(10),
          profile8Limit12(11),
          profile8Limit13(12),
          profile8Limit14(13),
          profile8Limit15(14),
          profile8Limit16(15),
          --
          profile12Limit1(16),
          profile12Limit2(17),
          profile12Limit3(18),
          profile12Limit4(19),
          profile12Limit5(20),
          profile12Limit6(21),
          profile12Limit7(22),
          profile12Limit8(23),
          profile12Limit9(24),
          profile12Limit10(25),
          profile12Limit11(26),
          profile12Limit12(27),
          profile12Limit13(28),
          profile12Limit14(29),
          profile12Limit15(30),
          profile12Limit16(31),
          --
          profile17Limit1(32),
          profile17Limit2(33),
          profile17Limit3(34),
          profile17Limit4(35),
          profile17Limit5(36),
          profile17Limit6(37),
          profile17Limit7(38),
          profile17Limit8(39),
          profile17Limit9(40),
          profile17Limit10(41),
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          profile17Limit11(42),
          profile17Limit12(43),
          profile17Limit13(44),
          profile17Limit14(45),
          profile17Limit15(46),
          profile17Limit16(47),
          --
          profile30Limit1(48),
          profile30Limit2(49),
          profile30Limit3(50),
          profile30Limit4(51),
          profile30Limit5(52),
          profile30Limit6(53),
          profile30Limit7(54),
          profile30Limit8(55),
          profile30Limit9(56),
          profile30Limit10(57),
          profile30Limit11(58),
          profile30Limit12(59),
          profile30Limit13(60),
          profile30Limit14(61),
          profile30Limit15(62),
          profile30Limit16(63)
     }
Xdsl2LineUs0Disable ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "Indicates if US0 is disabled for each limit PSD mask.
      The profiles are grouped in following profile classes:
      - Class 8: Profiles 8a, 8b, 8c, 8d
      - Class 12: Profiles 12a, 12b
      - Class 17: Profile 17a
      - Class 30: Profile 30a."
      SYNTAX BITS {
          profile8Us0Disable1(0),
          profile8Us0Disable2(1),
          profile8Us0Disable3(2),
          profile8Us0Disable4(3),
          profile8Us0Disable5(4),
          profile8Us0Disable6(5),
          profile8Us0Disable7(6),
          profile8Us0Disable8(7),
          profile8Us0Disable9(8),
          profile8Us0Disable10(9),
          profile8Us0Disable11(10),
          profile8Us0Disable12(11),
Morgenstern, et al.      Expires January 8, 2009               [Page 49]
Internet-Draft               VDSL2-LINE MIB                    July 2008
          profile8Us0Disable13(12),
          profile8Us0Disable14(13),
          profile8Us0Disable15(14),
          profile8Us0Disable16(15),
          --
          profile12Us0Disable1(16),
          profile12Us0Disable2(17),
          profile12Us0Disable3(18),
          profile12Us0Disable4(19),
          profile12Us0Disable5(20),
          profile12Us0Disable6(21),
          profile12Us0Disable7(22),
          profile12Us0Disable8(23),
          profile12Us0Disable9(24),
          profile12Us0Disable10(25),
          profile12Us0Disable11(26),
          profile12Us0Disable12(27),
          profile12Us0Disable13(28),
          profile12Us0Disable14(29),
          profile12Us0Disable15(30),
          profile12Us0Disable16(31),
          --
          profile17Us0Disable1(32),
          profile17Us0Disable2(33),
          profile17Us0Disable3(34),
          profile17Us0Disable4(35),
          profile17Us0Disable5(36),
          profile17Us0Disable6(37),
          profile17Us0Disable7(38),
          profile17Us0Disable8(39),
          profile17Us0Disable9(40),
          profile17Us0Disable10(41),
          profile17Us0Disable11(42),
          profile17Us0Disable12(43),
          profile17Us0Disable13(44),
          profile17Us0Disable14(45),
          profile17Us0Disable15(46),
          profile17Us0Disable16(47),
          --
          profile30Us0Disable1(48),
          profile30Us0Disable2(49),
          profile30Us0Disable3(50),
          profile30Us0Disable4(51),
          profile30Us0Disable5(52),
          profile30Us0Disable6(53),
          profile30Us0Disable7(54),
          profile30Us0Disable8(55),
          profile30Us0Disable9(56),
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          profile30Us0Disable10(57),
          profile30Us0Disable11(58),
          profile30Us0Disable12(59),
          profile30Us0Disable13(60),
          profile30Us0Disable14(61),
          profile30Us0Disable15(62),
          profile30Us0Disable16(63)
     }
Xdsl2LineUs0Mask ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "The US0 PSD masks to be allowed by the near-end xTU on
      the line. This parameter is only defined for G.993.2 Annex A.
      It is represented as a bitmap (0 if not allowed and 1 if
      allowed) with the following definitions."
      SYNTAX BITS {
          eu32(0),
          eu36(1),
          eu40(2),
          eu44(3),
          eu48(4),
          eu52(5),
          eu56(6),
          eu60(7),
          --
          eu64(8),
          eu128(9),
          reserved1(10),
          reserved2(11),
          reserved3(12),
          reserved4(13),
          reserved5(14),
          reserved6(15),
          --
          adlu32(16),
          adlu36(17),
          adlu40(18),
          adlu44(19),
          adlu48(20),
          adlu52(21),
          adlu56(22),
          adlu60(23),
          --
          adlu64(24),
          adlu128(25),
          reserved7(26),
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          reserved8(27),
          reserved9(28),
          reserved10(29),
          reserved11(30),
          reserved12(31)
     }
Xdsl2SymbolProtection ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type specifies the minimum impulse noise protection
       for the bearer channel if it is transported over DMT symbols
       with a subcarrier spacing of 4.3125 kHz.
       The possible values are:
       noProtection (i.e., INP not required), halfSymbol (i.e., INP
       length is 1/2 symbol), and 1-16 symbols in steps of 1
       symbol"
   SYNTAX      INTEGER {
               noProtection (1),
               halfSymbol (2),
               singleSymbol (3),
               twoSymbols (4),
               threeSymbols (5),
               fourSymbols (6),
               fiveSymbols (7),
               sixSymbols (8),
               sevenSymbols (9),
               eightSymbols (10),
               nineSymbols (11),
               tenSymbols (12),
               elevenSymbols (13),
               twelveSymbols (14),
               thirteeSymbols (15),
               fourteenSymbols (16),
               fifteenSymbols (17),
               sixteenSymbols (18)
             }
Xdsl2SymbolProtection8 ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type specifies the minimum impulse noise protection
       for the bearer channel if it is transported over DMT symbols
       with a subcarrier spacing of 8.625 kHz.
       The possible values are:
       noProtection (i.e., INP not required) and 1-16 symbols in
       steps of 1 symbol"
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   SYNTAX      INTEGER {
               noProtection (1),
               singleSymbol (2),
               twoSymbols (3),
               threeSymbols (4),
               fourSymbols (5),
               fiveSymbols (6),
               sixSymbols (7),
               sevenSymbols (8),
               eightSymbols (9),
               nineSymbols (10),
               tenSymbols (11),
               elevenSymbols (12),
               twelveSymbols (13),
               thirteeSymbols (14),
               fourteenSymbols (15),
               fifteenSymbols (16),
               sixteenSymbols (17)
             }
Xdsl2MaxBer ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Attributes with this syntax are configuration parameters
       that reference the maximum Bit Error Rate (BER).
       The possible values are:
         eminus3 (1)  - Maximum BER=E^-3
         eminus5 (2)  - Maximum BER=E^-5
         eminus7 (3)  - Maximum BER=E^-7"
   SYNTAX      INTEGER {
                  eminus3(1),
                  eminus5(2),
                  eminus7(3)
               }
Xdsl2ChInitPolicy ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This syntax serves for channel configuration parameters
       that reference the channel initialization policy.
       The possible values are:
         policy0 (1) - Policy 0 according to the applicable standard
         policy1 (2) - Policy 1 according to the applicable
         standard"
   SYNTAX      INTEGER {
                  policy0(1),
                  policy1(2)
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               }
Xdsl2ScMaskDs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Each one of the 4096 bits in this OCTET STRING array
      represents the corresponding bin in the downstream direction.
      A value of one indicates that the bin is not in use."
   SYNTAX      OCTET STRING (SIZE(0..512))
Xdsl2ScMaskUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Each one of the 4096 bits in this OCTET STRING array
      represents the corresponding bin in the upstream direction.
      A value of one indicates that the bin is not in use."
   SYNTAX      OCTET STRING (SIZE(0..512))
Xdsl2CarMask ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type defines an array of bands. Each band is
       represented by 4 octets and there is a maximum of 32 bands
       allowed.
       Each band consists of a 16 bit start subcarrier index followed by
       a 16 bit stop subcarrier index."
   SYNTAX      OCTET STRING (SIZE(0..128))
Xdsl2RfiBands ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type defines a subset of downstream PSD mask
       breakpoints used to notch radio frequency interference (RFI)
       bands.
       Each RFI band is represented by 4 octets: 16 bit start subcarrier
       index followed by a 16 bit stop subcarrier index.
       There is a maximum of 16 RFI bands allowed."
   SYNTAX      OCTET STRING (SIZE(0..64))
Xdsl2PsdMaskDs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 32 PSD Mask
       breakpoints.
       Each breakpoint occupies 3 octets: The first
       two octets hold the index of the subcarrier associated with the
       breakpoint.  The third octet holds the PSD reduction at the
       breakpoint from 0 (0dBm/Hz) to 255 (-127.5 dBm/Hz) using units of
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       0.5dBm/Hz."
   SYNTAX      OCTET STRING (SIZE(0..96))
Xdsl2PsdMaskUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 16 PSD Mask
       breakpoints.
       Each breakpoint occupies 3 octets: The first two octets hold the
       index of the subcarrier associated with the breakpoint.  The
       third octet holds the PSD reduction at the breakpoint from 0
       (0dBm/Hz) to 255 (-127.5 dBm/Hz) using units of
       0.5dBm/Hz."
   SYNTAX      OCTET STRING (SIZE(0..48))
Xdsl2Tssi ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 32 transmit
       spectrum shaping (TSSi) breakpoints.
       Each breakpoint occupies 3 octets: The first two octets hold the
       index of the subcarrier associated with the breakpoint.  The
       third octet holds the shaping parameter at the breakpoint. It is
       a value from 0 to 126 (units of -0.5dB). The special value 127
       indicates that the subcarrier is not transmitted."
   SYNTAX      OCTET STRING (SIZE(0..96))
Xdsl2LastTransmittedState ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION
        "This parameter represents the last successful transmitted
         initialization state in the last full initialization performed
         on the line. States are per the specific xDSL technology and
         are
         numbered from 0 (if G.994.1 is used) or 1 (if G.994.1 is not
         used) up to Showtime."
     SYNTAX      INTEGER {
       -- ADSL family ATU-C side --
       atucG9941(0),
       atucQuiet1(1),
       atucComb1(2),
       atucQuiet2(3),
       atucComb2(4),
       atucIcomb1(5),
       atucLineprob(6),
       atucQuiet3(7),
       atucComb3(8),
       atucIComb2(9),
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       atucMsgfmt(10),
       atucMsgpcb(11),
       atucQuiet4(12),
       atucReverb1(13),
       atucTref1(14),
       atucReverb2(15),
       atucEct(16),
       atucReverb3(17),
       atucTref2(18),
       atucReverb4(19),
       atucSegue1(20),
       atucMsg1(21),
       atucReverb5(22),
       atucSegue2(23),
       atucMedley(24),
       atucExchmarker(25),
       atucMsg2(26),
       atucReverb6(27),
       atucSegue3(28),
       atucParams(29),
       atucReverb7(30),
       atucSegue4(31),
       atucShowtime(32),
       -- ADSL family ATU-R side --
       aturG9941(100),
       aturQuiet1(101),
       aturComb1(102),
       aturQuiet2(103),
       aturComb2(104),
       aturIcomb1(105),
       aturLineprob(106),
       aturQuiet3(107),
       aturComb3(108),
       aturIcomb2(109),
       aturMsgfmt(110),
       aturMsgpcb(111),
       aturReverb1(112),
       aturQuiet4(113),
       aturReverb2(114),
       aturQuiet5(115),
       aturReverb3(116),
       aturEct(117),
       aturReverb4(118),
       aturSegue1(119),
       aturReverb5(120),
       aturSegue2(121),
       aturMsg1(122),
       aturMedley(123),
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       aturExchmarker(124),
       aturMsg2(125),
       aturReverb6(126),
       aturSegue3(127),
       aturParams(128),
       aturReverb7(129),
       aturSegue4(130),
       aturShowtime(131),
       -- VDSL2 VTU-C side --
       vtucG9941(200),
       vtucQuiet1(201),
       vtucChDiscov1(202),
       vtucSynchro1(203),
       vtucPilot1(204),
       vtucQuiet2(205),
       vtucPeriodic1(206),
       vtucSynchro2(207),
       vtucChDiscov2(208),
       vtucSynchro3(209),
       vtucTraining1(210),
       vtucSynchro4(211),
       vtucPilot2(212),
       vtucTeq(213),
       vtucEct(214),
       vtucPilot3(215),
       vtucPeriodic2(216),
       vtucTraining2(217),
       vtucSynchro5(218),
       vtucMedley(219),
       vtucSynchro6(220),
       vtucShowtime(221),
       -- VDSL2 VTU-R side --
       vturG9941(300),
       vturQuiet1(301),
       vturChDiscov1(302),
       vturSynchro1(303),
       vturLineprobe(304),
       vturPeriodic1(305),
       vturSynchro2(306),
       vturChDiscov2(307),
       vturSynchro3(308),
       vturQuiet2(309),
       vturTraining1(310),
       vturSynchro4(311),
       vturTeq(312),
       vturQuiet3(313),
       vturEct(314),
       vturPeriodic2(315),
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       vturTraining2(316),
       vturSynchro5(317),
       vturMedley(318),
       vturSynchro6(319),
       vturShowtime(320)
     }
Xdsl2LineStatus ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "Attributes with this syntax are status parameters
       that reflect the failure status for a given end point of a
       VDSL2/ADSL/ADSL2 or ADSL2+ link.
       This BITS structure can report the following failures:
        noDefect (0)      - This bit position positively reports
                            that no defect or failure exist.
        lossOfFraming (1) - Loss of frame synchronization.
        lossOfSignal (2)  - Loss of signal.
        lossOfPower (3)   - Loss of power.  Usually this failure may
                            be reported for CPE units only.
        initFailure (4)   - Recent initialization process failed.
                            Never active on xTU-R."
   SYNTAX BITS {
       noDefect(0),
       lossOfFraming(1),
       lossOfSignal(2),
       lossOfPower(3),
       initFailure(4)
     }
Xdsl2ChInpReport ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type is used to indicate the method used to compute the
       ACTINP. If set to inpComputedUsingFormula(1), the ACTINP is
       computed according to the INP_no_erasure formula (9.6/G.993.2).
       If set to inpEstimatedByXtur(2), the ACTINP is the value
       estimated by the xTU receiver.
        inpComputedUsingFormula (1) - ACTINP computed using
                                      INP_no_erasure formula.
        inpEstimatedByXtur (2)      - ACTINP estimated by
                                      the xTU receiver."
   SYNTAX      INTEGER {
                  inpComputedUsingFormula(1),
                  inpEstimatedByXtur(2)
               }
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Xdsl2ChAtmStatus ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "Attributes with this syntax are status parameters that
      reflect the failure status for Transmission Convergence (TC)
      layer of a given ATM interface (data path over a VDSL2/ADSL/
      ADSL2 or ADSL2+ link).
      This BITS structure can report the following failures:
       noDefect (0)             - This bit position positively
                                  reports that no defect or failure
                                  exist.
       noCellDelineation (1)    - The link was successfully
                                  initialized but cell delineation
                                  was never acquired on the
                                  associated ATM data path.
       lossOfCellDelineation (2)- Loss of cell delineation on the
                                  associated ATM data path."
   SYNTAX BITS {
       noDefect(0),
       noCellDelineation(1),
       lossOfCellDelineation(2)
     }
Xdsl2ChPtmStatus ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "Attributes with this syntax are status parameters that
      reflect the failure status for a given PTM interface (packet
      data path over a VDSL2/ADSL/ADSL2 or ADSL2+ link).
      This BITS structure can report the following failures:
          noDefect (0)    - This bit position positively
                            reports that no defect or failure exist.
          outOfSync (1)   - Out of synchronization."
   SYNTAX BITS {
          noDefect(0),
          outOfSync(1)
     }
Xdsl2UpboKLF ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Defines the upstream power backoff force mode (UPBOKLF).
      The three possible mode values are:
          auto(1)         - The VTUs will autonomously determine the
                            electrical length.
          override(2)     - Forces the VTU-R to use the electrical
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                            length, kl0, of the CO-MIB (UPBOKL) to
                            compute the UPBO.
          disableUpbo(3)  - Disables UPBO such that UPBO is not
                            utilized."
   SYNTAX INTEGER {
     auto(1),
     override(2),
     disableUpbo(3)
     }
Xdsl2BandUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Each value identifies a specific band in the upstream
      transmission direction (Excluding US0 band.).
      The possible values which identify a band are as follows:
          us1(5)          - Upstream band number 1 (US1).
          us2(7)          - Upstream band number 2 (US2).
          us3(9)          - Upstream band number 3 (US3).
          us4(11)         - Upstream band number 4 (US4)."
   SYNTAX        INTEGER {
     us1(5),
     us2(7),
     us3(9),
     us4(11)
     }
Xdsl2LinePsdMaskSelectUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type is used to define which upstream PSD mask is
      enabled. This type is used only for Annexes J and M of ITU-T Recs
      G.992.3 and G.992.5.
      adlu32Eu32 (1),   - ADLU-32 / EU-32
      adlu36Eu36 (2),   - ADLU-36 / EU-36
      adlu40Eu40 (3),   - ADLU-40 / EU-40
      adlu44Eu44 (4),   - ADLU-44 / EU-44
      adlu48Eu48 (5),   - ADLU-48 / EU-48
      adlu52Eu52 (6),   - ADLU-52 / EU-52
      adlu56Eu56 (7),   - ADLU-56 / EU-56
      adlu60Eu60 (8),   - ADLU-60 / EU-60
      adlu64Eu64 (9)    - ADLU-64 / EU-64"
   SYNTAX        INTEGER {
     adlu32Eu32(1),
     adlu36Eu36(2),
     adlu40Eu40(3),
     adlu44Eu44(4),
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     adlu48Eu48(5),
     adlu52Eu52(6),
     adlu56Eu56(7),
     adlu60Eu60(8),
     adlu64Eu64(9)
     }
Xdsl2LineCeFlag ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type is used to enable the use of the optional
       cyclic extension values. If the bit is set to 1, the optional
       cyclic extension values may be used. Otherwise, the cyclic
       extension shall be forced to the mandatory length (5N/32)
      enableCyclicExtension (0) - Enable use of optional
                                  Cyclic Extension values."
   SYNTAX        BITS {
     enableCyclicExtension(0)
     }
Xdsl2LineSnrMode ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type is used to enable the transmitter referred
       virtual noise. The value of 1, indicates that virtual
       noise is disabled. The value of 2, indicates that virtual
       noise is enabled.
      virtualNoiseDisabled (1) - virtual noise is disabled.
      virtualNoiseEnabled (2)  - virtual noise is enabled."
   SYNTAX        INTEGER {
     virtualNoiseDisabled(1),
     virtualNoiseEnabled(2)
     }
Xdsl2LineTxRefVnDs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 32 PSD Mask
       breakpoints.
       Each breakpoint occupies 3 octets: The first two octets hold the
       index of the subcarrier associated with the breakpoint.  The
       third octet holds the PSD reduction at the breakpoint from 0
       (-140 dBm/Hz) to 200 (-40 dBm/Hz) using units of 0.5dBm/Hz.
       A special value of 255 indicates a noise level of 0 W/Hz."
   SYNTAX      OCTET STRING (SIZE(0..96))
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Xdsl2LineTxRefVnUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 16 PSD Mask
       breakpoints.
       Each breakpoint occupies 3 octets: The first two octets hold the
       index of the subcarrier associated with the breakpoint.  The
       third octet holds the PSD reduction at the breakpoint from 0
       (-140 dBm/Hz) to 200 (-40 dBm/Hz) using units of 0.5dBm/Hz.
       A special value of 255 indicates a noise level of 0 W/Hz."
   SYNTAX      OCTET STRING (SIZE(0..48))
Xdsl2LineForceInp ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "
       This type is being used for specifing that the framer
       settings of all the bearers of a line in any transmission
       direction shall be selected such that the impulse noise
       protection computed according to the formula specified
       in the relevant Recommendation is greater than or equal
       to the minimal impulse noise protection requirement.
      forceFramerForInp(0) -  Select framer setting to satisfy
                              impulse noise protection
                              requirements."
   SYNTAX        BITS {
     forceFramerForInp(0)
     }
Xdsl2BitsAlloc ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type specifies a array of nibbles, where each nibble
       indicates the bits allocation for a subcarrier.
       Each nibble has a value in the range 0 to 15 to indicate
       the bits allocation."
   SYNTAX      OCTET STRING (SIZE(0..256))
Xdsl2MrefPsdDs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Attributes with this syntax are MEDLEY Reference PSD status
       parameters in the downstream direction. This is expressed as
       the set of
       breakpoints exchanged at initialization.
       The OCTET STRING contains up to 48 pairs of values in the
       following structure:
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       Octets 0-1 -- Index of 1st subcarrier used in the
                   context of a first breakpoint.
       Octets 2-3 -- The PSD level for the subcarrier indicated
                   in octets 0-1.
       Octets 4-7 -- Same, for a 2nd breakpoint
       Octets 8-11 -- Same, for a 3rd breakpoint
       And so on until
       Octets 188-191 -- Same, for a 48th breakpoint.
       Each subcarrier index is an unsigned number in the range 1 to
       NSds (i.e., highest supported subcarrier index in the downstream
       direction).
       The PSD level is an integer value in the 0 to 4095 range. It is
       represented in units of 0.1 dB offset from -140dBm/Hz."
   SYNTAX      OCTET STRING (SIZE(0..192))
Xdsl2MrefPsdUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Attributes with this syntax are MEDLEY Reference PSD status
       parameters in the upstream direction. This is expressed
       as the set of
       breakpoints exchanged at initialization.
       The OCTET STRING contains up to 32 pairs of values in the
       following structure:
       Octets 0-1 -- Index of 1st subcarrier used in the
                   context of a first breakpoint.
       Octets 2-3 -- The PSD level for the subcarrier indicated
                   in octets 0-1.
       Octets 4-7 -- Same, for a 2nd breakpoint
       Octets 8-11 -- Same, for a 3rd breakpoint
       And so on until
       Octets 124-127 -- Same, for a 32nd breakpoint.
       Each subcarrier index is an unsigned number in the range 1 to
       NSus (i.e., highest supported subcarrier index in the upstream
       direction).
       The PSD level is an integer value in the 0 to 4095 range. It is
       represented in units of 0.1 dB offset from -140dBm/Hz."
   SYNTAX      OCTET STRING (SIZE(0..128))
END
VDSL2-LINE-MIB DEFINITIONS ::= BEGIN
IMPORTS
   MODULE-IDENTITY,
   OBJECT-TYPE,
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   transmission,
   Unsigned32,
   NOTIFICATION-TYPE,
   Integer32,
   Counter32
      FROM SNMPv2-SMI
   ifIndex
      FROM IF-MIB
   TruthValue,
   RowStatus
       FROM SNMPv2-TC
   SnmpAdminString
      FROM SNMP-FRAMEWORK-MIB
   HCPerfIntervalThreshold,
   HCPerfTimeElapsed
      FROM  HC-PerfHist-TC-MIB   -- [RFC3705]
   Xdsl2Unit,
   Xdsl2Direction,
   Xdsl2Band,
   Xdsl2TransmissionModeType,
   Xdsl2RaMode,
   Xdsl2InitResult,
   Xdsl2OperationModes,
   Xdsl2PowerMngState,
   Xdsl2ConfPmsForce,
   Xdsl2LinePmMode,
   Xdsl2LineLdsf,
   Xdsl2LdsfResult,
   Xdsl2LineBpsc,
   Xdsl2BpscResult,
   Xdsl2LineReset,
   Xdsl2SymbolProtection,
   Xdsl2SymbolProtection8,
   Xdsl2MaxBer,
   Xdsl2ChInitPolicy,
   Xdsl2ScMaskDs,
   Xdsl2ScMaskUs,
   Xdsl2CarMask,
   Xdsl2RfiBands,
   Xdsl2PsdMaskDs,
   Xdsl2PsdMaskUs,
   Xdsl2Tssi,
   Xdsl2LastTransmittedState,
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   Xdsl2LineStatus,
   Xdsl2ChInpReport,
   Xdsl2ChAtmStatus,
   Xdsl2ChPtmStatus,
   Xdsl2UpboKLF,
   Xdsl2BandUs,
   Xdsl2LineProfiles,
   Xdsl2LineUs0Mask,
   Xdsl2LineClassMask,
   Xdsl2LineLimitMask,
   Xdsl2LineUs0Disable,
   Xdsl2LinePsdMaskSelectUs,
   Xdsl2LineCeFlag,
   Xdsl2LineSnrMode,
   Xdsl2LineTxRefVnDs,
   Xdsl2LineTxRefVnUs,
   Xdsl2LineForceInp,
   Xdsl2BitsAlloc,
   Xdsl2MrefPsdDs,
   Xdsl2MrefPsdUs
          FROM   VDSL2-LINE-TC-MIB       -- [This document]
   MODULE-COMPLIANCE,
   OBJECT-GROUP,
   NOTIFICATION-GROUP
      FROM SNMPv2-CONF;
vdsl2MIB MODULE-IDENTITY
   LAST-UPDATED "200807010000Z" -- July 1, 2008
   ORGANIZATION "ADSLMIB Working Group"
   CONTACT-INFO "WG-email:  adslmib@ietf.org
   Info:      https://www1.ietf.org/mailman/listinfo/adslmib
             Chair:     Mike Sneed
                        Sand Channel Systems
             Postal:    P.O. Box 37324
                        Raleigh NC 27627-732
             Email:     sneedmike@hotmail.com
             Phone:     +1 206 600 7022
             Co-Chair:  Menachem Dodge
                        ECI Telecom Ltd.
             Postal:    30 Hasivim St.
                        Petach Tikva 49517,
                        Israel.
             Email:     mbdodge@ieee.org
Morgenstern, et al.      Expires January 8, 2009               [Page 65]
Internet-Draft               VDSL2-LINE MIB                    July 2008
             Phone:     +972 3 926 8421
             Co-editor: Moti Morgenstern
                        ECI Telecom Ltd.
             Postal:    30 Hasivim St.
                        Petach Tikva 49517,
                        Israel.
             Email:     moti.morgenstern@ecitele.com
             Phone:     +972 3 926 6258
             Co-editor: Scott Baillie
                        NEC Australia
             Postal:    649-655 Springvale Road,
                        Mulgrave, Victoria 3170,
                        Australia.
             Email:     scott.baillie@nec.com.au
             Phone:     +61 3 9264 3986
             Co-editor: Umberto Bonollo
                        NEC Australia
             Postal:    649-655 Springvale Road,
                        Mulgrave, Victoria 3170,
                        Australia.
             Email:     umberto.bonollo@nec.com.au
             Phone:     +61 3 9264 3385
            "
   DESCRIPTION
        "
         This document defines a Management Information Base (MIB)
         module for use with network management protocols in the
         Internet community for the purpose of managing VDSL2, ADSL,
         ADSL2, and ADSL2+ lines.
         The MIB module described in RFC 2662 [RFC2662] defines
         objects used for managing Asymmetric Bit-Rate DSL (ADSL)
         interfaces per [T1E1.413], [G.992.1], and [G.992.2].
         These object descriptions are based upon the specifications
         for the ADSL Embedded Operations Channel (EOC) as defined
         in American National Standards Institute (ANSI) T1E1.413
         [T1E1.413] and International Telecommunication Union (ITU-T)
         G.992.1 [G.992.1] and G.992.2 [G.992.2].
         The MIB module described in RFC 4706 [RFC4706] defines
         objects used for managing ADSL2 interfaces per [G.992.3]
         and [G.992.4], and ADSL2+ interfaces per [G.992.5]. That MIB
         is also capable of managing ADSL interfaces per [T1E1.413],
         [G.992.1], and [G.992.2].
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         This document does not obsolete RFC 2662 [RFC2662] and
         RFC 4706 [RFC4706], but rather provides a more comprehensive
         management model that manages VDSL2 interfaces per G.993.2
         [G.993.2] as well as ADSL, ADSL2 and ADSL2+ technologies
         per T1E1.413, G.992.1, G.992.2, G.992.3, G.992.4, and
         G.992.5
         ([T1E1.413], [G.992.1], [G.992.2], [G.992.3], [G.992.4], and
         [G.992.5] respectively).
         Additionally, the management framework for VDSL2 lines
         specified by the Digital Subscriber Line Forum
         (DSLF) has been taken into consideration [TR-129].  That
         framework is based on ITU-T G.997.1 standard [G.997.1] and
         its amendment 1 [G.997.1-Am1].
         The MIB module is located in the MIB tree under MIB 2
         transmission, as discussed in the MIB-2 Integration (RFC 2863
         [RFC2863]) section of this document.
         Copyright (C) The IETF Trust (2008).  This version of
         this MIB module is part of RFC XXXX: see the RFC itself for
         full legal notices."
-- RFC Ed.: replace XXXX with assigned number & remove this note
   REVISION "200807010000Z" -- July 1, 2008
   DESCRIPTION "Initial version, published as RFC XXXX."
-- RFC Ed.: replace XXXX with assigned number & remove this note
      ::= { transmission xxx }
-- IANA, please assign a branch number under transmission.
-- RFC Ed.: Please fill in xxx once assigned by IANA.
  vdsl2            OBJECT IDENTIFIER ::= { vdsl2MIB 1 }
  ------------------------------------------------
  xdsl2Line          OBJECT IDENTIFIER ::= { vdsl2 1 }
  xdsl2Status        OBJECT IDENTIFIER ::= { vdsl2 2 }
  xdsl2Inventory     OBJECT IDENTIFIER ::= { vdsl2 3 }
  xdsl2PM            OBJECT IDENTIFIER ::= { vdsl2 4 }
  xdsl2Profile       OBJECT IDENTIFIER ::= { vdsl2 5 }
  xdsl2Scalar        OBJECT IDENTIFIER ::= { vdsl2 6 }
  xdsl2Notifications OBJECT IDENTIFIER ::= { vdsl2 0 }
  xdsl2Conformance   OBJECT IDENTIFIER ::= { vdsl2 7 }
  ------------------------------------------------
  xdsl2PMLine      OBJECT IDENTIFIER ::= { xdsl2PM 1 }
  xdsl2PMChannel   OBJECT IDENTIFIER ::= { xdsl2PM 2 }
  ------------------------------------------------
  xdsl2ProfileLine      OBJECT IDENTIFIER ::= { xdsl2Profile 1 }
  xdsl2ProfileChannel   OBJECT IDENTIFIER ::= { xdsl2Profile 2 }
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  xdsl2ProfileAlarmConf OBJECT IDENTIFIER ::= { xdsl2Profile 3 }
  ------------------------------------------------
  xdsl2ScalarSC         OBJECT IDENTIFIER ::= { xdsl2Scalar 1 }
  ------------------------------------------------
------------------------------------------------
--          xdsl2LineTable                    --
------------------------------------------------
xdsl2LineTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2LineEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineTable contains configuration, command and
       status parameters of the VDSL2/ADSL/ADSL2 or ADSL2+ line.
       The index of this table is an interface index where the interface
       has an ifType of vdsl2(xxx).
       Several objects in this table MUST be maintained in a persistent
       manner."
   ::= { xdsl2Line 1 }
xdsl2LineEntry  OBJECT-TYPE
   SYNTAX      Xdsl2LineEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineTable contains configuration, commands
       and status parameters of the VDSL2/ADSL/ADSL2 or ADSL2+
       line."
   INDEX  { ifIndex }
   ::= { xdsl2LineTable 1 }
Xdsl2LineEntry  ::=
   SEQUENCE {
      xdsl2LineCnfgTemplate            SnmpAdminString,
      xdsl2LineCnfgFallbackTemplate    SnmpAdminString,
      xdsl2LineAlarmCnfgTemplate       SnmpAdminString,
      xdsl2LineCmndConfPmsf            Xdsl2ConfPmsForce,
      xdsl2LineCmndConfLdsf            Xdsl2LineLdsf,
      xdsl2LineCmndConfLdsfFailReason  Xdsl2LdsfResult,
      xdsl2LineCmndConfBpsc            Xdsl2LineBpsc,
      xdsl2LineCmndConfBpscFailReason  Xdsl2BpscResult,
      xdsl2LineCmndConfBpscReqCount    Unsigned32,
      xdsl2LineCmndAutomodeColdStart   TruthValue,
      xdsl2LineCmndConfReset           Xdsl2LineReset,
      xdsl2LineStatusActTemplate       SnmpAdminString,
      xdsl2LineStatusXtuTransSys       Xdsl2TransmissionModeType,
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      xdsl2LineStatusPwrMngState       Xdsl2PowerMngState,
      xdsl2LineStatusInitResult        Xdsl2InitResult,
      xdsl2LineStatusLastStateDs       Xdsl2LastTransmittedState,
      xdsl2LineStatusLastStateUs       Xdsl2LastTransmittedState,
      xdsl2LineStatusXtur              Xdsl2LineStatus,
      xdsl2LineStatusXtuc              Xdsl2LineStatus,
      xdsl2LineStatusAttainableRateDs  Unsigned32,
      xdsl2LineStatusAttainableRateUs  Unsigned32,
      xdsl2LineStatusActPsdDs          Integer32,
      xdsl2LineStatusActPsdUs          Integer32,
      xdsl2LineStatusActAtpDs          Integer32,
      xdsl2LineStatusActAtpUs          Integer32,
      xdsl2LineStatusActProfile        Xdsl2LineProfiles,
      xdsl2LineStatusActLimitMask      Xdsl2LineLimitMask,
      xdsl2LineStatusActUs0Mask        Xdsl2LineUs0Mask,
      xdsl2LineStatusActSnrModeDs      Xdsl2LineSnrMode,
      xdsl2LineStatusActSnrModeUs      Xdsl2LineSnrMode,
      xdsl2LineStatusElectricalLength  Unsigned32,
      xdsl2LineStatusTssiDs            Xdsl2Tssi,
      xdsl2LineStatusTssiUs            Xdsl2Tssi,
      xdsl2LineStatusMrefPsdDs         Xdsl2MrefPsdDs,
      xdsl2LineStatusMrefPsdUs         Xdsl2MrefPsdUs,
      xdsl2LineStatusTrellisDs         TruthValue,
      xdsl2LineStatusTrellisUs         TruthValue,
      xdsl2LineStatusActualCe          Unsigned32
   }
xdsl2LineCnfgTemplate  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the xDSL2
       Line Configuration Templates Table, xdsl2LineConfTemplateTable,
       that applies for this line.
       This object MUST be maintained in a persistent manner."
   REFERENCE    "DSL Forum TR-129, paragraph #5.1"
   DEFVAL       { "DEFVAL" }
   ::= { xdsl2LineEntry 1 }
xdsl2LineCnfgFallbackTemplate  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "This object is used to identify the template that will be
       used if the xDSL2 line fails to operate using the primary
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       template. The primary template is identified using the
       xdsl2LineCnfgTemplate attribute.
       For example, a xDSL2 line may fallback to a template with a lower
       rate if the rate specified in the primary template cannot be
       achieved.
       The value of this object identifies a row in the xDSL2 Line
       Configuration Template Table, xdsl2LineConfTemplateTable.
       Any row in the xdsl2LineConfTemplateTable table may be used as a
       fallback template.
       If the xDSL2 line fails to operate using the fallback template
       then the primary template should be retried.
       The xTU-C should continue to alternate between the primary and
       fallback templates until one of them succeeds.
       If the value of this object is a zero-length string then no
       fallback template is defined and only the primary template will
       be used.
       Note that implementation of this object is not mandatory.
       If this object is not supported, any attempt to modify this
       object should result in the SET request being rejected.
       This object MUST be maintained in a persistent manner."
   ::= { xdsl2LineEntry 2 }
xdsl2LineAlarmCnfgTemplate  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the xDSL2
       Line Alarm Configuration Template Table,
       xdsl2LineAlarmConfTemplateTable, which applies to this line.
       This object MUST be maintained in a persistent manner."
   REFERENCE    "DSL Forum TR-129, paragraph #5.1"
   DEFVAL       { "DEFVAL" }
   ::= { xdsl2LineEntry 3 }
xdsl2LineCmndConfPmsf  OBJECT-TYPE
   SYNTAX      Xdsl2ConfPmsForce
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "Power management state forced (PMSF).  Defines the line
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       states to be forced by the near-end xTU on this line.
       The various possible values are:
          l3toL0 (0),
          l0toL2 (2),
          l0orL2toL3 (3).
       This object MUST be maintained in a persistent manner."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.3 (PMSF)"
   DEFVAL       { l3toL0 }
   ::= { xdsl2LineEntry 4 }
xdsl2LineCmndConfLdsf  OBJECT-TYPE
   SYNTAX      Xdsl2LineLdsf
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "Loop diagnostics mode forced (LDSF).
       Defines whether the line should be forced into the loop
       diagnostics mode by the near-end xTU of this line. Note that
       a loop diagnostics may be initiated by the far-end xTU at any
       time.
       Only when the xdsl2LineStatusPwrMngState attribute is in the
       l3(4) state and the xdsl2LineCmndConfPmsf attribute is in the
       l0orL2toL3(3) state, can the line be forced into loop diagnostic
       mode procedures. Upon successful completion of the loop
       diagnostic mode procedures, the Access Node shall set this
       attribute to inhibit(0), and xdsl2LineStatusPwrMngState will
       remain in the l3(4) state. The loop diagnostic data shall be
       available at least until xdsl2LineCmndConfPmsf is set to the
       l3toL0(0) state.
       The results of the loop diagnostic procedure are stored in the
       tables xdsl2SCStatusTable, xdsl2SCStatusBandTable and
       xdsl2SCStatusSegmentTable. The status of the loop diagnostic
       procedue is indicated by xdsl2LineCmndConfLdsfFailReason.
       As long as loop diagnostic procedures are not completed
       successfully, attempts shall be made to do so, until the loop
       diagnostic mode is no longer forced on the line through this
       configuration parameter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.8 (LDSF)"
   DEFVAL       { inhibit }
   ::= { xdsl2LineEntry 5 }
xdsl2LineCmndConfLdsfFailReason  OBJECT-TYPE
   SYNTAX      Xdsl2LdsfResult
   MAX-ACCESS  read-only
Morgenstern, et al.      Expires January 8, 2009               [Page 71]
Internet-Draft               VDSL2-LINE MIB                    July 2008
   STATUS      current
   DESCRIPTION
      "The status of the most recent occasion when the Loop
       diagnostics mode forced (LDSF) command was issued for the
       associated line.
       Possible values are:
          none        (1) - The default value in case LDSF was never
                            requested for the associated line.
          success     (2) - The recent command completed
                            successfully.
          inProgress  (3) - The Loop Diagnostics process is in
                            progress.
          unsupported (4) - The NE or the line card doesn't support
                            LDSF.
          cannotRun   (5) - The NE cannot initiate the command, due
                            to a nonspecific reason.
          aborted     (6) - The Loop Diagnostics process aborted.
          failed      (7) - The Loop Diagnostics process failed.
          illegalMode (8) - The NE cannot initiate the command, due
                            to the specific mode of the relevant
                            line.
          adminUp     (9) - The NE cannot initiate the command, as
                            the relevant line is administratively
                            'Up'.
          tableFull   (10)- The NE cannot initiate the command, due
                            to reaching the maximum number of rows
                            in the results table.
          noResources (11)- The NE cannot initiate the command, due
                            to lack of internal memory resources."
   DEFVAL       { none }
   ::= { xdsl2LineEntry 6 }
xdsl2LineCmndConfBpsc  OBJECT-TYPE
   SYNTAX      Xdsl2LineBpsc
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "Request a bits per subcarrier measurement to be made.
       A request for a bits per subcarrier measurement is made by
       setting this attribute to the value of measure(2). Upon
       completion of the measurement request, the Access Node shall set
       this attribute to idle(1).
       Note that a bits per subcarrier measurement is also performed
       during a line diagnostic procedure. This attribute provides an
       additional mechanism to fetch the bits per subcarrier data. This
       additional mechanism is provided so that bits per subcarrier
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       data may be fetched without forcing the line into no power state.
       This is useful because the bits per subcarrier allocation may be
       adjusted at show time due to rate adaption and bit swapping.
       The implementation of this additional mechanism for measuring
       bits per subcarrier is not mandatory.
       The results of the bits per subcarrier measurement are stored in
       xdsl2LineSegmentTable. The status of the bits per subcarrier
       measurement is indicated by
       xdsl2LineCmndConfBpscFailReason."
   DEFVAL       { idle }
   ::= { xdsl2LineEntry 7 }
xdsl2LineCmndConfBpscFailReason  OBJECT-TYPE
   SYNTAX      Xdsl2BpscResult
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The status of the most recent bits per subcarrier
       measurement request issued for the associated line.
       Possible values are:
          none        (1) - The default value, in case a measurement
                            was never requested for the associated
                            line.
          success     (2) - The recent measurement request completed
                            successfully.
          inProgress  (3) - The bits per subcarrier measurement is
                            in progress.
          unsupported (4) - The bits per subcarrier request
                            mechanism is not supported.
          failed      (5) - The measurement request has failed and no
                            results are available.
          noResources (6) - The NE cannot initiate the command, due
                            to lack of internal memory resources."
   DEFVAL       { none }
   ::= { xdsl2LineEntry 8 }
xdsl2LineCmndConfBpscReqCount  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Measurement request counter.
       This counter is incremented by one every time a request for a
       measurement is made. A measurement request is made by setting the
       xdsl2LineCmndConfBpsc attribute to the value measure(2).
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       SNMP managers can use this attribute to check that the
       measurement results retrieved by the manager where not interupted
       by another measurement request."
   DEFVAL       { 0 }
   ::= { xdsl2LineEntry 9 }
xdsl2LineCmndAutomodeColdStart   OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "Automode cold start forced.  This parameter is defined in
       order to improve testing of the performance of xTUs supporting
       automode when it is enabled in the MIB.
       Change the value of this parameter to 'true' indicates a change
       in loop conditions applied to the devices under test.  The xTUs
       shall reset any historical information used for automode and for
       shortening G.994.1 handshake and initialization.
       Automode is the case where multiple operation-modes are enabled
       through the xdsl2LConfProfXtuTransSysEna object in the line
       configuration profile being used for the line, and where the
       selection of the actual operation-mode depends not only on the
       common capabilities of both xTUs (as exchanged in G.994.1), but
       also on achievable data rates under given loop conditions."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.10
                (Automode Cold Start Forced)"
   DEFVAL       { false }
   ::= { xdsl2LineEntry 10 }
xdsl2LineCmndConfReset   OBJECT-TYPE
      SYNTAX      Xdsl2LineReset
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "Request a line reset to occur.
          If this attribute is set to the value of reset(2), then force
          the line to reset (i.e., the modems will retrain).
          When the line has successfully reset, the SNMP agent will
          set the value of this attribute to idle(1).
          Note that the xdsl2LineCmndConfPmsf attribute will always take
          precedence over this attribute.
          If the xdsl2LineCmndConfPmsf attribute is set to the value
          l0orL2toL3(3), then the line MUST NOT return to the showtime
          state due to a reset request action performed using this
          attribute."
   DEFVAL       { idle }
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      ::= { xdsl2LineEntry 11 }
xdsl2LineStatusActTemplate  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This object is used to identify the template that is
       currently in use for this line.
       This attribute is updated when a successfull line initialisation
       occurs.
       This attribute indicates if the primary template
       (xdsl2LineCnfgTemplate) is in use or the fallback template
       (xdsl2LineCnfgFallbackTemplate) is in use.
       If the line is not successfully initialised then the value of
       this object will be a zero-length string."
   ::= { xdsl2LineEntry 12 }
xdsl2LineStatusXtuTransSys  OBJECT-TYPE
   SYNTAX      Xdsl2TransmissionModeType
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The xTU Transmission System (xTS) in use.
       It is coded in a bit-map representation with one bit set to
       '1' (the selected coding for the DSL line).  This
       parameter may be derived from the handshaking procedures defined
       in Recommendation G.994.1.  A set of xDSL line transmission
       modes, with one bit per mode."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.1
                (xDSL transmission system)"
   DEFVAL       { {} }
   ::= { xdsl2LineEntry 13 }
xdsl2LineStatusPwrMngState  OBJECT-TYPE
   SYNTAX      Xdsl2PowerMngState
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The current power management state.  One of four possible
       power management states:
          L0 - Synchronized and full transmission (i.e., Showtime).
          L1 - Low Power with reduced net data rate (G.992.2 only).
          L2 - Low Power with reduced net data rate (G.992.3 and
               G.992.4 only).
          L3 - No power.
      The various possible values are: l0(1), l1(2), l2(3), l3(4)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.5
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                (Line power management state)"
   DEFVAL       { l3 }
      ::= { xdsl2LineEntry 14 }
xdsl2LineStatusInitResult  OBJECT-TYPE
   SYNTAX      Xdsl2InitResult
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Indicates the result of the last full initialization
       performed on the line.  It is an enumeration type with the
       following values: noFail(0), configError(1),
       configNotFeasible(2), commFail(3), noPeerAtu(4),
       otherCause(5)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.6
                (Initialization success/failure cause)"
   DEFVAL       { noFail }
   ::= { xdsl2LineEntry 15 }
xdsl2LineStatusLastStateDs  OBJECT-TYPE
   SYNTAX      Xdsl2LastTransmittedState
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The last successful transmitted initialization state in
       the downstream direction in the last full initialization
       performed on the line."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.7
                (Downstream last transmitted state)"
   DEFVAL       { atucG9941 }
   ::= { xdsl2LineEntry 16 }
xdsl2LineStatusLastStateUs  OBJECT-TYPE
   SYNTAX      Xdsl2LastTransmittedState
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The last successful transmitted initialization state in the
       upstream direction in the last full initialization performed on
       the line."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.8
                (Upstream last transmitted state)"
   DEFVAL       { aturG9941 }
   ::= { xdsl2LineEntry 17 }
xdsl2LineStatusXtur  OBJECT-TYPE
   SYNTAX      Xdsl2LineStatus
   MAX-ACCESS  read-only
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   STATUS      current
   DESCRIPTION
      "Indicates current state (existing failures) of the xTU-R.
       This is a bit-map of possible conditions."
   REFERENCE    "ITU-T G.997.1, paragraph #7.1.1.2
                (Line far-end failures)"
   DEFVAL       { { noDefect } }
   ::= { xdsl2LineEntry 18 }
xdsl2LineStatusXtuc  OBJECT-TYPE
   SYNTAX      Xdsl2LineStatus
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Indicates current state (existing failures) of the xTU-C.
       This is a bit-map of possible conditions."
   REFERENCE    "ITU-T G.997.1, paragraph #7.1.1.1
                (Line near-end failures)"
   DEFVAL       { { noDefect } }
   ::= { xdsl2LineEntry 19 }
xdsl2LineStatusAttainableRateDs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Maximum Attainable Data Rate Downstream.
       The maximum downstream net data rate currently attainable by
       the xTU-C transmitter and the xTU-R receiver, coded in
       bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.19 (ATTNDRds)
   "
   DEFVAL       { 0 }
   ::= { xdsl2LineEntry 20 }
xdsl2LineStatusAttainableRateUs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Maximum Attainable Data Rate Upstream.
       The maximum upstream net data rate currently attainable by the
       xTU-R transmitter and the xTU-C receiver, coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.20 (ATTNDRus)
   "
   DEFVAL       { 0 }
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   ::= { xdsl2LineEntry 21 }
xdsl2LineStatusActPsdDs OBJECT-TYPE
   SYNTAX      Integer32 (-900..0 | 2147483647)
   UNITS       "0.1 dBm/Hz"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual Power Spectrum Density (PSD) Downstream.  The average
       downstream transmit PSD over the subcarriers used for downstream.
       It ranges from -900 to 0 units of 0.1 dBm/Hz (Physical values are
       -90 to 0 dBm/Hz).
       A value of 0x7FFFFFFF (2147483647) indicates the measurement is
       out of range to be represented."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.21 (ACTPSDds)
   "
   DEFVAL       { 2147483647 }
   ::= { xdsl2LineEntry 22 }
xdsl2LineStatusActPsdUs OBJECT-TYPE
   SYNTAX      Integer32 (-900..0 | 2147483647)
   UNITS       "0.1 dBm/Hz"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual Power Spectrum Density (PSD) Upstream.  The average
       upstream transmit PSD over the subcarriers used for upstream.
       It ranges from -900 to 0 units of 0.1 dBm/Hz (Physical values are
       -90 to 0 dBm/Hz).
       A value of 0x7FFFFFFF (2147483647) indicates the measurement is
       out of range to be represented."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.22 (ACTPSDus)
   "
   DEFVAL       { 2147483647 }
   ::= { xdsl2LineEntry 23 }
xdsl2LineStatusActAtpDs  OBJECT-TYPE
   SYNTAX      Integer32 (-310..310 | 2147483647)
   UNITS       "0.1 dBm"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual Aggregate Transmit Power Downstream.
       The total amount of transmit power delivered by the xTU-C at
       the U-C reference point, at the instant of measurement.  It
       ranges from -310 to 310 units of 0.1 dBm (Physical values are -31
       to 31 dBm).
       A value of 0x7FFFFFFF (2147483647) indicates the measurement is
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       out of range to be represented."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.24 (ACTATPds)
   "
   DEFVAL       { 2147483647 }
   ::= { xdsl2LineEntry 24 }
xdsl2LineStatusActAtpUs  OBJECT-TYPE
   SYNTAX      Integer32 (-310..310 | 2147483647)
   UNITS       "0.1 dBm"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual Aggregate Transmit Power Upstream.
       The total amount of transmit power delivered by the xTU-R at the
       U-R reference point, at the instant of measurement.  It ranges
       from -310 to 310 units of 0.1 dBm (Physical values are -31
       to 31 dBm).
       A value of 0x7FFFFFFF (2147483647) indicates the measurement is
       out of range to be represented."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.25 (ACTATPus)
   "
   DEFVAL       { 2147483647 }
   ::= { xdsl2LineEntry 25 }
xdsl2LineStatusActProfile  OBJECT-TYPE
   SYNTAX      Xdsl2LineProfiles
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The G.993.2 profile in use.
       The configuration parameter xdsl2LConfProfProfiles defines
       the set of allowed G.993.2 profiles. This parameter indicates
       the profile in use on this line.
       This parameter may be derived from the handshaking procedures
       defined in ITU-T Rec. G.994.1."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.2 (VDSL2 Profile)
   "
   DEFVAL       { {} }
   ::= { xdsl2LineEntry 26 }
xdsl2LineStatusActLimitMask  OBJECT-TYPE
   SYNTAX      Xdsl2LineLimitMask
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The Limit PSD mask and band plan in use.
       The configuration parameter xdsl2LConfProfLimitMask defines
       the set of allowed G.993.2 limit PSD masks.
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       This parameter indicates the limit PSD mask in use on this
       line."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.3
                (VDSL2 Limit PSD Mask and Band plan)"
   DEFVAL       { {} }
   ::= { xdsl2LineEntry 27 }
xdsl2LineStatusActUs0Mask  OBJECT-TYPE
   SYNTAX      Xdsl2LineUs0Mask
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The US0 PSD mask in use.
       The configuration parameter xdsl2LConfProfUs0Mask defines
       the set of allowed US0 PSD masks.
       This parameter indicates the US0 PSD mask in use on this line.
       This parameter may be derived from the handshaking procedures
       defined in ITU-T Rec. G.994.1."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.4
                (VDSL2 US0 PSD Mask)"
   DEFVAL       { {} }
   ::= { xdsl2LineEntry 28 }
xdsl2LineStatusActSnrModeDs  OBJECT-TYPE
   SYNTAX      Xdsl2LineSnrMode
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This parameter indicates if the transmitter
       referred virtual noise is active on the line in the downstream
       direction.
       The configuration parameter xdsl2LConfProfSnrModeDs is used to
       configure referred virtual noise."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.15 (ACTSNRMODEds)
   "
   DEFVAL       { virtualNoiseDisabled }
   ::= { xdsl2LineEntry 29 }
xdsl2LineStatusActSnrModeUs  OBJECT-TYPE
   SYNTAX      Xdsl2LineSnrMode
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This parameter indicates if the transmitter referred virtual
       noise is active on the line in the upstream direction.
       The configuration parameter xdsl2LConfProfSnrModeUs is used to
       configure referred virtual noise."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.18 (ACTSNRMODEus)
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   "
   DEFVAL       { virtualNoiseDisabled }
   ::= { xdsl2LineEntry 30 }
xdsl2LineStatusElectricalLength  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..1280)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This parameter contains the estimated electrical length
       expressed in dB at 1 MHz, kl0. This is the final electrical
       length that would have been sent from the VTU-O to VTU-R if the
       electrical length was not forced by the CO-MIB.
       The value ranges from 0 to 128 dB in steps of 0.1 dB."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.23 (UPBOKLE)"
   DEFVAL       { 0 }
   ::= { xdsl2LineEntry 31 }
xdsl2LineStatusTssiDs  OBJECT-TYPE
     SYNTAX      Xdsl2Tssi
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "The transmit spectrum shaping (TSSi) breakpoints expressed
      as the set of breakpoints exchanged during G.994.1.
      Each breakpoint is a pair of values occupying 3 octets with the
      following structure:
      First 2 octets - Index of the subcarrier used in the context of
                       the breakpoint.
      Third octet    - The shaping parameter at the breakpoint.
      Subcarrier index is an unsigned number in the range 1 to NSCds.
      The shaping parameter value is in the range 0 to 126 (units of
      -0.5dB). The special value 127 indicates that the subcarrier is
      not transmitted."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.29.5 (TSSpsds)"
     ::= { xdsl2LineEntry 32 }
xdsl2LineStatusTssiUs  OBJECT-TYPE
     SYNTAX      Xdsl2Tssi
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "The transmit spectrum shaping (TSSi) breakpoints expressed
      as the set of breakpoints exchanged during G.994.1.
      Each breakpoint is a pair of values occupying 3 octets with the
      following structure:
      First 2 octets - Index of the subcarrier used in the context of
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                       the breakpoint.
      Third octet    - The shaping parameter at the breakpoint.
      Subcarrier index is an unsigned number in the range 1 to NSCus.
      The shaping parameter value is in the range 0 to 126 (units of
      -0.5dB). The special value 127 indicates that the subcarrier is
      not transmitted."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.29.6 (TSSpsus)"
     ::= { xdsl2LineEntry 33 }
xdsl2LineStatusMrefPsdDs  OBJECT-TYPE
     SYNTAX      Xdsl2MrefPsdDs
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "The MEDLEY Reference PSD status parameters
      in the downstreasm
      direction expressed as the set of breakpoints exchanged at
      initialization.
      The OCTET STRING contains up to 48 pairs of values in the
      following structure:
      Octets 0-1 -- Index of 1st subcarrier used in the context
                  of a first breakpoint.
      Octets 2-3 -- The PSD level for the subcarrier indicated
                  in octets 0-1.
      Octets 4-7 -- Same, for a 2nd breakpoint
      Octets 8-11 -- Same, for a 3rd breakpoint
      And so on until
      Octets 188-191 -- Same, for a 48th breakpoint.
      Each subcarrier index is an unsigned number in the range 1 to
      NSds (i.e., highest supported subcarrier index in the downstream
      direction).
      The PSD level is an integer value in the 0 to 4095 range. It is
      represented in units of 0.1 dB offset from -140dBm/Hz."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.29.7 (MREFPSDds)
   "
     ::= { xdsl2LineEntry 34 }
xdsl2LineStatusMrefPsdUs  OBJECT-TYPE
     SYNTAX      Xdsl2MrefPsdUs
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "The MEDLEY Reference PSD status parameters in the
      upstreasm direction expressed as the set of breakpoints
      exchanged at initialization.
      The OCTET STRING contains up to 32 pairs of values in the
      following structure:
      Octets 0-1 -- Index of 1st subcarrier used in the context
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                   of a first breakpoint.
      Octets 2-3 -- The PSD level for the subcarrier indicated
                   in octets 0-1.
      Octets 4-7 -- Same, for a 2nd breakpoint
      Octets 8-11 -- Same, for a 3rd breakpoint
      And so on until
      Octets 124-127 -- Same, for a 32nd breakpoint.
      Each subcarrier index is an unsigned number in the range 1 to
      NSus (i.e., highest supported subcarrier index in the upstream
      direction).
      The PSD level is an integer value in the 0 to 4095 range. It is
      represented in units of 0.1 dB offset from -140dBm/Hz."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.29.8 (MREFPSDus)
   "
     ::= { xdsl2LineEntry 35 }
xdsl2LineStatusTrellisDs  OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This parameter reports whether trellis coding is in use in
      the downstream direction."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.30 (TRELLISds)
   "
   DEFVAL       { false }
   ::= { xdsl2LineEntry 36 }
xdsl2LineStatusTrellisUs  OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This parameter reports whether trellis coding is in use in
      the upstream direction."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.31 (TRELLISus)
   "
   DEFVAL       { false }
   ::= { xdsl2LineEntry 37 }
xdsl2LineStatusActualCe  OBJECT-TYPE
   SYNTAX      Unsigned32 (2..16)
   UNITS       "N/32 samples"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "(ACTUALCE)
       This parameter reports the cyclic extension used on the line. It
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       is coded as an unsigned integer from 2 to 16 in units of N/32
       samples, where 2N is the IDFT size."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.32 (ACTUALCE)
   "
   DEFVAL       { 2 }
   ::= { xdsl2LineEntry 38 }
------------------------------------------------
--          xdsl2LineSegmentTable             --
------------------------------------------------
xdsl2LineSegmentTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2LineSegmentEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineSegmentTable contains status parameters
       of VDSL2/ADSL/ADSL2 and ADSL2+ subcarriers.
       The parameters in this table are updated when a measurement
       request is made using the xdsl2LineCmndConfBpsc attribute.
       Note that a bits per subcarrier measurement is also performed
       during a line diagnostic procedure. This table provides an
       additional mechanism to fetch the bits per subcarrier data. This
       additional mechanism is provided so that bits per subcarrier
       data may be fetched without forcing the line into no power state.
       This is useful because the bits per subcarrier allocation may be
       adjusted at show time due to rate adaption and bit swapping.
       The implementation of this additional mechanism for measuring
       bits per subcarrier is not mandatory."
   ::= { xdsl2Status 1 }
xdsl2LineSegmentEntry  OBJECT-TYPE
   SYNTAX      Xdsl2LineSegmentEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineSegmentEntry contains status parameters
       of VDSL2/ADSL/ADSL2 and ADSL2+ subcarriers.
       Objects in the table refer to NSus and NSds. For G.993.2, the
       value of NSus and NSds are respectively the indices of the
       highest supported upstream and downstream subcarriers according
       to the selected implementation profile. For ADSL, NSus is equal
       to NSCus-1 and NSds is equal to NSCds-1.
       One index of this table is an interface index where the interface
       has an ifType of vdsl2(xxx). A second index of this table is the
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       transmission direction. A third index identifies the specific
       segment of the subcarriers status addressed."
   INDEX  { ifIndex,
            xdsl2LineSegmentDirection,
            xdsl2LineSegment   }
   ::= { xdsl2LineSegmentTable 1 }
Xdsl2LineSegmentEntry  ::=
   SEQUENCE {
      xdsl2LineSegmentDirection         Xdsl2Direction,
      xdsl2LineSegment                  Unsigned32,
      xdsl2LineSegmentBitsAlloc         Xdsl2BitsAlloc,
      xdsl2LineSegmentRowStatus         RowStatus
   }
xdsl2LineSegmentDirection  OBJECT-TYPE
     SYNTAX      Xdsl2Direction
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
     "The direction of the subcarrier either
      upstream or downstream."
     ::= { xdsl2LineSegmentEntry 1 }
xdsl2LineSegment  OBJECT-TYPE
     SYNTAX      Unsigned32(1..8)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
     "The segment of the subcarriers status information
      provided by this row.
      Status parameters in this table are retrieved in segments.
      The first segment of the status information is retrieved with
      xdsl2LineSegment=1, the second segment is retrieved with
      xdsl2LineSegment=2, and so on. When a status parameter is
      retrieved in n segments where n<8) then, for that parameter,
      GET operations for the remaining segment numbers (n+1 to 8) will
      respond with a zero-length OCTET STRING."
     ::= { xdsl2LineSegmentEntry 2 }
xdsl2LineSegmentBitsAlloc  OBJECT-TYPE
     SYNTAX      Xdsl2BitsAlloc
     UNITS       "bits"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "The bits allocation per subcarrier.  An array of 256 octets
      (512 nibbles), designed for supporting up to 512 (downstream)
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      subcarriers. When more then 512 subcarriers are supported, the
      status information is reported through multiple (up to 8)
      segments. The first segment is then used for the first 512
      subcarriers. The second segment is used for the subcarriers 512 to
      1023 and so on.
      The aggregate number of utilized nibbles on downstream direction
      (in all segments) depends on NSds, and on upstream direction it
      depends on NSus.
      This value is referred here as NS. The segment number is in
      xdsl2SCStatusSegment.
      Nibble i (0 <= i < MIN(NS-(segment-1)*512,512)) in each
      segment is set to a value in the range 0 to 15 to indicate that
      the respective downstream or upstream subcarrier j
      (j=(segement-1)*512+i) has the same amount of bits
      allocation."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.29.1 (BITSpsds)
                 and paragraph #7.5.1.29.2 (BITSpsus)"
     ::= { xdsl2LineSegmentEntry 3 }
xdsl2LineSegmentRowStatus  OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
     "Row Status.  The SNMP manager is not permitted to create rows
      in this table. The SNMP agent will create a row in this table for
      storing the results of a measurement performed on the associated
      line, if the row does not already exist.
      The SNMP agent may have limited resources; therefore, if multiple
      rows co-exist in this table, it may fail to add new rows to this
      table or allocate memory resources.
      If that occurs, the SNMP agent responds with the value
      'noResources' (for the xdsl2LineCmndConfBpscFailReason
      object in xdsl2LineTable).
      The management system (the operator) may delete rows from this
      table according to any scheme. E.g., after retrieving the results.
      When the SNMP manager deletes any row in this table, the SNMP
      agent MUST delete all rows in this table that have the same
      ifIndex value."
     ::= { xdsl2LineSegmentEntry 4 }
------------------------------------------------
--          xdsl2LineBandTable                --
------------------------------------------------
xdsl2LineBandTable  OBJECT-TYPE
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   SYNTAX      SEQUENCE  OF  Xdsl2LineBandEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineBandTable contains the, per-band line
       status parameters of the VDSL2/ADSL/ADSL2 or ADSL2+ line.
       The indexes of this table consist of an interface index where
       the interface has an ifType of vdsl2(xxx), together with a
       per-band index covering both VDSL2 and ADSL/ADSL2/ADSL2+.
       The parameters in this table are updated at line initialisation
       time and at showtime."
   ::= { xdsl2Line 2 }
xdsl2LineBandEntry  OBJECT-TYPE
   SYNTAX      Xdsl2LineBandEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineBandTable contains the, per-band line
       status parameters of the VDSL2/ADSL/ADSL2 or ADSL2+ line."
   INDEX  { ifIndex, xdsl2LineBand }
   ::= { xdsl2LineBandTable 1 }
Xdsl2LineBandEntry  ::=
   SEQUENCE {
      xdsl2LineBand                        Xdsl2Band,
      xdsl2LineBandStatusLnAtten           Unsigned32,
      xdsl2LineBandStatusSigAtten          Unsigned32,
      xdsl2LineBandStatusSnrMargin         Integer32
   }
xdsl2LineBand OBJECT-TYPE
     SYNTAX      Xdsl2Band
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
     "Identifies the band(s) associated with this line.
      For ADSL/ADSL2/ADSL2+ the values upstream(1) and downstream(2)
      will always be present.
      For VDSL2, a subset of {us0(3), ds1(4), us1(5) ... } will always
      be present (See Xdsl2Band for more details) together with rows for
      upstream(1) and downstream(2) in which only the
      xdsl2LineBandStatusSnrMargin attribute is expected to hold a valid
      (average) measurement."
     ::= { xdsl2LineBandEntry 1 }
xdsl2LineBandStatusLnAtten  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
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   UNITS       "0.1 dB"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Line Attenuation.
       When referring to a band in the downstream direction, it is
       the measured difference in the total power transmitted by the
       xTU-C and the total power received by the xTU-R over all
       subcarriers of that band during initialization.
       When referring to a band in the upstream direction, it is the
       measured difference in the total power transmitted by the xTU-R
       and the total power received by the xTU-C over all subcarriers of
       that band during initialization.
       Values range from 0 to 1270 in units of 0.1 dB (Physical values
       are 0 to 127 dB).
       A special value of 0x7FFFFFFF (2147483647) indicates the line
       attenuation is out of range to be represented.
       A special value of 0x7FFFFFFE (2147483646) indicates the line
       attenuation measurement is unavailable."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.9 (LATNds)
               and paragraph #7.5.1.10 (LATNus)6"
   DEFVAL       { 2147483646 }
   ::= { xdsl2LineBandEntry 2 }
xdsl2LineBandStatusSigAtten  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Signal Attenuation.
       When referring to a band in the downstream direction, it is
       the measured difference in the total power transmitted by the
       xTU-C and the total power received by the xTU-R over all
       subcarriers of that band during Showtime.
       When referring to a band in the upstream direction, it is the
       measured difference in the total power transmitted by the xTU-R
       and the total power received by the xTU-C over all subcarriers of
       that band during Showtime.
       Values range from 0 to 1270 in units of 0.1 dB (Physical values
       are 0 to 127 dB).
       A special value of 0x7FFFFFFF (2147483647) indicates the line
       attenuation is out of range to be represented.
       A special value of 0x7FFFFFFE (2147483646) indicates the line
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       attenuation measurement is unavailable."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.11 (SATNds)
               and paragraph #7.5.1.12 (SATNus)"
   DEFVAL       { 2147483646 }
   ::= { xdsl2LineBandEntry 3 }
xdsl2LineBandStatusSnrMargin  OBJECT-TYPE
   SYNTAX      Integer32 (-640..630 | 2147483646 | 2147483647)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "SNR Margin is the maximum increase in dB of the noise power
       received at the xTU (xTU-R for a band in the downstream direction
       and xTU-C for a band in the upstream direction), such that the
       BER requirements are met for all bearer channels received at the
       xTU. Values range from -640 to 630 in units of 0.1 dB (Physical
       values are -64 to 63 dB).
       A special value of 0x7FFFFFFF (2147483647) indicates the SNR
       Margin is out of range to be represented.
       A special value of 0x7FFFFFFE (2147483646) indicates the SNR
       Margin measurement is currently unavailable."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.13 (SNRMds)
               and paragraph #7.5.1.14 (SNRMpbds)
               and paragraph #7.5.1.16 (SNRMus)
               and paragraph #7.5.1.17 (SNRMpbus)"
   DEFVAL       { 2147483646 }
   ::= { xdsl2LineBandEntry 4 }
------------------------------------------------
--        xdsl2ChannelStatusTable             --
------------------------------------------------
xdsl2ChannelStatusTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2ChannelStatusEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2ChannelStatusTable contains status
       parameters of VDSL2/ADSL/ADSL2 or ADSL2+ channel.
       This table contains live data from equipment."
   ::= { xdsl2Status 2 }
xdsl2ChannelStatusEntry  OBJECT-TYPE
   SYNTAX      Xdsl2ChannelStatusEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2ChannelStatusTable contains status parameters
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       of VDSL2/ADSL/ADSL2 or ADSL2+ channel.
       The index of this table is an interface index where the interface
       has an ifType value that is applicable for a DSL channel and the
       termination unit."
   INDEX  { ifIndex, xdsl2ChStatusUnit }
   ::= { xdsl2ChannelStatusTable 1 }
Xdsl2ChannelStatusEntry  ::=
   SEQUENCE {
      xdsl2ChStatusUnit                Xdsl2Unit,
      xdsl2ChStatusActDataRate         Unsigned32,
      xdsl2ChStatusPrevDataRate        Unsigned32,
      xdsl2ChStatusActDelay            Unsigned32,
      xdsl2ChStatusActInp              Unsigned32,
      xdsl2ChStatusInpReport           Xdsl2ChInpReport,
      xdsl2ChStatusNFec                Unsigned32,
      xdsl2ChStatusRFec                Unsigned32,
      xdsl2ChStatusLSymb               Unsigned32,
      xdsl2ChStatusIntlvDepth          Unsigned32,
      xdsl2ChStatusIntlvBlock          Unsigned32,
      xdsl2ChStatusLPath               Unsigned32,
      xdsl2ChStatusAtmStatus           Xdsl2ChAtmStatus,
      xdsl2ChStatusPtmStatus           Xdsl2ChPtmStatus
   }
xdsl2ChStatusUnit  OBJECT-TYPE
   SYNTAX      Xdsl2Unit
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The termination unit xtuc(1) or xtur(2)."
   ::= { xdsl2ChannelStatusEntry 1 }
xdsl2ChStatusActDataRate  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The actual net data rate that the bearer channel is
       operating at, if in L0 power management state.  In L1 or L2
       states, it relates to the previous L0 state.  The data rate is
       coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.2.1
                (Actual data rate)"
   DEFVAL       { 0 }
   ::= { xdsl2ChannelStatusEntry 2 }
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xdsl2ChStatusPrevDataRate  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The previous net data rate that the bearer channel was
       operating at just before the latest rate change event.  This
       could be a full or short initialization, fast retrain, DRA or
       power management transitions, excluding transitions between L0
       state and L1 or L2 states.  The data rate is coded in
       bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.2.2
                (Previous data rate)"
   DEFVAL       { 0 }
   ::= { xdsl2ChannelStatusEntry 3 }
xdsl2ChStatusActDelay  OBJECT-TYPE
   SYNTAX      Unsigned32(0..8176)
   UNITS       "milliseconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The actual one-way interleaving delay introduced by the
       PMS-TC in the direction of the bearer channel, if in L0 power
       management state.  In L1 or L2 states, it relates to the previous
       L0 state.  It is coded in ms (rounded to the nearest ms)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.2.3
                (Actual interleaving delay)"
   DEFVAL       { 0 }
   ::= { xdsl2ChannelStatusEntry 4 }
xdsl2ChStatusActInp  OBJECT-TYPE
   SYNTAX      Unsigned32(0..255)
   UNITS       "0.1 symbols"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual impulse noise protection.
       This parameter reports the actual impulse noise protection (INP)
       on the bearer channel in the L0 state. In the L1 or L2 state, the
       parameter contains the INP in the previous L0 state. For ADSL,
       this value is computed according to the formula specified in the
       relevant Recommendation based on the actual framing parameters.
       For ITU-T Rec. G.993.2, the method to report this value is
       according to the INPREPORT parameter. The value is coded in
       fractions of DMT symbols with a granularity of 0.1 symbols.
       The range is from 0 to 25.4. The special value of 255 indicates
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       an ACTINP higher than 25.4."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.2.4 (ACTINP)"
   DEFVAL       { 0 }
   ::= { xdsl2ChannelStatusEntry 5 }
xdsl2ChStatusInpReport  OBJECT-TYPE
   SYNTAX      Xdsl2ChInpReport
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Impulse noise protection reporting mode.
       This parameter reports the method used to compute the ACTINP. If
       set to inpComputedUsingFormula(1), the ACTINP is computed
       according to the INP_no_erasure formula (9.6/G.993.2). If set to
       inpEstimatedByXtur(2), the ACTINP is the value estimated by the
       xTU receiver."
   REFERENCE    "ITU-T G.997.1 Amendment 1, paragraph #7.5.2.5
                (INPREPORT)"
   DEFVAL       { inpComputedUsingFormula }
   ::= { xdsl2ChannelStatusEntry 6 }
xdsl2ChStatusNFec  OBJECT-TYPE
   SYNTAX      Unsigned32(0..255)
   UNITS       "bytes"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual size of Reed-Solomon codeword.
       This parameter reports the actual number of Reed-Solomon
       redundancy bytes per codeword used in the latency path in which
       the bearer channel is transported. The value is coded in bytes.
       It ranges from 0 to 16.
       The value 0 indicates no Reed-Solomon coding."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.2.6.1 (NFEC)"
   DEFVAL       { 0 }
   ::= { xdsl2ChannelStatusEntry 7 }
xdsl2ChStatusRFec  OBJECT-TYPE
   SYNTAX      Unsigned32(0..16)
   UNITS       "bits"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual number of Reed-Solomon redundancy bytes.
       This parameter reports the actual number of Reed-Solomon
       redundancy bytes per codeword used in the latency path in which
       the bearer channel is transported. The value is coded in bytes.
       It ranges from 0 to 16.
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       The value 0 indicates no Reed-Solomon coding."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.2.6.2 (RFEC)"
   DEFVAL       { 0 }
   ::= { xdsl2ChannelStatusEntry 8 }
xdsl2ChStatusLSymb  OBJECT-TYPE
   SYNTAX      Unsigned32(0..65535)
   UNITS       "bits"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual number of bits per symbol.
       This parameter reports the actual number of bits per symbol
       assigned to the latency path in which the bearer channel is
       transported. This value does not include trellis overhead. The
       value is coded in bits.
       It ranges from 0 to 65535."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.2.6.3 (LSYMB)"
   DEFVAL       { 0 }
   ::= { xdsl2ChannelStatusEntry 9 }
xdsl2ChStatusIntlvDepth  OBJECT-TYPE
   SYNTAX      Unsigned32(1..4096)
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual interleaving depth.
       This parameter reports the actual depth of the interleaver used
       in the latency path in which the bearer channel is transported.
       The value ranges from 1 to 4096 in steps of 1.
       The value 1 indicates no interleaving."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.2.6.4 (INTLVDEPTH)
   "
   DEFVAL       { 1 }
   ::= { xdsl2ChannelStatusEntry 10 }
xdsl2ChStatusIntlvBlock  OBJECT-TYPE
   SYNTAX      Unsigned32(4..255)
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual interleaving block length.
       This parameter reports the actual block length of the interleaver
       used in the latency path in which the bearer channel is
       transported.
       The value ranges from 4 to 255 in steps of 1."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.2.6.5 (INTLVBLOCK)
   "
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   DEFVAL       { 4 }
   ::= { xdsl2ChannelStatusEntry 11 }
xdsl2ChStatusLPath  OBJECT-TYPE
   SYNTAX      Unsigned32(0..3)
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Actual latency path.
       This parameter reports the index of the actual latency path in
       which the bearer is transported.
       The valid values are 0, 1, 2 and 3.
       For G.992.1, the FAST path shall be mapped to the latency
       index 0, and the INTERLEAVED path shall be mapped to the latency
       index 1."
   REFERENCE    "ITU-T G.997.1 amendment 1, paragraph #7.5.2.7
   (LPATH)"
   DEFVAL       { 0 }
   ::= { xdsl2ChannelStatusEntry 12 }
xdsl2ChStatusAtmStatus  OBJECT-TYPE
   SYNTAX      Xdsl2ChAtmStatus
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Indicates current state (existing failures) of the DSL
       channel in case its Data Path is ATM.  This is a bit-map of
       possible conditions.  The various bit positions are:
          noDefect (0),
          noCellDelineation (1),
          lossOfCellDelineation (2).
      In case the channel is not of ATM Data Path the object is set
      to '0'."
   REFERENCE    "ITU-T G.997.1, paragraph #7.1.4
                (ATM data path failures)"
   DEFVAL       { { noDefect } }
   ::= { xdsl2ChannelStatusEntry 13 }
xdsl2ChStatusPtmStatus  OBJECT-TYPE
   SYNTAX      Xdsl2ChPtmStatus
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Indicates current state (existing failures) of the DSL
       channel in case its Data Path is PTM (Packet Transfer Mode).
       This is a bit-map of possible conditions.  The various bit
       positions are:
          noDefect (0),
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          outOfSync (1).
      In case the channel is not of PTM Data Path the object is set
      to '0'."
   REFERENCE    "ITU-T G.997.1, paragraph #7.1.5
                (PTM Data Path failures)"
   DEFVAL       { { noDefect } }
   ::= { xdsl2ChannelStatusEntry 14 }
------------------------------------------------
--    Scalars that relate to the SC Status Tables
------------------------------------------------
xdsl2ScalarSCMaxInterfaces  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This value determines the maximum number of
       interfaces supported by xdsl2SCStatusTable,
       xdsl2SCStatusBandTable, and xdsl2SCStatusSegmentTable."
   ::= { xdsl2ScalarSC 1 }
xdsl2ScalarSCAvailInterfaces  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This value determines the currently available number of
       interfaces listed in xdsl2SCStatusTable,
       xdsl2SCStatusBandTable, and xdsl2SCStatusSegmentTable."
   ::= { xdsl2ScalarSC 2 }
------------------------------------------------
--        xdsl2SCStatusTable                  --
------------------------------------------------
xdsl2SCStatusTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2SCStatusEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2SCStatusTable contains
       subcarrier status parameters for VDSL2/ADSL/ADSL2 and ADSL2+ that
       DO NOT refer to specific subcarriers.
       In addition, the table contains parameters that provide
       information about the size of parameters in
       xdsl2SCStatusSegmentTable.
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       The parameters in this table MUST be updated after a loop
       diagnostic procedure and MAY be updated after a line
       initialisation and MAY be updated at showtime."
   ::= { xdsl2Status 3 }
xdsl2SCStatusEntry  OBJECT-TYPE
   SYNTAX      Xdsl2SCStatusEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2SCStatusTable contains subcarrier status
       parameters for VDSL2/ADSL/ADSL2 and ADSL2+ that DO NOT refer to
       specific subcarriers.  In addition, the table contains parameters
       that provide information about the size of parameters in
       xdsl2SCStatusSegmentTable.
       One index of this table is an interface index where the interface
       has an ifType of vdsl2(xxx). A second index of this table is the
       transmission direction."
   INDEX  { ifIndex, xdsl2SCStatusDirection }
   ::= { xdsl2SCStatusTable 1 }
Xdsl2SCStatusEntry  ::=
   SEQUENCE {
      xdsl2SCStatusDirection         Xdsl2Direction,
      xdsl2SCStatusLinScale          Unsigned32,
      xdsl2SCStatusLinScGroupSize    Unsigned32,
      xdsl2SCStatusLogMt             Unsigned32,
      xdsl2SCStatusLogScGroupSize    Unsigned32,
      xdsl2SCStatusQlnMt             Unsigned32,
      xdsl2SCStatusQlnScGroupSize    Unsigned32,
      xdsl2SCStatusSnrMtime          Unsigned32,
      xdsl2SCStatusSnrScGroupSize    Unsigned32,
      xdsl2SCStatusAttainableRate    Unsigned32,
      xdsl2SCStatusRowStatus         RowStatus
   }
xdsl2SCStatusDirection  OBJECT-TYPE
     SYNTAX      Xdsl2Direction
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
     "The direction of the subcarrier either
      upstream or downstream."
     ::= { xdsl2SCStatusEntry 1 }
xdsl2SCStatusLinScale  OBJECT-TYPE
     SYNTAX      Unsigned32 (1..65535)
     MAX-ACCESS  read-only
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     STATUS      current
     DESCRIPTION
     "The scale factor to be applied to the H(f) linear
      representation values for the respective transmission direction.
      This parameter is only available after a loop diagnostic
      procedure. It is represented as an unsigned integer in the range
      from 1 to 2^16-1."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.26.1 (HLINSCds)
               and paragraph #7.5.1.26.7 (HLINSCus)"
     ::= { xdsl2SCStatusEntry 2 }
xdsl2SCStatusLinScGroupSize OBJECT-TYPE
     SYNTAX      Unsigned32(1 | 2 | 4 | 8)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "Number of subcarriers per group used to report the H(f)
      linear representation values for the respective transmission
      direction. The valid values are 1, 2, 4 and 8. For ADSL, this
      parameter is equal to one and, for VDSL2, it is equal to the size
      of a subcarrier group used to compute these parameters.
      This parameter is only available after a loop diagnostic
      procedure."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.26.2 (HLINGds)
               and paragraph #7.5.1.26.8 (HLINGus)"
     ::= { xdsl2SCStatusEntry 3 }
xdsl2SCStatusLogMt  OBJECT-TYPE
     SYNTAX      Unsigned32 (1..65535)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This parameter contains the number of symbols used to
      measure the Hlog(f) values. It is represented as an unsigned
      integer in the range from 1 to 2^16-1.
      After a loop diagnostic procedure, this parameter shall contain
      the number of symbols used to measure the Hlog(f). It should
      correspond to the value specified in the Recommendation (e.g., the
      number of symbols in 1 s time interval for ITU-T Rec.
      G.992.3)."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.26.4 (HLOGMTds)
               and paragraph #7.5.1.26.10 (HLOGMTus)"
     ::= { xdsl2SCStatusEntry 4 }
xdsl2SCStatusLogScGroupSize OBJECT-TYPE
     SYNTAX      Unsigned32(1 | 2 | 4 | 8)
     MAX-ACCESS  read-only
     STATUS      current
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     DESCRIPTION
     "Number of subcarriers per group used to report the H(f)
      logarithmic representation values for the respective
      transmission direction. The valid values are 1, 2, 4 and 8.
      For ADSL, this parameter is equal to one and, for VDSL2, it is
      equal to the size of a subcarrier group used to compute these
      parameters."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.26.5 (HLOGGds)
               and paragraph #7.5.1.26.11 (HLOGGus)"
     ::= { xdsl2SCStatusEntry 5 }
xdsl2SCStatusQlnMt  OBJECT-TYPE
     SYNTAX      Unsigned32 (1..65535)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This parameter contains the number of symbols used to
      measure the QLN(f) values. It is an unsigned integer in the range
      from 1 to 2^16-1. After a loop diagnostic procedure, this
      parameter shall contain the number of symbols used to measure the
      QLN(f). It should correspond to the value specified in the
      Recommendation (e.g., the number of symbols in 1 s time interval
      for ITU-T Rec. G.992.3)."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.27.1 (QLNMTds)
               and paragraph #7.5.1.27.4 (QLNMTus)"
     ::= { xdsl2SCStatusEntry 6 }
xdsl2SCStatusQlnScGroupSize OBJECT-TYPE
     SYNTAX      Unsigned32(1 | 2 | 4 | 8)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "Number of subcarriers per group used to report the Quiet
     Line Noise values for the respective transmission direction.
     The valid values are 1, 2, 4 and 8.
     For ADSL, this parameter is equal to one and, for VDSL2, it is
     equal to the size of a subcarrier group used to compute these
     parameters."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.27.2 (QLNGds)
               and paragraph #7.5.1.27.5 (QLNGus)"
     ::= { xdsl2SCStatusEntry 7 }
xdsl2SCStatusSnrMtime  OBJECT-TYPE
     SYNTAX      Unsigned32 (1..65535)
     UNITS       "symbols"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
Morgenstern, et al.      Expires January 8, 2009               [Page 98]
Internet-Draft               VDSL2-LINE MIB                    July 2008
     "This parameter contains the number of symbols used to measure
      the SNR(f) values. It is an unsigned integer in the range from 1
      to 2^16-1. After a loop diagnostic procedure, this parameter shall
      contain the number of symbols used to measure the SNR(f).
      It should correspond to the value specified in the Recommendation
      (e.g., the number of symbols in 1 s time interval for ITU-T Rec.
      G.992.3)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.28.1 (SNRMTds)
                 and paragraph #7.5.1.28.4 (SNRMTus)"
     ::= { xdsl2SCStatusEntry 8 }
xdsl2SCStatusSnrScGroupSize OBJECT-TYPE
     SYNTAX      Unsigned32(1 | 2 | 4 | 8)
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "Number of subcarriers per group used to report the SNR values
      on the respective transmission direction.
      The valid values are 1, 2, 4 and 8.
      For ADSL, this parameter is equal to one and, for VDSL2, it is
      equal to the size of a subcarrier group used to compute these
      parameters."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.28.2 (SNRGds)
               and paragraph #7.5.1.28.5 (SNRGus)"
     ::= { xdsl2SCStatusEntry 9 }
xdsl2SCStatusAttainableRate  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Maximum Attainable Data Rate.  The maximum net data rate
       currently attainable by the xTU-C transmitter and xTU-R receiver
       (when referring to downstream direction) or by the xTU-R
       transmitter and xTU-C receiver (when referring to upstream
       direction).  Value is coded in bits/s.
       This object reflects the value of the parameter following the
       most recent DELT performed on the associated line.  Once the DELT
       process is over, the parameter no longer changes until the row is
       deleted or a new DELT process is initiated.
       "
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.19 (ATTNDRds)
               and paragraph #7.5.1.20 (ATTNDRus)"
   ::= { xdsl2SCStatusEntry 10 }
xdsl2SCStatusRowStatus  OBJECT-TYPE
     SYNTAX      RowStatus
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     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
     "Row Status.  The SNMP manager is not permitted to create rows
      in this table. The SNMP agent will create a row in this table for
      storing the results of a DELT performed on the associated line, if
      the row does not already exist.
      When a row is created in this table, the SNMP agent should also
      create corresponding rows in the tables xdsl2SCStatusBandTable and
      xdsl2SCStatusSegmentTable.
      When a row is deleted in this table, the SNMP agent should also
      delete corresponding rows in the tables xdsl2SCStatusBandTable and
      xdsl2SCStatusSegmentTable.
      The SNMP agent may have limited resources; therefore, if multiple
      rows co-exist in this table, it may fail to add new rows to this
      table or allocate memory resources for a new DELT process.  If
      that occurs, the SNMP agent responds with either the value
      'tableFull' or the value 'noResources' (for
      the xdsl2LineCmndConfLdsfFailReason object in xdsl2LineTable).
      The management system (the operator) may delete rows from this
      table according to any scheme.  E.g., after retrieving the
      results."
     ::= { xdsl2SCStatusEntry 11 }
------------------------------------------------
--        xdsl2SCStatusBandTable              --
------------------------------------------------
xdsl2SCStatusBandTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2SCStatusBandEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2SCStatusBandTable contains subcarrier status
       parameters for VDSL2/ADSL/ADSL2 and ADSL2+ that are grouped per-
       band.
       For ADSL/ADSL2/ADSL2+, there is a single upstream band and a
       single downstream band.  For VDSL2, there are several downstream
       bands and several upstream bands.
       The parameters in this table are only available after a loop
       diagnostic procedure."
   ::= { xdsl2Status 4 }
xdsl2SCStatusBandEntry  OBJECT-TYPE
   SYNTAX      Xdsl2SCStatusBandEntry
   MAX-ACCESS  not-accessible
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   STATUS      current
   DESCRIPTION
      "The table xdsl2SCStatusBandTable contains subcarrier status
       parameters for VDSL2/ADSL/ADSL2 and ADSL2+ that are grouped per-
       band.
       For ADSL/ADSL2/ADSL2+, there is a single upstream band and a
       single downstream band.
       For VDSL2, there are several downstream bands and several
       upstream bands.
       One index of this table is an interface index where the interface
       has an ifType of vdsl2(xxx). A second index of this table is
       transmission band."
   INDEX  { ifIndex, xdsl2SCStatusBand }
   ::= { xdsl2SCStatusBandTable 1 }
Xdsl2SCStatusBandEntry  ::=
   SEQUENCE {
      xdsl2SCStatusBand                  Xdsl2Band,
      xdsl2SCStatusBandLnAtten           Unsigned32,
      xdsl2SCStatusBandSigAtten          Unsigned32
   }
xdsl2SCStatusBand OBJECT-TYPE
     SYNTAX      Xdsl2Band
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
     "The transmission band."
     ::= { xdsl2SCStatusBandEntry 1 }
xdsl2SCStatusBandLnAtten  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "When referring to a band in the downstream direction, it is
       the measured difference in the total power transmitted by the
       xTU-C and the total power received by the xTU-R over all
       subcarriers during diagnostics mode.
       When referring to a band in the upstream direction, it is the
       measured difference in the total power transmitted by the xTU-R
       and the total power received by the xTU-C over all subcarriers
       during diagnostics mode.
       It ranges from 0 to 1270 units of 0.1 dB (Physical values are 0
       to 127 dB).
       A special value of 0x7FFFFFFF (2147483647) indicates the line
       attenuation is out of range to be represented.
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       A special value of 0x7FFFFFFE (2147483646) indicates the line
       attenuation measurement is unavailable.
       This object reflects the value of the parameter following the
       most recent DELT performed on the associated line.  Once the DELT
       process is over, the parameter no longer changes until the row is
       deleted or a new DELT process is initiated."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.9 (LATNds)
               and paragraph #7.5.1.10 (LATNus)"
   DEFVAL       { 2147483646 }
   ::= { xdsl2SCStatusBandEntry 2 }
xdsl2SCStatusBandSigAtten  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..1270 | 2147483646 | 2147483647)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "When referring to a band the downstream direction, it is the
       measured difference in the total power transmitted by the xTU-C
       and the total power received by the xTU-R over all subcarriers
       during Showtime after the diagnostics mode.
       When referring to the upstream direction, it is the measured
       difference in the total power transmitted by the xTU-R and the
       total power received by the xTU-C over all subcarriers during
       Showtime after the diagnostics mode.
       It ranges from 0 to 1270 units of 0.1 dB (Physical values are 0
       to 127 dB).
       A special value of 0x7FFFFFFF (2147483647) indicates the line
       attenuation is out of range to be represented.
       A special value of 0x7FFFFFFE (2147483646) indicates the line
       attenuation measurement is unavailable.
       This object reflects the value of the parameter following the
       most recent DELT performed on the associated line.  Once the DELT
       process is over, the parameter no longer changes until the row is
       deleted or a new DELT process is initiated."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.11 (SATNds)
               and paragraph #7.5.1.12 (SATNus)"
   DEFVAL       { 2147483646 }
   ::= { xdsl2SCStatusBandEntry 3 }
------------------------------------------------
--        xdsl2SCStatusSegmentTable           --
------------------------------------------------
xdsl2SCStatusSegmentTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2SCStatusSegmentEntry
   MAX-ACCESS  not-accessible
   STATUS      current
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   DESCRIPTION
      "The table xdsl2SCStatusSegmentTable contains status
       parameters of VDSL2/ADSL/ADSL2 and ADSL2+ subcarriers.
       The parameters in this table MUST be updated after a loop
       diagnostic procedure and MAY be updated after a line
       initialisation and MAY be updated at showtime."
   ::= { xdsl2Status 5 }
xdsl2SCStatusSegmentEntry  OBJECT-TYPE
   SYNTAX      Xdsl2SCStatusSegmentEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2SCStatusSegmentEntry contains status
       parameters of VDSL2/ADSL/ADSL2 and ADSL2+ subcarriers.
       Several objects in the table refer to NSus and NSds. For G.993.2,
       the value of NSus and NSds are respectively the indices of the
       highest supported upstream and downstream subcarriers according
       to the selected implementation profile.
       For ADSL, NSus is equal to NSCus-1 and NSds is equal to NSCds-1.
       One index of this table is an interface index where the interface
       has an ifType of vdsl2(xxx). A second index of this table is the
       transmission direction. A third index identifies the specific
       segment of the subcarriers status addressed."
   INDEX  { ifIndex,
            xdsl2SCStatusDirection,
            xdsl2SCStatusSegment   }
   ::= { xdsl2SCStatusSegmentTable 1 }
Xdsl2SCStatusSegmentEntry  ::=
   SEQUENCE {
      xdsl2SCStatusSegment                  Unsigned32,
      xdsl2SCStatusSegmentLinReal           OCTET STRING,
      xdsl2SCStatusSegmentLinImg            OCTET STRING,
      xdsl2SCStatusSegmentLog               OCTET STRING,
      xdsl2SCStatusSegmentQln               OCTET STRING,
      xdsl2SCStatusSegmentSnr               OCTET STRING,
      xdsl2SCStatusSegmentBitsAlloc         Xdsl2BitsAlloc,
      xdsl2SCStatusSegmentGainAlloc         OCTET STRING
   }
xdsl2SCStatusSegment  OBJECT-TYPE
     SYNTAX      Unsigned32(1..8)
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
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     "The segment of the subcarriers status information provided by
      this row.
      Several status parameters in this table are retrieved in segments.
      The first segment of the status information is retrieved with
      xdsl2SCStatusSegment=1, the second segment is retrieved with
      xdsl2SCStatusSegment=2, and so on. When any status parameter is
      retrieved in n segments where n<8) then, for that parameter,
      GET operations for the remaining segment numbers (n+1 to 8) will
      respond with a zero-length OCTET STRING."
     ::= { xdsl2SCStatusSegmentEntry 1 }
xdsl2SCStatusSegmentLinReal  OBJECT-TYPE
     SYNTAX      OCTET STRING  (SIZE(0..1024))
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "An array of up to 512 complex H(f) linear representation
      values in linear scale for the respective transmission direction.
      It is designed to support up to 512 (downstream) subcarriers
      groups and can be retrieved in a single segment.
      The number of utilized values on downstream direction depends on
      NSds, and on upstream direction it depends on NSus.  This value is
      referred here as NS.
      Each array entry represents the real component [referred here as
      a(i)] of Hlin(f = i*Df) value for a particular subcarrier group
      index i (0 <= i < NS).
      Hlin(f) is represented as ((scale/2^15)*((a(i)+j*b(i))/2^15)),
      where scale is xdsl2SCStatusLinScale and a(i) and b(i)
      [provided by the xdsl2SCStatusSegmentLinImg object] are in the
      range (-2^15+1) to (+2^15-1).
      A special value a(i)=b(i)= -2^15 indicates that no measurement
      could be done for the subcarriers group because it is out of the
      passband or that the attenuation is out of range to be
      represented.  This parameter is only available after a loop
      diagnostic procedure.
      Each value in this array is 16 bits wide and is stored in big
      endian format."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.26.3 (HLINpsds)
               and paragraph #7.5.1.26.9 (HLINpsus)"
     ::= { xdsl2SCStatusSegmentEntry 2 }
xdsl2SCStatusSegmentLinImg  OBJECT-TYPE
     SYNTAX      OCTET STRING  (SIZE(0..1024))
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "An array of up to 512 complex H(f) linear representation
      values in linear scale for the respective transmission direction.
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      It is designed to support up to 512 (downstream) subcarriers
      groups and can be retrieved in a single segment.
      The number of utilized values on downstream direction depends on
      NSds, and on upstream direction it depends on NSus.  This value is
      referred here as NS.
      Each array entry represents the imaginary component [referred
      here as b(i)] of Hlin(f = i*Df) value for a particular
      subcarrier group index i (0 <= i < NS).
      Hlin(f) is represented as ((scale/2^15)*((a(i)+j*b(i))/2^15)),
      where scale is xdsl2SCStatusLinScale and a(i) [provided by the
      xdsl2SCStatusSegmentLinReal object] and b(i) are in the range
      (-2^15+1) to (+2^15-1).
      A special value a(i)=b(i)= -2^15 indicates that no measurement
      could be done for the subcarriers group because it is out of the
      passband or that the attenuation is out of range to be
      represented.  This parameter is only available after a loop
      diagnostic procedure.
      Each value in this array is 16 bits wide and is stored in big
      endian format."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.26.3 (HLINpsds)
               and paragraph #7.5.1.26.9 (HLINpsus)"
     ::= { xdsl2SCStatusSegmentEntry 3 }
xdsl2SCStatusSegmentLog  OBJECT-TYPE
     SYNTAX      OCTET STRING  (SIZE(0..1024))
     UNITS       "dB"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "An array of up to 512 real H(f) logarithmic representation
      values in dB for the respective transmission direction.  It is
      designed to support up to 512 (downstream) subcarriers groups
      and can be retrieved in a single segment.
      The number of utilized values on downstream direction depends
      on NSds, and on upstream direction it depends on NSus.  This
      value is referred here as NS.
      Each array entry represents the real Hlog(f = i*Df) value for a
      particular subcarrier group index i, (0 <= i < NS).
      The real Hlog(f) value is represented as (6-m(i)/10), with m(i)
      in the range 0 to 1022.  A special value m=1023 indicates that
      no measurement could be done for the subcarrier group because
      it is out of the passband or that the attenuation is out of
      range to be represented.  This parameter is applicable in loop
      diagnostic procedure and initialization.
      Each value in this array is 16 bits wide and is stored in big
      endian format."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.26.6 (HLOGpsds)
               and paragraph #7.5.1.26.12 (HLOGpsus)"
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     ::= { xdsl2SCStatusSegmentEntry 4 }
xdsl2SCStatusSegmentQln  OBJECT-TYPE
     SYNTAX      OCTET STRING  (SIZE(0..512))
     UNITS       "dBm/Hz"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "An array of up to 512 real Quiet Line Noise values in dBm/Hz
      for the respective transmission direction.  It is designed for up
      to 512 (downstream) subcarriers groups and can be retrieved in a
      single segment.
      The number of utilized values on downstream direction depends on
      NSds, and on upstream direction it depends on NSus.  This value is
      referred here as NS.
      Each array entry represents the QLN(f = i*Df) value for a
      particular subcarrier index i, (0 <= i < NS).
      The QLN(f) is represented as ( -23-n(i)/2), with n(i) in the range
      0 to 254.  A special value n(i)=255 indicates that no measurement
      could be done for the subcarrier group because it is out of the
      passband or that the noise PSD is out of range to be represented.
      This parameter is applicable in loop diagnostic procedure and
      initialization.  Each value in this array is 8 bits wide."
   REFERENCE  "ITU-T G.997.1, paragraph #7.5.1.27.3 (QLNpsds)
               and paragraph #7.5.1.27.6 (QLNpsus)"
     ::= { xdsl2SCStatusSegmentEntry 5 }
xdsl2SCStatusSegmentSnr  OBJECT-TYPE
     SYNTAX      OCTET STRING  (SIZE(0..512))
     UNITS       "0.5 dB"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "The SNR Margin per subcarrier group, expressing the ratio
      between the received signal power and received noise power per
      subscriber group.  It is an array of 512 octets, designed for
      supporting up to 512 (downstream) subcarriers groups and can be
      retrieved in a single segment.
      The number of utilized octets on downstream direction depends on
      NSds, and on upstream direction it depends on NSus.  This value is
      referred here as NS.
      Octet i (0 <= i < NS) is set to a value in the range 0 to
      254 to indicate that the respective downstream or upstream
      subcarrier group i has SNR of:
      (-32 + xdsl2SCStatusSegmentSnr(i)/2) in dB (i.e., -32 to 95dB).
      The special value 255 means that no measurement could be done for
      the subcarrier group because it is out of the PSD mask passband or
      that the noise PSD is out of range to be represented.  Each value
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      in this array is 8 bits wide."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.28.3 (SNRpsds)
                 and paragraph #7.5.1.28.6 (SNRpsus)"
     ::= { xdsl2SCStatusSegmentEntry 6 }
xdsl2SCStatusSegmentBitsAlloc  OBJECT-TYPE
     SYNTAX      Xdsl2BitsAlloc
     UNITS       "bits"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "The bits allocation per subcarrier.  An array of 256 octets
      (512 nibbles), designed for supporting up to 512 (downstream)
      subcarriers. When more then 512 subcarriers are supported, the
      status information is reported through multiple (up to 8)
      segments. The first segment is then used for the first 512
      subcarriers. The second segment is used for the subcarriers
      512 to 1023 and so on.
      The aggregate number of utilized nibbles on downstream direction
      (in all segments) depends on NSds, and on upstream direction it
      depends on NSus.
      This value is referred here as NS. The segment number is in
      xdsl2SCStatusSegment.
      Nibble i (0 <= i < MIN(NS-(segment-1)*512,512)) in each
      segment is set to a value in the range 0 to 15 to indicate that
      the respective downstream or upstream subcarrier j
      (j=(segement-1)*512+i) has the same amount of bits
      allocation."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.29.1 (BITSpsds)
                 and paragraph #7.5.1.29.2 (BITSpsus)"
     ::= { xdsl2SCStatusSegmentEntry 7 }
xdsl2SCStatusSegmentGainAlloc  OBJECT-TYPE
     SYNTAX      OCTET STRING  (SIZE(0..1024))
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "The gain allocation per subcarrier.  An array of 512 16-bits
      values, designed for supporting up to 512 (downstream)
      subcarriers. When more then 512 subcarriers are supported, the
      status information is reported through multiple (up to 8)
      segments. The first segment is then used for the first 512
      subcarriers. The second segment is used for the subcarriers 512 to
      1023 and so on.
      The aggregate number of utilized octets on downstream direction
      depends on NSds, and on upstream direction it depends on NSus.
      This value is referred here as NS. The segment number is in
      xdsl2SCStatusSegment.
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      Value i (0 <= i < MIN(NS-(segment-1)*512,512)) in each
      segment is set to a value in the range 0 to 4093 to indicate that
      the respective downstream or upstream subcarrier j
      (j=(segement-1)*512+i) has the same amount of gain value.
      The gain value is represented as a multiple of 1/512 on linear
      scale.  Each value in this array is 16 bits wide and is stored in
      big endian format."
   REFERENCE    "ITU-T G.997.1, paragraph #7.5.1.29.3 (GAINSpsds)
                 and paragraph #7.5.1.29.4 (GAINSpsus)"
     ::= { xdsl2SCStatusSegmentEntry 8 }
------------------------------------------------
--        xdsl2LineInventoryTable             --
------------------------------------------------
xdsl2LineInventoryTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2LineInventoryEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineInventoryTable contains inventory of the
       DSL termination unit."
   ::= { xdsl2Inventory 1 }
xdsl2LineInventoryEntry  OBJECT-TYPE
   SYNTAX      Xdsl2LineInventoryEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineInventoryTable contains inventory of DSL
       termination unit.
       The index of this table is an interface index where the interface
       has an ifType of vdsl2(xxx)."
   INDEX  { ifIndex, xdsl2LInvUnit }
   ::= { xdsl2LineInventoryTable 1 }
Xdsl2LineInventoryEntry  ::=
   SEQUENCE {
      xdsl2LInvUnit                      Xdsl2Unit,
      xdsl2LInvG994VendorId              OCTET STRING,
      xdsl2LInvSystemVendorId            OCTET STRING,
      xdsl2LInvVersionNumber             OCTET STRING,
      xdsl2LInvSerialNumber              OCTET STRING,
      xdsl2LInvSelfTestResult            Unsigned32,
      xdsl2LInvTransmissionCapabilities  Xdsl2TransmissionModeType
   }
xdsl2LInvUnit  OBJECT-TYPE
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   SYNTAX      Xdsl2Unit
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The termination unit xtuc{1} or xtur{2}."
   ::= { xdsl2LineInventoryEntry 1 }
xdsl2LInvG994VendorId  OBJECT-TYPE
   SYNTAX      OCTET STRING  (SIZE(8))
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The ATU G.994.1 Vendor ID as inserted in the G.994.1 CL/CLR
       message.  It consists of 8 binary octets, including a country
       code followed by a (regionally allocated) provider code, as
       defined in Recommendation T.35."
   REFERENCE    "ITU-T G.997.1, paragraph #7.4.1-7.4.2"
   ::= { xdsl2LineInventoryEntry 2 }
xdsl2LInvSystemVendorId  OBJECT-TYPE
   SYNTAX      OCTET STRING  (SIZE(8))
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The ATU System Vendor ID (identifies the xTU system
       integrator) as inserted in the Overhead Messages (both xTUs for
       G.992.3, G.992.4, G.992.5 and G.993.2) or in the Embedded
       Operations Channel (xTU-R in G.992.1 and G.992.2).
       It consists of 8 binary octets, with same format as used for
       Xdsl2InvG994VendorId."
   REFERENCE    "ITU-T G.997.1, paragraph #7.4.3-7.4.4"
   ::= { xdsl2LineInventoryEntry 3 }
xdsl2LInvVersionNumber  OBJECT-TYPE
   SYNTAX      OCTET STRING  (SIZE(0..16))
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The xTU version number (vendor-specific information) as
       inserted in the Overhead Messages (both xTUs for G.992.3,
       G.992.4, G.992.5 and G.993.2) or in the Embedded Operations
       Channel (xTU-R in G.992.1 and G.992.2).  It consists of up to 16
       binary octets."
   REFERENCE    "ITU-T G.997.1, paragraph #7.4.5-7.4.6"
   ::= { xdsl2LineInventoryEntry 4 }
xdsl2LInvSerialNumber  OBJECT-TYPE
   SYNTAX      OCTET STRING  (SIZE(0..32))
Morgenstern, et al.      Expires January 8, 2009              [Page 109]
Internet-Draft               VDSL2-LINE MIB                    July 2008
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The xTU serial number (vendor-specific information) as
       inserted in the Overhead Messages (both xTUs for G.992.3,
       G.992.4, G.992.5 and G.993.2) or in the Embedded Operations
       Channel (xTU-R in G.992.1 and G.992.2).  It is vendor specific
       information consisting of up to 32 ASCII characters."
   REFERENCE    "ITU-T G.997.1, paragraph #7.4.7-7.4.8"
   ::= { xdsl2LineInventoryEntry 5 }
xdsl2LInvSelfTestResult  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The xTU self-test result, coded as a 32-bit value.  The
       most significant octet of the result is '0' if the
       self-test passed, and '1' if the self-test failed.  The
       interpretation of the other octets is vendor discretionary."
   REFERENCE    "ITU-T G.997.1, paragraph #7.4.9-7.4.10"
   DEFVAL       { 0 }
   ::= { xdsl2LineInventoryEntry 6 }
xdsl2LInvTransmissionCapabilities  OBJECT-TYPE
   SYNTAX      Xdsl2TransmissionModeType
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The xTU transmission system capability list of the different
       coding types.  It is coded in a bit-map representation with 1 or
       more bits set.  A bit set to '1' means that the xTU
       supports the respective coding.  The value may be derived from
       the handshaking procedures defined in G.994.1.  A set of xDSL
       line transmission modes, with one bit per mode."
   REFERENCE    "ITU-T G.997.1, paragraph #7.4.11-7.4.12"
   ::= { xdsl2LineInventoryEntry 7 }
------------------------------------------------
--        xdsl2LineConfTemplateTable          --
------------------------------------------------
xdsl2LineConfTemplateTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2LineConfTemplateEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineConfTemplateTable contains VDSL2/ADSL/
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       ADSL2 and ADSL2+ line configuration templates.
       Note that this table is also used to configure the number of
       bearer channels.
       When the number of bearer channels is increased, the SNMP agent
       SHOULD create rows in all tables indexed by a channel index. When
       the number of bearer channels is decreased, the SNMP agent SHOULD
       delete rows in all tables indexed by a channel index.
       For example, if the value of xdsl2LConfTempChan4ConfProfile is
       set to a non null value then rows SHOULD be created in
       xdsl2ChannelStatusTable, xdsl2PMChCurrTable, and all other tables
       indexed by a channel index.
       For example, if the value of xdsl2LConfTempChan2ConfProfile is
       set to a null value then rows SHOULD be deleted in
       xdsl2ChannelStatusTable, xdsl2PMChCurrTable, and all other
       tables indexed by a channel index.
       Entries in this table MUST be maintained in a persistent
       manner."
   ::= { xdsl2ProfileLine 1 }
xdsl2LineConfTemplateEntry  OBJECT-TYPE
   SYNTAX      Xdsl2LineConfTemplateEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineConfTemplateTable contains VDSL2/ADSL/
       ADSL2 and ADSL2+ line configuration templates.
       A default template with an index of 'DEFVAL' will always exist
       and its parameters will be set to vendor-specific values, unless
       otherwise specified in this document."
   INDEX  { xdsl2LConfTempTemplateName }
   ::= { xdsl2LineConfTemplateTable 1 }
Xdsl2LineConfTemplateEntry  ::=
   SEQUENCE {
      xdsl2LConfTempTemplateName      SnmpAdminString,
      xdsl2LConfTempLineProfile       SnmpAdminString,
      xdsl2LConfTempChan1ConfProfile  SnmpAdminString,
      xdsl2LConfTempChan1RaRatioDs    Unsigned32,
      xdsl2LConfTempChan1RaRatioUs    Unsigned32,
      xdsl2LConfTempChan2ConfProfile  SnmpAdminString,
      xdsl2LConfTempChan2RaRatioDs    Unsigned32,
      xdsl2LConfTempChan2RaRatioUs    Unsigned32,
      xdsl2LConfTempChan3ConfProfile  SnmpAdminString,
      xdsl2LConfTempChan3RaRatioDs    Unsigned32,
      xdsl2LConfTempChan3RaRatioUs    Unsigned32,
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      xdsl2LConfTempChan4ConfProfile  SnmpAdminString,
      xdsl2LConfTempChan4RaRatioDs    Unsigned32,
      xdsl2LConfTempChan4RaRatioUs    Unsigned32,
      xdsl2LConfTempRowStatus         RowStatus
   }
xdsl2LConfTempTemplateName  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "This object identifies a row in this table."
   REFERENCE    "DSL Forum TR-129, paragraph #5.4"
   ::= { xdsl2LineConfTemplateEntry 1 }
xdsl2LConfTempLineProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the
       VDSL2/ADSL/ADSL2 and ADSL2+ line configuration Profile Table,
       (xdsl2LineConfProfTable) that applies for this DSL line."
   REFERENCE    "DSL Forum TR-129, paragraph #5.4"
   DEFVAL       { "DEFVAL" }
   ::= { xdsl2LineConfTemplateEntry 2 }
xdsl2LConfTempChan1ConfProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the VDSL2/
       ADSL/ADSL2 and ADSL2+ channel configuration Profile Table,
       (xdsl2ChConfProfileTable) that applies to DSL bearer channel #1.
       The channel profile name specified here MUST match the name of an
       existing row in the xdsl2ChConfProfileTable table."
   DEFVAL       { "DEFVAL" }
   ::= { xdsl2LineConfTemplateEntry 3 }
xdsl2LConfTempChan1RaRatioDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..100)
   UNITS       "percent"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Rate Adaptation Ratio.  The ratio (in %) that should be
       taken into account for the bearer channel #1 when performing rate
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       adaptation on Downstream.  The ratio refers to the available data
       rate in excess of the Minimum Data Rate, summed over all bearer
       channels.
       Also, the 100 - xdsl2LConfTempChan1RaRatioDs is the ratio of
       excess data rate to be assigned to all other bearer channels on
       Downstream direction.  The sum of rate adaptation ratios over all
       bearers on the same direction shall be equal to 100%.
       "
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.4
                (Rate adaptation ratio)"
   DEFVAL       { 100 }
   ::= { xdsl2LineConfTemplateEntry 4 }
xdsl2LConfTempChan1RaRatioUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..100)
   UNITS       "percent"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Rate Adaptation Ratio.  The ratio (in %) that should be
       taken into account for the bearer channel #1 when performing
       rate adaptation on Upstream.  The ratio refers to the available
       data rate in excess of the Minimum Data Rate, summed over all
       bearer channels.
       Also, the 100 - xdsl2LConfTempChan1RaRatioUs is the ratio of
       excess data rate to be assigned to all other bearer channels on
       Upstream direction.  The sum of rate adaptation ratios over all
       bearers on the same direction shall be equal to 100 %."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.4
                (Rate adaptation ratio)"
   DEFVAL       { 100 }
   ::= { xdsl2LineConfTemplateEntry 5 }
xdsl2LConfTempChan2ConfProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the VDSL2/
       ADSL/ADSL2 and ADSL2+ channel configuration Profile Table,
       (xdsl2ChConfProfileTable) that applies to DSL bearer channel #2.
       If the channel is unused, then the object is set to a zero-length
       string.
       This object may be set to a zero-length string only if
       xdsl2LConfTempChan3ConfProfile contains a zero-length
       string."
   DEFVAL       { "" }
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   ::= { xdsl2LineConfTemplateEntry 6 }
xdsl2LConfTempChan2RaRatioDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..100)
   UNITS       "percent"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Rate Adaptation Ratio.  The ratio (in %) that should be
       taken into account for the bearer channel #2 when performing
       rate adaptation on Downstream.  The ratio refers to the available
       data rate in excess of the Minimum Data Rate, summed over all
       bearer channels.
       Also, the 100 - xdsl2LConfTempChan2RaRatioDs is the ratio of
       excess data rate to be assigned to all other bearer channels on
       Downstream direction.  The sum of rate adaptation ratios over all
       bearers on the same direction shall be equal to
       100%."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.4
                (Rate adaptation ratio)"
   DEFVAL       { 0 }
   ::= { xdsl2LineConfTemplateEntry 7 }
xdsl2LConfTempChan2RaRatioUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..100)
   UNITS       "percent"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Rate Adaptation Ratio.  The ratio (in %) that should be
       taken into account for the bearer channel #2 when performing
       rate adaptation on Upstream.  The ratio refers to the available
       data rate in excess of the Minimum Data Rate, summed over all
       bearer channels.
       Also, the 100 - xdsl2LConfTempChan2RaRatioUs is the ratio of
       excess data rate to be assigned to all other bearer channels on
       Upstream direction.  The sum of rate adaptation ratios over all
       bearers on the same direction shall be equal to 100 %."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.4
                (Rate adaptation ratio)"
   DEFVAL       { 0 }
   ::= { xdsl2LineConfTemplateEntry 8 }
xdsl2LConfTempChan3ConfProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
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      "The value of this object identifies the row in the VDSL2/
       ADSL/ADSL2 and ADSL2+ channel configuration Profile Table,
       (xdsl2ChConfProfileTable) that applies to DSL bearer channel #3.
       If the channel is unused, then the object is set to a zero-length
       string.
       This object may be set to a zero-length string only if
       xdsl2LConfTempChan4ConfProfile contains a zero-length string.
       This object may be set to a non-zero-length string only if
       xdsl2LConfTempChan2ConfProfile contains a non-zero-length
       string."
   DEFVAL       { "" }
   ::= { xdsl2LineConfTemplateEntry 9 }
xdsl2LConfTempChan3RaRatioDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..100)
   UNITS       "percent"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Rate Adaptation Ratio.  The ratio (in %) that should be
       taken into account for the bearer channel #3 when performing
       rate adaptation on Downstream.  The ratio refers to the available
       data rate in excess of the Minimum Data Rate, summed over all
       bearer channels.
       Also, the 100 - xdsl2LConfTempChan3RaRatioDs is the ratio of
       excess data rate to be assigned to all other bearer channels on
       Downstream direction.  The sum of rate adaptation ratios over all
       bearers on the same direction shall be equal to 100%.
       "
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.4
                (Rate adaptation ratio)"
   DEFVAL       { 0 }
   ::= { xdsl2LineConfTemplateEntry 10 }
xdsl2LConfTempChan3RaRatioUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..100)
   UNITS       "percent"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Rate Adaptation Ratio.  The ratio (in %) that should be
       taken into account for the bearer channel #3 when performing
       rate adaptation on Upstream.  The ratio refers to the available
       data rate in excess of the Minimum Data Rate, summed over all
       bearer channels.
       Also, the 100 - xdsl2LConfTempChan3RaRatioUs is the ratio of
       excess data rate to be assigned to all other bearer channels on
       Upstream direction.  The sum of rate adaptation ratios over all
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       bearers on the same direction shall be equal to 100%."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.4
                (Rate adaptation ratio)"
   DEFVAL       { 0 }
   ::= { xdsl2LineConfTemplateEntry 11 }
xdsl2LConfTempChan4ConfProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the VDSL2/
       ADSL/ADSL2 and ADSL2+ channel configuration Profile Table,
       (xdsl2ChConfProfileTable) that applies to DSL bearer channel #4.
       If the channel is unused, then the object is set to a zero-length
       string.
       This object may be set to a non-zero-length string only if
       xdsl2LConfTempChan3ConfProfile contains a non-zero-length
       string."
   DEFVAL       { "" }
   ::= { xdsl2LineConfTemplateEntry 12 }
xdsl2LConfTempChan4RaRatioDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..100)
   UNITS       "percent"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Rate Adaptation Ratio.  The ratio (in %) that should be
       taken into account for the bearer channel #4 when performing rate
       adaptation on Downstream.  The ratio refers to the available data
       rate in excess of the Minimum Data Rate, summed over all bearer
       channels.
       Also, the 100 - xdsl2LConfTempChan4RaRatioDs is the ratio of
       excess data rate to be assigned to all other bearer channels.
       The sum of rate adaptation ratios over all bearers on the same
       direction shall sum to 100%."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.4
                (Rate adaptation ratio)"
   DEFVAL       { 0 }
   ::= { xdsl2LineConfTemplateEntry 13 }
xdsl2LConfTempChan4RaRatioUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..100)
   UNITS       "percent"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
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      "Rate Adaptation Ratio.  The ratio (in %) that should be
       taken into account for the bearer channel #4 when performing rate
       adaptation on Upstream.  The ratio refers to the available data
       rate in excess of the Minimum Data Rate, summed over all bearer
       channels.
       Also, the 100 - xdsl2LConfTempChan4RaRatioUs is the ratio of
       excess data rate to be assigned to all other bearer channels.
       The sum of rate adaptation ratios over all bearers on the same
       direction shall sum to 100%."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.4
                (Rate adaptation ratio)"
   DEFVAL       { 0 }
   ::= { xdsl2LineConfTemplateEntry 14 }
xdsl2LConfTempRowStatus  OBJECT-TYPE
   SYNTAX      RowStatus
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This object is used to create a new row or to modify or
       delete an existing row in this table.
       A template is activated by setting this object to 'active'.
       When 'active' is set, the system will validate the template.
       Before a template can be deleted or taken out of service (by
       setting this object to 'destroy' or 'notInService'), it MUST be
       first unreferenced from all associated lines."
   ::= { xdsl2LineConfTemplateEntry 15 }
------------------------------------------
--        xdsl2LineConfProfTable        --
------------------------------------------
xdsl2LineConfProfTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2LineConfProfEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineConfProfTable contains VDSL2/ADSL/
       ADSL2 and ADSL2+ line configuration profiles.
       Entries in this table MUST be maintained in a persistent
       manner."
   ::= { xdsl2ProfileLine 2 }
xdsl2LineConfProfEntry  OBJECT-TYPE
   SYNTAX      Xdsl2LineConfProfEntry
   MAX-ACCESS  not-accessible
   STATUS      current
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   DESCRIPTION
      "The table xdsl2LineConfProfTable contains VDSL2/ADSL/
       ADSL2 and ADSL2+ line configuration profiles.
       A default profile with an index of 'DEFVAL' will always exist and
       its parameters will be set to vendor-specific values, unless
       otherwise specified in this document."
   INDEX  { xdsl2LConfProfProfileName }
   ::= { xdsl2LineConfProfTable 1 }
Xdsl2LineConfProfEntry  ::=
   SEQUENCE {
      xdsl2LConfProfProfileName          SnmpAdminString,
      xdsl2LConfProfScMaskDs             Xdsl2ScMaskDs,
      xdsl2LConfProfScMaskUs             Xdsl2ScMaskUs,
      xdsl2LConfProfVdsl2CarMask         Xdsl2CarMask,
      xdsl2LConfProfRfiBands             Xdsl2RfiBands,
      xdsl2LConfProfRaModeDs             Xdsl2RaMode,
      xdsl2LConfProfRaModeUs             Xdsl2RaMode,
      xdsl2LConfProfRaUsNrmDs            Unsigned32,
      xdsl2LConfProfRaUsNrmUs            Unsigned32,
      xdsl2LConfProfRaUsTimeDs           Unsigned32,
      xdsl2LConfProfRaUsTimeUs           Unsigned32,
      xdsl2LConfProfRaDsNrmDs            Unsigned32,
      xdsl2LConfProfRaDsNrmUs            Unsigned32,
      xdsl2LConfProfRaDsTimeDs           Unsigned32,
      xdsl2LConfProfRaDsTimeUs           Unsigned32,
      xdsl2LConfProfTargetSnrmDs         Unsigned32,
      xdsl2LConfProfTargetSnrmUs         Unsigned32,
      xdsl2LConfProfMaxSnrmDs            Unsigned32,
      xdsl2LConfProfMaxSnrmUs            Unsigned32,
      xdsl2LConfProfMinSnrmDs            Unsigned32,
      xdsl2LConfProfMinSnrmUs            Unsigned32,
      xdsl2LConfProfMsgMinUs             Unsigned32,
      xdsl2LConfProfMsgMinDs             Unsigned32,
      xdsl2LConfProfCeFlag               Xdsl2LineCeFlag,
      xdsl2LConfProfSnrModeDs            Xdsl2LineSnrMode,
      xdsl2LConfProfSnrModeUs            Xdsl2LineSnrMode,
      xdsl2LConfProfTxRefVnDs            Xdsl2LineTxRefVnDs,
      xdsl2LConfProfTxRefVnUs            Xdsl2LineTxRefVnUs,
      xdsl2LConfProfXtuTransSysEna       Xdsl2TransmissionModeType,
      xdsl2LConfProfPmMode               Xdsl2LinePmMode,
      xdsl2LConfProfL0Time               Unsigned32,
      xdsl2LConfProfL2Time               Unsigned32,
      xdsl2LConfProfL2Atpr               Unsigned32,
      xdsl2LConfProfL2Atprt              Unsigned32,
      xdsl2LConfProfProfiles             Xdsl2LineProfiles,
      xdsl2LConfProfDpboEPsd             Xdsl2PsdMaskDs,
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      xdsl2LConfProfDpboEsEL             Unsigned32,
      xdsl2LConfProfDpboEsCableModelA    Unsigned32,
      xdsl2LConfProfDpboEsCableModelB    Unsigned32,
      xdsl2LConfProfDpboEsCableModelC    Unsigned32,
      xdsl2LConfProfDpboMus              Unsigned32,
      xdsl2LConfProfDpboFMin             Unsigned32,
      xdsl2LConfProfDpboFMax             Unsigned32,
      xdsl2LConfProfUpboKL               Unsigned32,
      xdsl2LConfProfUpboKLF              Xdsl2UpboKLF,
      xdsl2LConfProfUs0Mask              Xdsl2LineUs0Mask,
      xdsl2LConfProfForceInp             Xdsl2LineForceInp,
      xdsl2LConfProfRowStatus            RowStatus
   }
xdsl2LConfProfProfileName  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "This object identifies a row in this table."
     ::= { xdsl2LineConfProfEntry 1 }
xdsl2LConfProfScMaskDs  OBJECT-TYPE
   SYNTAX      Xdsl2ScMaskDs
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Subcarriers mask.  A bitmap of 4096 bits that allows masking
       up to 4096 downstream subcarriers, depending on NSCds.  If bit i
       (0 <= i < NSCds) is set to '1', the respective
       downstream subcarrier i is masked, and if set to '0',
       the respective subcarrier is unmasked.  Note that there should
       always be unmasked subcarriers (i.e., the object cannot be all
       1's).  Also note that if NSCds < 4096, all bits i (NSCds
       < i <= 4096) should be set to '1'."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.6 (CARMASKds)
   "
   ::= { xdsl2LineConfProfEntry 2 }
xdsl2LConfProfScMaskUs  OBJECT-TYPE
   SYNTAX      Xdsl2ScMaskUs
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Subcarriers mask.  A bitmap of 4096 bits that allows masking
       up to 4096 downstream subcarriers, depending on NSCds.  If bit i
       (0 <= i < NSCus) is set to '1', the respective
       upstream subcarrier i is masked, and if set to '0', the
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       respective subcarrier is unmasked.  Note that there should always
       be unmasked subcarriers (i.e., the object cannot be all
       1's).  Also note that if NSCus < 4096, all bits i (NSCus
       < i <= 4096) should be set to '1'."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.7 (CARMASKus)
   "
   ::= { xdsl2LineConfProfEntry 3 }
xdsl2LConfProfVdsl2CarMask  OBJECT-TYPE
   SYNTAX      Xdsl2CarMask
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "VDSL2 specific subcarriers mask.  This configuration
       parameter defines the restrictions, additional to the band plan,
       to determine the set of subcarriers allowed for transmission in
       both upstream and downstream directions.
       The parameter shall describe the not masked subcarriers as one or
       more frequency bands. Each band is represented by start and stop
       subcarrier indices with a subcarrier spacing of 4.3125kHz. The
       valid range of subcarrier indices runs from 0 to at least the
       index of the highest allowed subcarrier in both transmission
       directions among all profiles enabled by the parameter
       xdsl2LConfProfProfiles.
       Up to 32 bands may be specified. Other subcarriers shall be
       masked."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.8 (VDSL2-
   CARMASK)
   "
   ::= { xdsl2LineConfProfEntry 4 }
xdsl2LConfProfRfiBands  OBJECT-TYPE
   SYNTAX      Xdsl2RfiBands
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "For ITU-T Rec. G.992.5, this configuration parameter defines
       the subset of downstream PSD mask breakpoints, as specified in
       xdsl2LConfProfPsdMaskDs (PSDMASKds), that shall be used to notch
       an RFI band. This subset consists of pairs of consecutive
       subcarrier indices belonging to breakpoints: [ti; ti + 1],
       corresponding to the low level of the notch.
       The specific interpolation around these points is defined in the
       relevant Recommendations (e.g., ITU-T Rec. G.992.5).
       The CO-MIB shall define the RFI notches using breakpoints in
       xdsl2LConfProfPsdMaskDs (PSDMASKds) as specified in the relevant
       Recommendations (e.g., ITU-T Rec. G.992.5).
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       For ITU-T Rec. G.993.2, this configuration parameter defines the
       bands where the PSD shall be reduced as specified in
       #7.2.1.2/G.993.2. Each band shall be represented by a start and
       stop subcarrier indices with a subcarrier spacing of 4.3125 kHz.
       Up to 16 bands may be specified. This parameter defines the RFI
       bands for both upstream and downstream directions."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.10 (RFIBANDS)
   "
   ::= { xdsl2LineConfProfEntry 5 }
xdsl2LConfProfRaModeDs  OBJECT-TYPE
   SYNTAX      Xdsl2RaMode
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The mode of operation of a rate-adaptive xTU-C in the
       transmit direction.  The parameter can take three values:
          manual(1),
          raInit(2),
          dynamicRa(3)."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.4.1 (RA-MODEds)
   "
   DEFVAL      { manual }
   ::= { xdsl2LineConfProfEntry 6 }
xdsl2LConfProfRaModeUs  OBJECT-TYPE
   SYNTAX      Xdsl2RaMode
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The mode of operation of a rate-adaptive xTU-R in the
       transmit direction.  The parameter can take three values:
          manual(1),
          raInit(2),
          dynamicRa(3)."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.4.2 (RA-MODEus)
   "
   DEFVAL      { manual }
   ::= { xdsl2LineConfProfEntry 7 }
xdsl2LConfProfRaUsNrmDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..310)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The Downstream Up-Shift Noise Margin value, to be used when
       xdsl2LConfProfRaModeDs is set to dynamicRa.  If the downstream
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       noise margin is above this value, and stays above it,
       for more than
       the time specified by the xdsl2LConfProfRaUsTimeDs, the xTU-R
       shall attempt to increase the downstream net data rate.  The
       Downstream Up-Shift Noise Margin ranges from 0 to 310 units of
       0.1 dB (Physical values are 0 to 31 dB)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.4.3 (RA-USNRMds)
   "
   DEFVAL       { 10 }
   ::= { xdsl2LineConfProfEntry 8 }
xdsl2LConfProfRaUsNrmUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..310)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The Upstream Up-Shift Noise Margin value, to be used when
       xdsl2LConfProfRaModeUs is set to dynamicRa.  If the upstream
       noise margin is above this value, and stays above it,
       for more than
       the time specified by the xdsl2LConfProfRaUsTimeUs, the xTU-C
       shall attempt to increase the upstream net data rate.
       The Upstream Up-Shift Noise Margin ranges from 0 to 310 units of
       0.1 dB (Physical values are 0 to 31 dB)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.4.4 (RA-USNRMus)
   "
   DEFVAL       { 10 }
   ::= { xdsl2LineConfProfEntry 9 }
xdsl2LConfProfRaUsTimeDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..16383)
   UNITS       "seconds"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The Downstream Up-Shift Time Interval, to be used when
       xdsl2LConfProfRaModeDs is set to dynamicRa.  The interval of time
       that the downstream noise margin should stay above the Downstream
       Up-Shift Noise Margin before the xTU-R shall attempt to increase
       the downstream net data rate.  The time interval ranges from 0 to
       16383 seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.4.5 (RA-UTIMEds)
   "
   DEFVAL       { 3600 }
   ::= { xdsl2LineConfProfEntry 10 }
xdsl2LConfProfRaUsTimeUs  OBJECT-TYPE
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   SYNTAX      Unsigned32(0..16383)
   UNITS       "seconds"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The Upstream Up-Shift Time Interval, to be used when
       xdsl2LConfProfRaModeUs is set to dynamicRa.  The interval of time
       the upstream noise margin should stay above the Upstream Up-Shift
       Noise Margin before the xTU-C shall attempt to increase the
       upstream net data rate.  The time interval ranges from 0 to 16383
       seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.4.6 (RA-UTIMEus)
   "
   DEFVAL       { 3600 }
   ::= { xdsl2LineConfProfEntry 11 }
xdsl2LConfProfRaDsNrmDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..310)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The Downstream Down-Shift Noise Margin value, to be used
       when xdsl2LConfProfRaModeDs is set to dynamicRa.  If the
       downstream noise margin is below this value,
       and stays below that value,
       for more than the time specified by the xdsl2LConfProfRaDsTimeDs,
       the xTU-R shall attempt to decrease the downstream net data rate.
       The Downstream Down-Shift Noise Margin ranges from 0 to 310 units
       of 0.1 dB (Physical values are 0 to 31 dB)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.4.7 (RA-DSNRMds)
   "
   DEFVAL       { 10 }
   ::= { xdsl2LineConfProfEntry 12 }
xdsl2LConfProfRaDsNrmUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..310)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The Upstream Downshift Noise Margin value, to be used when
       xdsl2LConfProfRaModeUs is set to dynamicRa.  If the upstream
       noise margin is below this value,
       and stays below that value, for more
       than the time specified by the xdsl2LConfProfRaDsTimeUs, the
       xTU-C shall attempt to decrease the upstream net data rate.
       The Upstream Down-Shift Noise Margin ranges from 0 to 310 units
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       of 0.1 dB (Physical values are 0 to 31 dB)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.4.8 (RA-DSNRMus)
   "
   DEFVAL       { 10 }
   ::= { xdsl2LineConfProfEntry 13 }
xdsl2LConfProfRaDsTimeDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..16383)
   UNITS       "seconds"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The Downstream Downshift Time Interval, to be used when
       xdsl2LConfProfRaModeDs is set to dynamicRa.  The interval of
       time the downstream noise margin should stay below the Downstream
       Down-Shift Noise Margin before the xTU-R shall attempt to
       decrease the downstream net data rate.  The time interval ranges
       from 0 to 16383 seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.4.9 (RA-DTIMEds)
   "
   DEFVAL       { 3600 }
   ::= { xdsl2LineConfProfEntry 14 }
xdsl2LConfProfRaDsTimeUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..16383)
   UNITS       "seconds"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The Upstream Down-Shift Time Interval, to be used when
       xdsl2LConfProfRaModeUs is set to dynamicRa.  The interval of time
       the upstream noise margin should stay below the Upstream Down-
       Shift Noise Margin before the xTU-C shall attempt to decrease the
       upstream net data rate.  The time interval ranges from 0 to 16383
       seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.4.10 (RA-DTIMEus)
   "
   DEFVAL       { 3600 }
   ::= { xdsl2LineConfProfEntry 15 }
xdsl2LConfProfTargetSnrmDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..310)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The minimum Noise Margin the xTU-R receiver shall achieve,
       relative to the BER requirement for each of the downstream bearer
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       channels, to successfully complete initialization.
       The target noise margin ranges from 0 to 310 units of 0.1 dB
       (Physical values are 0 to 31 dB)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.3.1 (TARSNRMds)
   "
   DEFVAL       { 60 }
   ::= { xdsl2LineConfProfEntry 16 }
xdsl2LConfProfTargetSnrmUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..310)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The minimum Noise Margin the xTU-C receiver shall achieve,
       relative to the BER requirement for each of the upstream bearer
       channels, to successfully complete initialization.
       The target noise margin ranges from 0 to 310 units of 0.1 dB
       (Physical values are 0 to 31 dB)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.3.2 (TARSNRMus)
   "
   DEFVAL       { 60 }
   ::= { xdsl2LineConfProfEntry 17 }
xdsl2LConfProfMaxSnrmDs  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..310 | 2147483647)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The maximum Noise Margin the xTU-R receiver shall try to
       sustain.  If the Noise Margin is above this level, the xTU-R
       shall request that the xTU-C reduce the xTU-C transmit power to
       get a noise margin below this limit (if this functionality is
       supported).  The maximum noise margin ranges from 0 to 310 units
       of 0.1 dB (Physical values are 0 to 31 dB).  A value of
       0x7FFFFFFF (2147483647) means that there is no maximum."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.3.3 (MAXSNRMds)
   "
   DEFVAL       { 310 }
   ::= { xdsl2LineConfProfEntry 18 }
xdsl2LConfProfMaxSnrmUs  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..310 | 2147483647)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
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      "The maximum Noise Margin the xTU-C receiver shall try to
       sustain.  If the Noise Margin is above this level, the xTU-C
       shall request that the xTU-R reduce the xTU-R transmit power to
       get a noise margin below this limit (if this functionality is
       supported).  The maximum noise margin ranges from 0 to 310 units
       of 0.1 dB (Physical values are 0 to 31 dB).  A value of
       0x7FFFFFFF (2147483647) means that there is no maximum."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.3.4 (MAXSNRMus)
   "
   DEFVAL       { 310 }
   ::= { xdsl2LineConfProfEntry 19 }
xdsl2LConfProfMinSnrmDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..310)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The minimum Noise Margin the xTU-R receiver shall tolerate.
       If the noise margin falls below this level, the xTU-R shall
       request that the xTU-C increase the xTU-C transmit power.
       If an increase to xTU-C transmit power is not possible, a loss-
       of-margin (LOM) defect occurs, the xTU-R shall fail and attempt
       to reinitialize and the NMS shall be notified.  The minimum noise
       margin ranges from 0 to 310 units of 0.1 dB (Physical values are
       0 to 31 dB).  A value of 0 means that there is no minimum."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.3.5 (MINSNRMds)
   "
   DEFVAL       { 10 }
   ::= { xdsl2LineConfProfEntry 20 }
xdsl2LConfProfMinSnrmUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..310)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The minimum Noise Margin the xTU-C receiver shall tolerate.
       If the noise margin falls below this level, the xTU-C shall
       request that the xTU-R increase the xTU-R transmit power.
       If an increase of xTU-R transmit power is not possible, a loss-
       of-margin (LOM) defect occurs, the xTU-C shall fail and attempt
       to re-initialize and the NMS shall be notified.  The minimum
       noise margin ranges from 0 to 310 units of 0.1 dB (Physical
       values are 0 to 31 dB).  A value of 0 means that there is no
       minimum."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.3.6 (MINSNRMus)
   "
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   DEFVAL       { 10 }
   ::= { xdsl2LineConfProfEntry 21 }
xdsl2LConfProfMsgMinUs  OBJECT-TYPE
   SYNTAX      Unsigned32(4000..248000)
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Minimum Overhead Rate Upstream.  Defines the minimum rate of
       the message-based overhead that shall be maintained by the xTU in
       upstream direction.  Expressed in bits per second and ranges from
       4000 to 248000 bps."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.5.1 (MSGMINus)
   "
   DEFVAL       { 4000 }
  ::= { xdsl2LineConfProfEntry 22 }
xdsl2LConfProfMsgMinDs  OBJECT-TYPE
   SYNTAX      Unsigned32(4000..248000)
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Minimum Overhead Rate Downstream.  Defines the minimum rate
       of the message-based overhead that shall be maintained by the xTU
       in downstream direction.  Expressed in bits per second and ranges
       from 4000 to 248000 bps."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.5.2 (MSGMINds)
   "
   DEFVAL       { 4000 }
   ::= { xdsl2LineConfProfEntry 23 }
xdsl2LConfProfCeFlag  OBJECT-TYPE
   SYNTAX      Xdsl2LineCeFlag
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This parameter is a bit that enables the use of the optional
       cyclic extension values. If the bit is set to 1, the optional
       cyclic extension values may be used. Otherwise, the cyclic
       extension shall be forced to the mandatory length (5N/32)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.6.1 (CEFLAG)"
   DEFVAL       { { } }
   ::= { xdsl2LineConfProfEntry 24 }
xdsl2LConfProfSnrModeDs  OBJECT-TYPE
   SYNTAX      Xdsl2LineSnrMode
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   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This parameter enables the transmitter referred virtual
       noise in the downstream direction. If set to 1, the virtual noise
       is disabled. If set to 2, the virtual noise is enabled."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.7.1 (SNRMODEds)
   "
   DEFVAL       { virtualNoiseDisabled }
   ::= { xdsl2LineConfProfEntry 25 }
xdsl2LConfProfSnrModeUs  OBJECT-TYPE
   SYNTAX      Xdsl2LineSnrMode
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This parameter enables the transmitter referred virtual
       noise in the upstream direction. If set to 1, the virtual noise
       is disabled. If set to 2, the virtual noise is enabled."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.7.2 (SNRMODEus)
   "
   DEFVAL       { virtualNoiseDisabled }
   ::= { xdsl2LineConfProfEntry 26 }
xdsl2LConfProfTxRefVnDs  OBJECT-TYPE
   SYNTAX      Xdsl2LineTxRefVnDs
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the downstream
       transmitter referred virtual noise .
       The TXREFVNds shall be specified through a set of breakpoints.
       Each breakpoint shall consist of a subcarrier index t, with a
       subcarrier spacing of 4.3125 kHz, and a noise PSD level
       (expressed in dBm/Hz) at that subcarrier. The set of breakpoints
       can then be represented as:
       [(t1,PSD1), (t2, PSD2), ... , (tN, PSDN)].
       The subcarrier index shall be coded as an unsigned integer. The
       noise level ranges from -40 dBm/Hz to -140 dBm/Hz in steps of 0.5
       dBm/Hz.
       A special value indicates a noise level of 0 W/Hz.
       The maximum number of breakpoints is 32."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.7.3 (TXREFVNds)
   "
   ::= { xdsl2LineConfProfEntry 27 }
xdsl2LConfProfTxRefVnUs  OBJECT-TYPE
   SYNTAX      Xdsl2LineTxRefVnUs
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   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the upstream
       transmitter referred virtual noise.
       The TXREFVNus shall be specified through a set of breakpoints.
       Each breakpoint shall consist of a subcarrier index t, with a
       subcarrier spacing of 4.3125 kHz, and a noise PSD level
       (expressed in dBm/Hz) at that subcarrier. The set of breakpoints
       can then be represented as:
       [(t1, PSD1), (t2, PSD2), ... , (tN, PSDN)].
       The subcarrier index shall be coded as an unsigned integer. The
       noise level ranges from -40 dBm/Hz to -140 dBm/Hz in steps of 0.5
       dBm/Hz.
       A special value indicates a noise level of 0 W/Hz.
       The maximum number of breakpoints is 16."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.7.4 (TXREFVNus)
   "
   ::= { xdsl2LineConfProfEntry 28 }
xdsl2LConfProfXtuTransSysEna  OBJECT-TYPE
   SYNTAX      Xdsl2TransmissionModeType
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "xTU Transmission System Enabling (XTSE).  A list of the
       different coding types enabled in this profile.  It is coded in a
       bit-map representation with 1 or more bits set.  A bit set to
       '1' means that the xTUs may apply the respective
       coding for the DSL line.  A bit set to '0' means that
       the xTUs cannot apply the respective coding for the ADSL line.
       All 'reserved' bits should be set to
       '0'."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.1 (XTSE)"
   ::= { xdsl2LineConfProfEntry 29 }
xdsl2LConfProfPmMode  OBJECT-TYPE
   SYNTAX      Xdsl2LinePmMode
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Power management state Enabling (PMMode).  Defines the power
       states the xTU-C or xTU-R may autonomously transition to on
       this line.
       The various bit positions are: allowTransitionsToIdle (0) and
       allowTransitionsToLowPower (1).  A bit with a '1' value
       means that the xTU is allowed to transit into the respective
       state and a '0' value means that the xTU is not allowed
Morgenstern, et al.      Expires January 8, 2009              [Page 129]
Internet-Draft               VDSL2-LINE MIB                    July 2008
       to transit into the respective state."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.4 (PMMode)"
   DEFVAL  { { allowTransitionsToIdle, allowTransitionsToLowPower } }
   ::= { xdsl2LineConfProfEntry 30 }
xdsl2LConfProfL0Time  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..255)
   UNITS       "seconds"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The minimum time (in seconds) between an Exit from the L2
       state and the next Entry into the L2 state.
       It ranges from 0 to 255 seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.5 (L0-TIME)
   "
   DEFVAL       { 255 }
   ::= { xdsl2LineConfProfEntry 31 }
xdsl2LConfProfL2Time  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..255)
   UNITS       "seconds"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The minimum time (in seconds) between an Entry into the
       L2 state and the first Power Trim in the L2 state and between two
       consecutive Power Trims in the L2 State.
       It ranges from 0 to 255 seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.6 (L2-TIME)
   "
   DEFVAL       { 255 }
   ::= { xdsl2LineConfProfEntry 32 }
xdsl2LConfProfL2Atpr  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..31)
   UNITS       "dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The maximum aggregate transmit power reduction (in dB) that
       can be performed at transition of L0 to L2 state or through a
       single Power Trim in the L2 state.
       It ranges from 0 dB to 31 dB."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.7 (L2-ATPR)
   "
   DEFVAL       { 10 }
   ::= { xdsl2LineConfProfEntry 33 }
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xdsl2LConfProfL2Atprt  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..31)
   UNITS       "dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The total maximum aggregate transmit power reduction (in dB)
       that can be performed in an L2 state. This is the sum of all
       reductions of L2 Request (i.e., at transition of L0 to L2 state)
       and Power Trims."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.9 (L2-ATPRT)
   "
   DEFVAL       { 31 }
   ::= { xdsl2LineConfProfEntry 34 }
xdsl2LConfProfProfiles  OBJECT-TYPE
   SYNTAX      Xdsl2LineProfiles
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      " The configuration parameter contains the G.993.2 profiles
       to be allowed by the near-end xTU on this line.
       It is coded in a bitmap representation (0 if not allowed, 1 if
       allowed) "
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.1.11 (PROFILES)
   "
   DEFVAL       { { profile8a,  profile8b,  profile8c,
                    profile8d,  profile12a, profile12b,
                    profile17a, profile30a } }
   ::= { xdsl2LineConfProfEntry 35 }
xdsl2LConfProfDpboEPsd  OBJECT-TYPE
   SYNTAX      Xdsl2PsdMaskDs
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the PSD mask that is
       assumed to be permitted at the exchange. This parameter shall use
       the same format as xdsl2LConfProfPsdMaskDs (PSDMASKds). The
       maximum number of breakpoints for xdsl2LConfProfDpboEPsd is
       16."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.13 (DPBOEPSD)
   "
   ::= { xdsl2LineConfProfEntry 36 }
xdsl2LConfProfDpboEsEL  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..511)
   UNITS       "0.5 dB"
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   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the assumed electrical
       length of cables (E-side cables) connecting exchange based DSL
       services to a remote flexibility point (cabinet), that hosts the
       xTU-C that is subject to spectrally shaped downstream power back-
       off (DPBO) depending on this length. The electrical length is
       defined as the loss (in dB) of an equivalent length of
       hypothetical cable at a reference frequency defined by the
       network operator or in spectrum management regulations.
       This parameter shall be coded as an unsigned integer representing
       an electrical length from 0 dB (coded as 0) to 255.5 dB (coded as
       511) in steps of 0.5 dB. All values in the range are valid. If
       this parameter is set to zero, the DPBO shall be disabled."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.13 (DPBOESEL)
   "
   DEFVAL      { 0 }
   ::= { xdsl2LineConfProfEntry 37 }
xdsl2LConfProfDpboEsCableModelA  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..640)
   UNITS       "2^-8"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The E-side Cable Model parameter A (DPBOESCMA) of the cable
       model (DPBOESCM) for cables connecting exchange based DSL
       services to a remote flexibility point (cabinet), that hosts the
       xTU-C that is subject to spectrally shaped downstream power back-
       off (DPBO) depending on this value.
       The cable model is in terms of three scalars
       xdsl2LConfProfDpboEsCableModelA (DPBOESCMA),
       xdsl2LConfProfDpboEsCableModelB(DPBOESCMB), and
       xdsl2LConfProfDpboEsCableModelC (DPBOESCMC), that are used to
       estimate the frequency dependent loss of E-side cables calculated
       from the xdsl2LConfProfDpboEsEL (DPBOESEL) parameter. Possible
       values shall be coded as unsigned integers representing a scalar
       value from -1 (coded as 0) to 1.5 (coded as 640) in steps of
       2^-8. All values in the range are valid. This parameter is used
       only for G.993.2."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.13 (DPBOESCMA)
   "
   DEFVAL      { 0 }
   ::= { xdsl2LineConfProfEntry 38 }
xdsl2LConfProfDpboEsCableModelB  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..640)
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   UNITS       "2^-8"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The E-side Cable Model parameter B (DPBOESCMB) of the cable
       model (DPBOESCM) for cables connecting exchange based DSL
       services to a remote flexibility point (cabinet), that hosts the
       xTU-C that is subject to spectrally shaped downstream power back-
       off (DPBO) depending on this value.
       The cable model is in terms of three scalars
       dsl2LConfProfDpboEsCableModelA (DPBOESCMA),
       xdsl2LConfProfDpboEsCableModelB(DPBOESCMB), and
       xdsl2LConfProfDpboEsCableModelC (DPBOESCMC), that are used to
       estimate the frequency dependent loss of E-side cables calculated
       from the xdsl2LConfProfDpboEsEL (DPBOESEL) parameter. Possible
       values shall be coded as unsigned integers representing a scalar
       value from -1 (coded as 0) to 1.5 (coded as 640) in steps of
       2^-8. All values in the range are valid. This parameter is used
       only for G.993.2."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.13 (DPBOESCMB)
   "
   DEFVAL      { 0 }
   ::= { xdsl2LineConfProfEntry 39 }
xdsl2LConfProfDpboEsCableModelC  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..640)
   UNITS       "2^-8"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The E-side Cable Model parameter C (DPBOESCMC) of the cable
       model (DPBOESCM) for cables connecting exchange based DSL
       services to a remote flexibility point (cabinet), that hosts the
       xTU-C that is subject to spectrally shaped downstream power back-
       off (DPBO) depending on this value.
       The cable model is in terms of three scalars
       xdsl2LConfProfDpboEsCableModelA (DPBOESCMA),
       xdsl2LConfProfDpboEsCableModelB(DPBOESCMB), and
       xdsl2LConfProfDpboEsCableModelC (DPBOESCMC), that are used to
       estimate the frequency dependent loss of E-side cables calculated
       from the xdsl2LConfProfDpboEsEL (DPBOESEL) parameter. Possible
       values shall be coded as unsigned integers representing a scalar
       value from -1 (coded as 0) to 1.5 (coded as 640) in steps of
       2^-8. All values in the range are valid. This parameter is used
       only for G.993.2."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.13 (DPBOESCMC)
   "
   DEFVAL      { 0 }
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   ::= { xdsl2LineConfProfEntry 40 }
xdsl2LConfProfDpboMus OBJECT-TYPE
   SYNTAX      Unsigned32 (0..255)
   UNITS       "0.5 dBm/Hz"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the assumed Minimum
       Usable receive PSD mask (in dBm/Hz) for exchange based services,
       used to modify parameter xdsl2LConfProfDpboFMax (DPBOFMAX)
       defined below [to determine the DPBO]. It shall be coded as an
       unsigned integer representing a PSD mask level from 0 dBm/Hz
       (coded as 0) to -127.5 dBm/Hz (coded as 255) in steps of 0.5
       dBm/Hz. All values in the range are valid.
       NOTE - The PSD mask level is 3.5 dB above the signal PSD level.
       This parameter is used only for G.993.2."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.13 (DPBOMUS)
   "
   DEFVAL      { 0 }
   ::= { xdsl2LineConfProfEntry 41 }
xdsl2LConfProfDpboFMin OBJECT-TYPE
   SYNTAX      Unsigned32 (0..2048)
   UNITS       "4.3125 kHz"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the minimum frequency
       from which the DPBO shall be applied. It ranges from 0 kHz (coded
       as 0) to 8832 kHz (coded as 2048) in steps of 4.3125 kHz. This
       parameter is used only for G.993.2."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.13 (DPBOFMIN)
   "
   DEFVAL      { 32 }
   ::= { xdsl2LineConfProfEntry 42 }
xdsl2LConfProfDpboFMax OBJECT-TYPE
   SYNTAX      Unsigned32 (32..6956)
   UNITS       "4.3125 kHz"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the maximum frequency
       at which DPBO may be applied. It ranges from 138 kHz (coded as
       32) to 29997.75 kHz (coded as 6956) in steps of 4.3125 kHz.
       This parameter is used only for G.993.2."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.13 (DPBOFMAX)
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   "
   DEFVAL      { 512 }
   ::= { xdsl2LineConfProfEntry 43 }
xdsl2LConfProfUpboKL  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..1280)
   UNITS       "0.1 dB"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the electrical length
       expressed in dB at 1MHz, kl0, configured by the CO-MIB.
       The value ranges from 0 (coded as 0) to 128 dB (coded as 1280) in
       steps of 0.1 dB. This parameter is relevant only if
       xdsl2LConfProfUpboKLF is set to override(2), which indicates that
       this parameter's value will override the VTUs' determination of
       the electrical length.
       If xdsl2LConfProfUpboKLF is set either to auto(1) or
       disableUpbo(3), then this parameter will be ignored."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.14 (UPBOKL)"
   DEFVAL      { 0 }
   ::= { xdsl2LineConfProfEntry 44 }
xdsl2LConfProfUpboKLF OBJECT-TYPE
   SYNTAX      Xdsl2UpboKLF
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Defines the upstream power backoff force mode.
       The three possible mode values are:
          auto(1),
          override(2),
          disableUpbo(3)."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.14 (UPBOKLF)
   "
   DEFVAL      { disableUpbo }
   ::= { xdsl2LineConfProfEntry 45 }
xdsl2LConfProfUs0Mask  OBJECT-TYPE
   SYNTAX      Xdsl2LineUs0Mask
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The configuration parameter contains the US0 PSD masks to be
       allowed by the near-end xTU on the line. This parameter is only
       defined for G.993.2 Annex A. It is represented as a  bitmap (0 if
       not allowed and 1 if allowed)."
   REFERENCE    "ITU-T G.997.1 Amendment 1, paragraph #7.3.1.2.18
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                (US0MASK)"
   DEFVAL       { {} }
   ::= { xdsl2LineConfProfEntry 46 }
xdsl2LConfProfForceInp  OBJECT-TYPE
   SYNTAX      Xdsl2LineForceInp
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This parameter indicates that the framer settings of the
        bearer shall be selected such that the impulse noise protection
        computed according to the formula specified in the relevant
        Recommendation is greater than or equal to the minimal impulse
        noise protection requirement.
        This flag shall have the same value for all the bearers of one
        line in the same direction."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.5 (FORCEINP)"
   DEFVAL       { {} }
   ::= { xdsl2LineConfProfEntry 47 }
xdsl2LConfProfRowStatus  OBJECT-TYPE
   SYNTAX      RowStatus
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This object is used to create a new row or to modify or
       delete an existing row in this table.
       A profile is activated by setting this object to 'active'.
       When 'active' is set, the system will validate the profile.
       Before a profile can be deleted or taken out of service (by
       setting this object to 'destroy' or 'notInService'), it MUST be
       first unreferenced from all associated templates.
       When a row is created in this table, the SNMP agent should also
       create corresponding rows in the tables
       xdsl2LineConfProfModeSpecTable and
       xdsl2LineConfProfModeSpecBandUsTable.
       When a row is deleted in this table, the SNMP agent should also
       delete corresponding rows in the tables
       xdsl2LineConfProfModeSpecTable and
       xdsl2LineConfProfModeSpecBandUsTable."
   ::= { xdsl2LineConfProfEntry 48 }
------------------------------------------
--    xdsl2LineConfProfModeSpecTable    --
------------------------------------------
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xdsl2LineConfProfModeSpecTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2LineConfProfModeSpecEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineConfProfModeSpecTable extends the DSL
       line configuration profile by xDSL Mode Specific parameters.
       A row in this table that has an index of xdsl2LConfProfXdslMode
       == defMode(1), is called a 'mandatory' row.
       A row in this table that has an index such that
       xdsl2LConfProfXdslMode is not equal to defMode(1), is called an
       'optional' row.
       When a row in the xdsl2LineConfProfTable table (the parent row)
       is created, the SNMP agent will automatically create a
       'mandatory' row in this table.
       When the parent row is deleted, the SNMP agent will automatically
       delete all associated rows in this table.
       Any attempt to delete the 'mandatory' row using the
       xdsl2LConfProfModeSpecRowStatus attribute will be rejected by the
       SNMP agent.
       The manager MAY create an 'optional' row in this table using the
       xdsl2LConfProfModeSpecRowStatus attribute if the parent row
       exists.
       The manager MAY delete an 'optional' row in this table using the
       xdsl2LConfProfModeSpecRowStatus attribute at any time.
       If the actual transmission mode of a DSL line does not match one
       of the 'optional' rows in this table, then the line will use the
       PSD configuration from the 'mandatory' row.
       Entries in this table MUST be maintained in a persistent
       manner."
   ::= { xdsl2ProfileLine 3 }
xdsl2LineConfProfModeSpecEntry  OBJECT-TYPE
   SYNTAX      Xdsl2LineConfProfModeSpecEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineConfProfModeSpecTable extends the
       DSL line configuration profile by DSL Mode Specific
       parameters."
   INDEX  { xdsl2LConfProfProfileName, xdsl2LConfProfXdslMode }
   ::= { xdsl2LineConfProfModeSpecTable 1 }
Xdsl2LineConfProfModeSpecEntry  ::=
   SEQUENCE {
      xdsl2LConfProfXdslMode             Xdsl2OperationModes,
      xdsl2LConfProfMaxNomPsdDs          Integer32,
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      xdsl2LConfProfMaxNomPsdUs          Integer32,
      xdsl2LConfProfMaxNomAtpDs          Unsigned32,
      xdsl2LConfProfMaxNomAtpUs          Unsigned32,
      xdsl2LConfProfMaxAggRxPwrUs        Integer32,
      xdsl2LConfProfPsdMaskDs            Xdsl2PsdMaskDs,
      xdsl2LConfProfPsdMaskUs            Xdsl2PsdMaskUs,
      xdsl2LConfProfPsdMaskSelectUs      Xdsl2LinePsdMaskSelectUs,
      xdsl2LConfProfClassMask            Xdsl2LineClassMask,
      xdsl2LConfProfLimitMask            Xdsl2LineLimitMask,
      xdsl2LConfProfUs0Disable           Xdsl2LineUs0Disable,
      xdsl2LConfProfModeSpecRowStatus    RowStatus
   }
xdsl2LConfProfXdslMode    OBJECT-TYPE
   SYNTAX      Xdsl2OperationModes
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The DSL Mode is a way of categorizing the various xDSL
       transmission modes into groups, each group (xDSL Mode) shares
       the same PSD configuration.
       There should be multiple entries in this table for a given line
       profile in case multiple bits are set in
       xdsl2LConfProfXtuTransSysEna for that profile."
   REFERENCE    "DSL Forum TR-129, paragraph #5.5"
   ::= { xdsl2LineConfProfModeSpecEntry 1 }
xdsl2LConfProfMaxNomPsdDs  OBJECT-TYPE
   SYNTAX      Integer32(-600..-300)
   UNITS       "0.1 dBm/Hz"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The maximum nominal transmit PSD in the downstream direction
       during initialization and Showtime.  It ranges from -600 to -300
       units of 0.1 dBm/Hz.  (physical values are -60 to -30
       dBm/Hz)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.1 (MAXNOMPSDds)
   "
   DEFVAL       { -300 }
  ::= { xdsl2LineConfProfModeSpecEntry 2 }
xdsl2LConfProfMaxNomPsdUs  OBJECT-TYPE
   SYNTAX      Integer32(-600..-300)
   UNITS       "0.1 dBm/Hz"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
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      "The maximum nominal transmit PSD in the upstream direction
       during initialization and Showtime.  It ranges from -600 to
       -300 units of 0.1 dBm/Hz.  (physical values are -60 to -30
       dBm/Hz)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.2 (MAXNOMPSDus)
   "
   DEFVAL       { -300 }
   ::= { xdsl2LineConfProfModeSpecEntry 3 }
xdsl2LConfProfMaxNomAtpDs  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..255)
   UNITS       "0.1 dBm"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The maximum nominal aggregate transmit power in the
       downstream direction during initialization and Showtime.  It
       ranges from 0 to 255 units of 0.1 dBm (physical values are 0
       to 25.5 dBm)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.3 (MAXNOMATPds)
   "
   DEFVAL       { 255 }
   ::= { xdsl2LineConfProfModeSpecEntry 4 }
xdsl2LConfProfMaxNomAtpUs  OBJECT-TYPE
   SYNTAX      Unsigned32 (0..255)
   UNITS       "0.1 dBm"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The maximum nominal aggregate transmit power in the upstream
       direction during initialization and Showtime.  It ranges from
       0 to 255 units of 0.1 dBm (physical values are 0 to 25.5
       dBm)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.4 (MAXNOMATPus)
   "
   DEFVAL       { 255 }
   ::= { xdsl2LineConfProfModeSpecEntry 5 }
xdsl2LConfProfMaxAggRxPwrUs  OBJECT-TYPE
   SYNTAX      Integer32(-255..255 | 2147483647)
   UNITS       "0.1 dBm"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The maximum upstream aggregate receive power over the
       relevant set of subcarriers.  The xTU-C should verify that the
       upstream power cutback is such that this maximum aggregate
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       receive power value is honored.  It ranges from -255 to 255
       units of 0.1 dBm (physical values are -25.5 to 25.5 dBm).
       A value of 0x7FFFFFFF (2147483647) means that there is no
       limit."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.5 (MAXRXPWRus)
   "
   DEFVAL       { 255 }
   ::= { xdsl2LineConfProfModeSpecEntry 6 }
xdsl2LConfProfPsdMaskDs   OBJECT-TYPE
   SYNTAX      Xdsl2PsdMaskDs
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
     "The downstream PSD mask applicable at the U-C2 reference
      point.
      This parameter is used only for G.992.5 and it may impose PSD
      restrictions (breakpoints) in addition to the Limit PSD mask
      defined in G.992.5.
      This is a string of 32 pairs of values in the following
      structure:
      Octets 0-1 - Index of 1st subcarrier used in the context of a
                   first breakpoint.
      Octet 2    - The PSD reduction for the subcarrier indicated in
                   octets 0 and 1.
      Octets 3-5 - Same, for a 2nd breakpoint.
      Octets 6-8 - Same, for a 3rd breakpoint.
      This architecture continues until octets 94-95, which are
      associated with a 32nd breakpoint.
      Each subcarrier index is an unsigned number in the range 1 and
      NSCds.  Each PSD reduction value is in the range 0 (0dBm/Hz) to
      255 (-127.5dBm/Hz) with steps of 0.5dBm/Hz.  Valid values are in
      the range 0 to 190 (0 to -95dBm/Hz).
      When the number of breakpoints is less than 32, all remaining
      octets are set to the value 0.  Note that the content of this
      object should be correlated with the subcarriers mask and with
      the RFI setup."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.9 (PSDMASKds)
   "
     ::= { xdsl2LineConfProfModeSpecEntry 7 }
xdsl2LConfProfPsdMaskUs   OBJECT-TYPE
   SYNTAX      Xdsl2PsdMaskUs
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
     "The upstream PSD mask applicable at the U-R2 reference
      point.
Morgenstern, et al.      Expires January 8, 2009              [Page 140]
Internet-Draft               VDSL2-LINE MIB                    July 2008
      This parameter is used only for G.992.5 and it may impose PSD
      restrictions (breakpoints) in addition to the Limit PSD mask
      defined in G.992.5.
      This is a string of 16 pairs of values in the following
      structure:
      Octets 0-1 - Index of 1st subcarrier used in the context of a
                   first breakpoint.
      Octet 2    - The PSD reduction for the subcarrier indicated in
                   octets 0 and 1.
      Octets 3-5 - Same, for a 2nd breakpoint.
      Octets 6-8 - Same, for a 3rd breakpoint.
      This architecture continues until octets 9-47, which are
      associated with a 16th breakpoint.
      Each subcarrier index is an unsigned number in the range 1 and
      NSCus.  Each PSD reduction value is in the range 0 (0dBm/Hz) to
      255 (-127.5dBm/Hz) with steps of 0.5dBm/Hz.  Valid values are in
      the range 0 to 190 (0 to -95dBm/Hz).
      When the number of breakpoints is less than 16, all remaining
      octets are set to the value 0.  Note that the content of this
      object should be correlated with the subcarriers mask and with
      the RFI setup."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.12 (PSDMASKus)
   "
     ::= { xdsl2LineConfProfModeSpecEntry 8 }
xdsl2LConfProfPsdMaskSelectUs  OBJECT-TYPE
   SYNTAX      Xdsl2LinePsdMaskSelectUs
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
     "The selected upstream PSD mask.  This parameter is used only
      for Annexes J and M of G.992.3 and G.992.5, and the same
      selection is used for all relevant enabled bits in
      xdsl2LConfProfXtuTransSysEna."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.11
                (Upstream PSD mask selection)"
   DEFVAL       { adlu32Eu32 }
    ::= { xdsl2LineConfProfModeSpecEntry 9 }
xdsl2LConfProfClassMask  OBJECT-TYPE
   SYNTAX      Xdsl2LineClassMask
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "In order to reduce the number of configuration
       possibilities, the limit Power Spectral Density masks (see
       LIMITMASK) are grouped in PSD mask classes.
       Each class is designed such that the PSD levels of each limit PSD
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       mask of a specific class are equal in their respective passband
       above 552 kHz.
       This parameter is defined per VDSL2 Annex enabled in the
       xdsl2LConfProfXtuTransSysEna object. It selects a single PSD mask
       class per Annex that is activated at the VTU-O."
   REFERENCE    "ITU-T G.997.1 Amendment 1, paragraph #7.3.1.2.15
                (CLASSMASK)"
   DEFVAL       { a998ORb997M1cORc998B }
   ::= { xdsl2LineConfProfModeSpecEntry 10 }
xdsl2LConfProfLimitMask  OBJECT-TYPE
   SYNTAX      Xdsl2LineLimitMask
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter contains the G.993.2 limit
       PSD masks of the selected PSD mask class, enabled by the near-end
       xTU on this line for each class of profiles.
       This parameter is defined per VDSL2 Annex enabled in the
       xdsl2LConfProfXtuTransSysEna object.
       Through this parameter several limit PSD masks of the selected
       PSD mask class (xdsl2LConfProfClassMask) may be enabled. The
       enabling parameter is coded in a bitmap representation (0 if the
       associated mask is not allowed, 1 if it is allowed)."
   REFERENCE    "ITU-T G.997.1 Amendment 1, paragraph #7.3.1.2.16
                (LIMITMASK)"
   DEFVAL       { {} }
   ::= { xdsl2LineConfProfModeSpecEntry 11 }
xdsl2LConfProfUs0Disable  OBJECT-TYPE
   SYNTAX      Xdsl2LineUs0Disable
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter indicates if the use of US0 is
       disabled for each limit PSD mask enabled in the
       xdsl2LConfProfLimitMask parameter.
       This parameter is defined per VDSL2 Annex enabled in the
       xdsl2LConfProfXtuTransSysEna object.
       For each limit PSD mask enabled in xdsl2LConfProfLimitMask
       parameter, a bit shall indicate if US0 is disabled. The disabling
       parameter is coded as a bitmap. The bit is set to 1 if US0 is
       disabled for the associated limit mask.
       This parameter and the xdsl2LConfProfLimitMask parameter use the
       same structure."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.1.2.17 (US0DISABLE)
   "
   DEFVAL       { {} }
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   ::= { xdsl2LineConfProfModeSpecEntry 12 }
xdsl2LConfProfModeSpecRowStatus  OBJECT-TYPE
   SYNTAX      RowStatus
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This object is used to create a new row or to modify or
       delete an existing row in this table.
       A profile is activated by setting this object to 'active'.
       When 'active' is set, the system will validate the profile.
       Before a profile can be deleted or taken out of service (by
       setting this object to 'destroy' or 'notInService'), it MUST be
       first unreferenced from all associated templates."
   ::= { xdsl2LineConfProfModeSpecEntry 13 }
----------------------------------------------
--   xdsl2LineConfProfModeSpecBandUsTable   --
----------------------------------------------
xdsl2LineConfProfModeSpecBandUsTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2LineConfProfModeSpecBandUsEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineConfProfModeSpecBandUsTable extends
       xdsl2LineConfProfModeSpecTable with upstream-band-specific
       parameters for VDSL2, such as upstream power back-off
       parameters, xdsl2LConfProfUpboPsdA and xdsl2LConfProfUpboPsdB
       (UPBOPSD-pb).
       When a parent 'mandatory row' is created in
       xdsl2LineConfProfModeSpecTable, the SNMP agent will automatically
       create several 'mandatory' rows in this table--  one for each
       upstream band:
       Note: A mandatory row is one where xdsl2LConfProfXdslMode =
       defMode(1). When the parent row is deleted, the SNMP agent will
       automatically delete all associated rows in this table. Any
       attempt to delete a 'mandatory' row using the
       xdsl2LConfProfModeSpecBandUsRowStatus attribute will be rejected
       by the SNMP agent. The manager only MAY create a new 'optional'
       row in this table using the xdsl2LConfProfModeSpecBandUsRowStatus
       attribute if the associated parent optional row exists, and the
       value of xdsl2LConfProfXdslMode is a G.993.2 value.  The manager
       MAY delete an 'optional' row in this table using the
       xdsl2LConfProfModeSpecBandUsRowStatus attribute at any time.
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       With respect to xdsl2LConfProfUpboPsdA and xdsl2LConfProfUpboPsdB
       parameters, for a given upstream band, if an optional row is
       missing from this table, then that means upstream power back-off
       is disabled for that upstream band.
       Entries in this table MUST be maintained in a persistent
       manner."
   ::= { xdsl2ProfileLine 4 }
xdsl2LineConfProfModeSpecBandUsEntry  OBJECT-TYPE
   SYNTAX      Xdsl2LineConfProfModeSpecBandUsEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineConfProfModeSpecBandUsTable extends
       xdsl2LineConfProfModeSpecTable with upstream-band-specific
       parameters for VDSL2, such as upstream power back-off parameters,
       xdsl2LConfProfUpboPsdA and xdsl2LConfProfUpboPsdB (UPBOPSD-
       pb)."
   INDEX       { xdsl2LConfProfProfileName, xdsl2LConfProfXdslMode,
                 xdsl2LConfProfXdslBandUs}
   ::= { xdsl2LineConfProfModeSpecBandUsTable 1 }
Xdsl2LineConfProfModeSpecBandUsEntry  ::=
   SEQUENCE {
      xdsl2LConfProfXdslBandUs                 Xdsl2BandUs,
      xdsl2LConfProfUpboPsdA                   Integer32,
      xdsl2LConfProfUpboPsdB                   Integer32,
      xdsl2LConfProfModeSpecBandUsRowStatus    RowStatus
   }
xdsl2LConfProfXdslBandUs    OBJECT-TYPE
   SYNTAX      Xdsl2BandUs
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "Each value identifies a specific band in the upstream
       transmission direction (excluding US0 band)."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.14"
   ::= { xdsl2LineConfProfModeSpecBandUsEntry 1 }
xdsl2LConfProfUpboPsdA  OBJECT-TYPE
   SYNTAX      Integer32(4000..8095)
   UNITS       "0.01 dBm/Hz"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the 'a' reference
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       parameter of the UPBO reference PSD used to compute the
       upstream power back-off for the upstream band. A UPBOPSD
       defined for each band shall consist of two parameters [a, b].
       Parameter 'a' (xdsl2LConfProfUpboPsdA) ranges from 40 dBm/Hz
       (coded as 4000) to 80.95 dBm/Hz (coded as 8095) in steps of 0.01
       dBm/Hz; and parameter 'b' (xdsl2LConfProfUpboPsdB) ranges from 0
       dBm/Hz (coded as 0) to 40.95 dBm/Hz (coded as 4095) in steps of
       0.01 dBm/Hz. The UPBO reference PSD at the frequency 'f'
       expressed in MHz shall be equal to '-a-b(SQRT(f))'. Setting
       xdsl2LConfProfUpboPsdA to 4000 and xdsl2LConfProfUpboPsdB to 0 is
       a special configuration to disable UPBO in the respective
       upstream band."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.14 (UPBOPSD-pb)
   "
   DEFVAL      { 4000 }
  ::= { xdsl2LineConfProfModeSpecBandUsEntry 2 }
xdsl2LConfProfUpboPsdB  OBJECT-TYPE
   SYNTAX      Integer32(0..4095)
   UNITS       "0.01 dBm/Hz"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This configuration parameter defines the 'b' reference
       parameter of the UPBO reference PSD used to compute the
       upstream power back-off for the upstream band. A UPBOPSD
       defined for each band shall consist of two parameters [a, b].
       Parameter 'a' (xdsl2LConfProfUpboPsdA) ranges from 40 dBm/Hz
       (coded as 4000) to 80.95 dBm/Hz (coded as 8095) in steps of 0.01
       dBm/Hz; and parameter 'b' (xdsl2LConfProfUpboPsdB) ranges from 0
       dBm/Hz (coded as 0) to 40.95 dBm/Hz (coded as 4095) in steps of
       0.01 dBm/Hz. The UPBO reference PSD at the frequency 'f'
       expressed in MHz shall be equal to '-a-b(SQRT(f))'. Setting
       xdsl2LConfProfUpboPsdA to 4000 and xdsl2LConfProfUpboPsdB to 0 is
       a special configuration to disable UPBO in the respective
       upstream band."
   REFERENCE   "ITU-T G.997.1, paragraph #7.3.1.2.14 (UPBOPSD-pb)
   "
   DEFVAL      { 0 }
  ::= { xdsl2LineConfProfModeSpecBandUsEntry 3 }
xdsl2LConfProfModeSpecBandUsRowStatus  OBJECT-TYPE
   SYNTAX      RowStatus
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This object is used to create a new row or to modify or
       delete an existing row in this table.
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       A profile is activated by setting this object to 'active'.
       When 'active' is set, the system will validate the profile.
       Before a profile can be deleted or taken out of service (by
       setting this object to 'destroy' or 'notInService'), it MUST be
       first unreferenced from all associated templates."
   ::= { xdsl2LineConfProfModeSpecBandUsEntry 4 }
------------------------------------------------
--          xdsl2ChConfProfileTable           --
------------------------------------------------
xdsl2ChConfProfileTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2ChConfProfileEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2ChConfProfileTable contains DSL channel
       profile configuration.
       Entries in this table MUST be maintained in a persistent
       manner."
   ::= { xdsl2ProfileChannel 1 }
xdsl2ChConfProfileEntry  OBJECT-TYPE
   SYNTAX      Xdsl2ChConfProfileEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2ChConfProfileTable contains DSL channel
       profile configuration.
       A default profile with an index of 'DEFVAL' will always exist and
       its parameters will be set to vendor-specific values, unless
       otherwise specified in this document."
   INDEX  { xdsl2ChConfProfProfileName }
   ::= { xdsl2ChConfProfileTable 1 }
Xdsl2ChConfProfileEntry  ::=
   SEQUENCE {
      xdsl2ChConfProfProfileName          SnmpAdminString,
      xdsl2ChConfProfMinDataRateDs        Unsigned32,
      xdsl2ChConfProfMinDataRateUs        Unsigned32,
      xdsl2ChConfProfMinResDataRateDs     Unsigned32,
      xdsl2ChConfProfMinResDataRateUs     Unsigned32,
      xdsl2ChConfProfMaxDataRateDs        Unsigned32,
      xdsl2ChConfProfMaxDataRateUs        Unsigned32,
      xdsl2ChConfProfMinDataRateLowPwrDs  Unsigned32,
      xdsl2ChConfProfMinDataRateLowPwrUs  Unsigned32,
      xdsl2ChConfProfMaxDelayDs           Unsigned32,
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      xdsl2ChConfProfMaxDelayUs           Unsigned32,
      xdsl2ChConfProfMinProtectionDs      Xdsl2SymbolProtection,
      xdsl2ChConfProfMinProtectionUs      Xdsl2SymbolProtection,
      xdsl2ChConfProfMinProtection8Ds     Xdsl2SymbolProtection8,
      xdsl2ChConfProfMinProtection8Us     Xdsl2SymbolProtection8,
      xdsl2ChConfProfMaxBerDs             Xdsl2MaxBer,
      xdsl2ChConfProfMaxBerUs             Xdsl2MaxBer,
      xdsl2ChConfProfUsDataRateDs         Unsigned32,
      xdsl2ChConfProfDsDataRateDs         Unsigned32,
      xdsl2ChConfProfUsDataRateUs         Unsigned32,
      xdsl2ChConfProfDsDataRateUs         Unsigned32,
      xdsl2ChConfProfImaEnabled           TruthValue,
      xdsl2ChConfProfMaxDelayVar          Unsigned32,
      xdsl2ChConfProfInitPolicy           Xdsl2ChInitPolicy,
      xdsl2ChConfProfRowStatus            RowStatus
   }
xdsl2ChConfProfProfileName  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "This object identifies a row in this table."
   ::= { xdsl2ChConfProfileEntry 1 }
xdsl2ChConfProfMinDataRateDs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Minimum Data Rate on Downstream direction.  The minimum net
       data rate for the bearer channel, coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.1
                (Minimum data rate)"
   ::= { xdsl2ChConfProfileEntry 2 }
xdsl2ChConfProfMinDataRateUs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Minimum Data Rate on Upstream direction.  The minimum net
       data rate for the bearer channel, coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.1
                (Minimum data rate)"
   ::= { xdsl2ChConfProfileEntry 3 }
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xdsl2ChConfProfMinResDataRateDs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Minimum Reserved Data Rate on Downstream direction.  The
       minimum reserved net data rate for the bearer channel, coded
       in bit/s.  This parameter is used only if the Rate Adaptation
       Mode in the direction of the bearer channel (i.e.,
       xdsl2LConfProfRaModeDs) is set to dynamicRa."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.2
                (Minimum reserved data rate)"
   ::= { xdsl2ChConfProfileEntry 4 }
xdsl2ChConfProfMinResDataRateUs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Minimum Reserved Data Rate on Upstream direction.  The
       minimum reserved net data rate for the bearer channel, coded in
       bit/s.  This parameter is used only if the Rate Adaptation Mode
       in the direction of the bearer channel (i.e.,
       xdsl2LConfProfRaModeUs) is set to dynamicRa."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.2
                (Minimum reserved data rate)"
   ::= { xdsl2ChConfProfileEntry 5 }
xdsl2ChConfProfMaxDataRateDs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Maximum Data Rate on Downstream direction.  The maximum net
       data rate for the bearer channel, coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.3
                (Maximum data rate)"
   ::= { xdsl2ChConfProfileEntry 6 }
xdsl2ChConfProfMaxDataRateUs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
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      "Maximum Data Rate on Upstream direction.  The maximum net
       data rate for the bearer channel, coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.3
                (Maximum data rate)"
   ::= { xdsl2ChConfProfileEntry 7 }
xdsl2ChConfProfMinDataRateLowPwrDs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This parameter specifies the minimum net data rate for
       the bearer channel as desired by the operator of the system
       during the low power state (L1/L2). The power management low
       power states L1 and L2 are defined in ITU-T Recs G.992.2 and
       G.992.3 respectively.
       The data rate is coded in steps of bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.5
                (Minimum Data Rate in low power state)"
   ::= { xdsl2ChConfProfileEntry 8 }
xdsl2ChConfProfMinDataRateLowPwrUs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This parameter specifies the minimum net data rate for
       the bearer channel as desired by the operator of the system
       during the low power state (L1/L2). The power management low
       power states L1 and L2 are defined in ITU-T Recs G.992.2 and
       G.992.3 respectively.
       The data rate is coded in steps of bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.1.5
                (Minimum Data Rate in low power state)"
   ::= { xdsl2ChConfProfileEntry 9 }
xdsl2ChConfProfMaxDelayDs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..63)
   UNITS       "milliseconds"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Maximum Interleave Delay on Downstream direction.  The
       maximum one-way interleaving delay introduced by the PMS-TC on
       Downstream direction.  The xTUs shall choose the S (factor) and D
       (depth) values such that the actual one-way interleaving delay
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       (Xdsl2ChStatusActDelay) is as close as possible to, but less than
       or equal to xdsl2ChConfProfMaxDelayDs.  The delay is coded in ms,
       with the value 0 indicating no delay bound is being
       imposed."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.2
                (Maximum interleaving delay)"
   ::= { xdsl2ChConfProfileEntry 10 }
xdsl2ChConfProfMaxDelayUs  OBJECT-TYPE
   SYNTAX      Unsigned32(0..63)
   UNITS       "milliseconds"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Maximum Interleave Delay on Upstream direction.  The maximum
       one-way interleaving delay introduced by the PMS-TC on Upstream
       direction.  The xTUs shall choose the S (factor) and D (depth)
       values such that the actual one-way interleaving delay
       (Xdsl2ChStatusActDelay) is as close as possible to, but less than
       or equal to xdsl2ChConfProfMaxDelayUs.  The delay is coded in ms,
       with the value 0 indicating no delay bound is being
       imposed."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.2
                (Maximum interleaving delay)"
   ::= { xdsl2ChConfProfileEntry 11 }
xdsl2ChConfProfMinProtectionDs  OBJECT-TYPE
   SYNTAX      Xdsl2SymbolProtection
   UNITS       "symbols"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This parameter specifies the minimum impulse noise
       protection for the bearer channel if it is transported over DMT
       symbols with a subcarrier spacing of 4.3125 kHz. The impulse
       noise protection is expressed in DMT symbols with a subcarrier
       spacing of 4.3125 kHz and can take the values 1/2 and any integer
       from 0 to 16, inclusive. If the xTU does not support the
       configured INPMIN value, it shall use the nearest supported
       impulse noise protection greater than INPMIN."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.3 (INPMINds)"
   DEFVAL       { noProtection }
   ::= { xdsl2ChConfProfileEntry 12 }
xdsl2ChConfProfMinProtectionUs  OBJECT-TYPE
   SYNTAX      Xdsl2SymbolProtection
   UNITS       "symbols"
   MAX-ACCESS  read-create
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   STATUS      current
   DESCRIPTION
      "This parameter specifies the minimum impulse noise
       protection for the bearer channel if it is transported over DMT
       symbols with a subcarrier spacing of 4.3125 kHz. The impulse
       noise protection is expressed in DMT symbols with a subcarrier
       spacing of 4.3125 kHz and can take the values 1/2 and any integer
       from 0 to 16, inclusive. If the xTU does not support the
       configured INPMIN value, it shall use the nearest supported
       impulse noise protection greater than INPMIN."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.3 (INPMINus)"
   DEFVAL       { noProtection }
   ::= { xdsl2ChConfProfileEntry 13 }
xdsl2ChConfProfMinProtection8Ds  OBJECT-TYPE
   SYNTAX      Xdsl2SymbolProtection8
   UNITS       "symbols"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This parameter specifies the minimum impulse noise
       protection for the bearer channel if it is transported over DMT
       symbols with a subcarrier spacing of 8.625 kHz. The impulse noise
       protection is expressed in DMT symbols with a subcarrier spacing
       of 8.625 kHz and can take any integer value from 0 to 16,
       inclusive."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.4 (INPMIN8ds)
   "
   DEFVAL       { noProtection }
   ::= { xdsl2ChConfProfileEntry 14 }
xdsl2ChConfProfMinProtection8Us  OBJECT-TYPE
   SYNTAX      Xdsl2SymbolProtection8
   UNITS       "symbols"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This parameter specifies the minimum impulse noise
       protection for the bearer channel if it is transported over DMT
       symbols with a subcarrier spacing of 8.625 kHz. The impulse noise
       protection is expressed in DMT symbols with a subcarrier spacing
       of 8.625 kHz and can take any integer value from 0 to 16,
       inclusive."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.4 (INPMIN8us)
   "
   DEFVAL       { noProtection }
   ::= { xdsl2ChConfProfileEntry 15 }
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xdsl2ChConfProfMaxBerDs  OBJECT-TYPE
   SYNTAX      Xdsl2MaxBer
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Maximum Bit Error Ratio on Downstream direction.  The
       maximum bit error ratio for the bearer channel.  The parameter
       can take the following values (for 1E-3, 1E-5 or 1E-7):
          eminus3 (1),
          eminus5 (2),
          eminus7 (3)"
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.6
                (Maximum bit error ratio)"
   DEFVAL       { eminus5 }
  ::= { xdsl2ChConfProfileEntry 16 }
xdsl2ChConfProfMaxBerUs  OBJECT-TYPE
   SYNTAX      Xdsl2MaxBer
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Maximum Bit Error Ratio on Upstream direction.  The maximum
       bit error ratio for the bearer channel.  The parameter can take
       the following values (for 1E-3, 1E-5 or 1E-7):
          eminus3 (1),
          eminus5 (2),
          eminus7 (3)"
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.6
                (Maximum bit error ratio)"
   DEFVAL       { eminus5 }
   ::= { xdsl2ChConfProfileEntry 17 }
xdsl2ChConfProfUsDataRateDs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Data Rate Threshold Upshift for downstream direction.  An
       'Up-Shift rate change' event is triggered when the
       actual downstream data rate exceeds, by more than the threshold,
       the data rate at the last entry into Showtime.  The parameter is
       coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.8.1
                (Data rate threshold upshift)"
   ::= { xdsl2ChConfProfileEntry 18 }
xdsl2ChConfProfDsDataRateDs  OBJECT-TYPE
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   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Data Rate Threshold Downshift for downstream direction.  A
       'Down-Shift rate change' event is triggered when the
       actual downstream data rate is below the data rate at the last
       entry into Showtime, by more than the threshold.  The parameter
       is coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.8.2
                (Data rate threshold downshift)"
   ::= { xdsl2ChConfProfileEntry 19 }
xdsl2ChConfProfUsDataRateUs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Data Rate Threshold Upshift for upstream direction.  An
       'Up-Shift rate change' event is triggered when the
       actual upstream data rate exceeds, by more than the threshold,
       the data rate at the last entry into Showtime.  The parameter is
       coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.8.1
                (Data rate threshold upshift)"
   ::= { xdsl2ChConfProfileEntry 20 }
xdsl2ChConfProfDsDataRateUs  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "bits/second"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Data Rate Threshold Downshift for upstream direction.  A
       'Down-Shift rate change' event is triggered when the
       actual upstream data rate is below the data rate at the last
       entry into Showtime, by more than the threshold.  The parameter
       is coded in bit/s."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.2.8.2
                (Data rate threshold downshift)"
   ::= { xdsl2ChConfProfileEntry 21 }
xdsl2ChConfProfImaEnabled  OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-create
   STATUS      current
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   DESCRIPTION
      "IMA Mode Enable.  The parameter enables the IMA operation
       mode in the ATM Data Path.  Relevant only if the channel is of
       ATM Data Path.  When in 'enable' state, the ATM data
       path should comply with the requirements for IMA
       transmission."
   REFERENCE    "ITU-T G.997.1, paragraph #7.3.4.1
                (IMA operation mode enable parameter)"
   DEFVAL       { false }
 ::= { xdsl2ChConfProfileEntry 22 }
xdsl2ChConfProfMaxDelayVar  OBJECT-TYPE
   SYNTAX      Unsigned32(1..255)
   UNITS       "0.1 milliseconds"
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Maximum delay variation (DVMAX).
       This optional VDSL2 specific parameter specifies the maximum
       value for the delay variation allowed in an OLR procedure.
       It is ranges from 1 to 254 units of 0.1 milliseconds (i.e., 0.1
       to 25.4 milliseconds) with the special value 255 which indicates
       that no delay variation bound is imposed."
   REFERENCE    "ITU-T G.997.1 Amendment 1, paragraph #7.3.2.9
   (DVMAX)"
   DEFVAL       { 255 }
 ::= { xdsl2ChConfProfileEntry 23 }
xdsl2ChConfProfInitPolicy  OBJECT-TYPE
   SYNTAX      Xdsl2ChInitPolicy
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "Channel Initialization Policy Selection (CIPOLICY).
       This optional parameter indicates which policy shall be applied
       to determine the transceiver configuration parameters at
       initialization. The valid values for CIPOLICY are policy0 and
       policy1. Those policies are defined in the respective
       Recommendations."
   REFERENCE    "ITU-T G.997.1 Amendment 1, paragraph #7.3.2.10
                (CIPOLICY)"
   DEFVAL       { policy0 }
 ::= { xdsl2ChConfProfileEntry 24 }
xdsl2ChConfProfRowStatus  OBJECT-TYPE
   SYNTAX      RowStatus
   MAX-ACCESS  read-create
   STATUS      current
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   DESCRIPTION
      "This object is used to create a new row or to modify or
       delete an existing row in this table.
       A profile is activated by setting this object to 'active'.
       When 'active' is set, the system will validate the profile.
       Before a profile can be deleted or taken out of service (by
       setting this object to 'destroy' or 'notInService'), it MUST be
       first unreferenced from all associated templates."
   ::= { xdsl2ChConfProfileEntry 25 }
------------------------------------------------
--      xdsl2LineAlarmConfTemplateTable       --
------------------------------------------------
xdsl2LineAlarmConfTemplateTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2LineAlarmConfTemplateEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineAlarConfTemplateTable contains DSL
       line alarm configuration templates.
        Entries in this table MUST be maintained in a persistent
        manner."
   ::= { xdsl2ProfileAlarmConf 1 }
xdsl2LineAlarmConfTemplateEntry  OBJECT-TYPE
   SYNTAX      Xdsl2LineAlarmConfTemplateEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2LineAlarmConfTemplateTable contains DSL
       line PM thresholds templates.
       A default template with an index of 'DEFVAL' will always exist
       and its parameters will be set to vendor specific values, unless
       otherwise specified in this document."
   INDEX  { xdsl2LAlarmConfTempTemplateName }
   ::= { xdsl2LineAlarmConfTemplateTable 1 }
Xdsl2LineAlarmConfTemplateEntry  ::=
   SEQUENCE {
      xdsl2LAlarmConfTempTemplateName      SnmpAdminString,
      xdsl2LAlarmConfTempLineProfile       SnmpAdminString,
      xdsl2LAlarmConfTempChan1ConfProfile  SnmpAdminString,
      xdsl2LAlarmConfTempChan2ConfProfile  SnmpAdminString,
      xdsl2LAlarmConfTempChan3ConfProfile  SnmpAdminString,
      xdsl2LAlarmConfTempChan4ConfProfile  SnmpAdminString,
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      xdsl2LAlarmConfTempRowStatus         RowStatus
   }
xdsl2LAlarmConfTempTemplateName  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "This object identifies a row in this table."
   ::= { xdsl2LineAlarmConfTemplateEntry 1 }
xdsl2LAlarmConfTempLineProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the DSL Line
       Thresholds Configuration Profile Table
       (xdsl2LineAlarmConfProfileTable) that applies to this line."
   REFERENCE    "DSL Forum TR-129, paragraph #8.2"
   DEFVAL       { "DEFVAL" }
   ::= { xdsl2LineAlarmConfTemplateEntry 2 }
xdsl2LAlarmConfTempChan1ConfProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(1..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the DSL
       Channel Thresholds Configuration Profile Table
       (xdsl2ChAlarmConfProfileTable) that applies for DSL bearer
       channel #1.  The channel profile name specified here MUST match
       the name of an existing row in the xdsl2ChAlarmConfProfileTable
       table."
   REFERENCE    "DSL Forum TR-129, paragraph #8.4"
   DEFVAL       { "DEFVAL" }
   ::= { xdsl2LineAlarmConfTemplateEntry 3 }
xdsl2LAlarmConfTempChan2ConfProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the DSL
       Channel Thresholds Configuration Profile Table
       (xdsl2ChAlarmConfProfileTable) that applies for DSL bearer
       channel #2.  The channel profile name specified here MUST match
       the name of an existing row in the xdsl2ChAlarmConfProfileTable
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       table.  If the channel is unused, then the object is set to a
       zero-length string."
   REFERENCE    "DSL Forum TR-129, paragraph #8.4"
   DEFVAL       { "" }
   ::= { xdsl2LineAlarmConfTemplateEntry 4 }
xdsl2LAlarmConfTempChan3ConfProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the DSL
       Channel Thresholds Configuration Profile Table
       (xdsl2ChAlarmConfProfileTable) that applies for DSL bearer
       channel #3.  The channel profile name specified here MUST match
       the name of an existing row in the xdsl2ChAlarmConfProfileTable
       table.
       This object may be set to a non-zero-length string only if
       xdsl2LAlarmConfTempChan2ConfProfile contains a non-zero-length
       string."
   REFERENCE    "DSL Forum TR-129, paragraph #8.4"
   DEFVAL       { "" }
   ::= { xdsl2LineAlarmConfTemplateEntry 5 }
xdsl2LAlarmConfTempChan4ConfProfile  OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "The value of this object identifies the row in the DSL
       Channel Thresholds Configuration Profile Table
       (xdsl2ChAlarmConfProfileTable) that applies for DSL bearer
       channel #4.  The channel profile name specified here MUST match
       the name of an existing row in the xdsl2ChAlarmConfProfileTable
       table.
       This object may be set to a non-zero-length string only if
       xdsl2LAlarmConfTempChan3ConfProfile contains a non-zero-length
       string."
   REFERENCE    "DSL Forum TR-129, paragraph #8.4"
   DEFVAL       { "" }
   ::= { xdsl2LineAlarmConfTemplateEntry 6 }
xdsl2LAlarmConfTempRowStatus  OBJECT-TYPE
   SYNTAX      RowStatus
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
      "This object is used to create a new row or to modify or
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       delete an existing row in this table.
       A template is activated by setting this object to 'active'.
       When 'active' is set, the system will validate the template.
       Before a template can be deleted or taken out of service (by
       setting this object to 'destroy' or 'notInService'), it MUST be
       first unreferenced from all associated lines."
   ::= { xdsl2LineAlarmConfTemplateEntry 7 }
------------------------------------------------
--      xdsl2LineAlarmConfProfileTable        --
------------------------------------------------
xdsl2LineAlarmConfProfileTable  OBJECT-TYPE
     SYNTAX      SEQUENCE  OF  Xdsl2LineAlarmConfProfileEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
      "The table xdsl2LineAlarmConfProfileTable contains DSL
       line PM thresholds profiles.
        Entries in this table MUST be maintained in a persistent
        manner."
     ::= { xdsl2ProfileAlarmConf 2 }
xdsl2LineAlarmConfProfileEntry  OBJECT-TYPE
     SYNTAX      Xdsl2LineAlarmConfProfileEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
      "The table xdsl2LineAlarmConfProfileTable contains DSL
       line PM thresholds profiles.
       A default profile with an index of 'DEFVAL' will always exist and
       its parameters will be set to vendor-specific values, unless
       otherwise specified in this document."
     INDEX  { xdsl2LineAlarmConfProfileName }
     ::= { xdsl2LineAlarmConfProfileTable 1 }
Xdsl2LineAlarmConfProfileEntry ::=
     SEQUENCE {
     xdsl2LineAlarmConfProfileName                SnmpAdminString,
     xdsl2LineAlarmConfProfileXtucThresh15MinFecs
                                          HCPerfIntervalThreshold,
     xdsl2LineAlarmConfProfileXtucThresh15MinEs
                                          HCPerfIntervalThreshold,
     xdsl2LineAlarmConfProfileXtucThresh15MinSes
                                           HCPerfIntervalThreshold,
Morgenstern, et al.      Expires January 8, 2009              [Page 158]
Internet-Draft               VDSL2-LINE MIB                    July 2008
     xdsl2LineAlarmConfProfileXtucThresh15MinLoss
                                           HCPerfIntervalThreshold,
     xdsl2LineAlarmConfProfileXtucThresh15MinUas
                                           HCPerfIntervalThreshold,
     xdsl2LineAlarmConfProfileXturThresh15MinFecs
                                           HCPerfIntervalThreshold,
     xdsl2LineAlarmConfProfileXturThresh15MinEs
                                           HCPerfIntervalThreshold,
     xdsl2LineAlarmConfProfileXturThresh15MinSes
                                           HCPerfIntervalThreshold,
     xdsl2LineAlarmConfProfileXturThresh15MinLoss
                                           HCPerfIntervalThreshold,
     xdsl2LineAlarmConfProfileXturThresh15MinUas
                                           HCPerfIntervalThreshold,
     xdsl2LineAlarmConfProfileThresh15MinFailedFullInt   Unsigned32,
     xdsl2LineAlarmConfProfileThresh15MinFailedShrtInt   Unsigned32,
     xdsl2LineAlarmConfProfileRowStatus                   RowStatus
     }
xdsl2LineAlarmConfProfileName  OBJECT-TYPE
     SYNTAX      SnmpAdminString (SIZE(1..32))
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
     "This object identifies a row in this table."
     ::= { xdsl2LineAlarmConfProfileEntry 1 }
xdsl2LineAlarmConfProfileXtucThresh15MinFecs  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MFecs counter, when
      xdsl2PMLCurrUnit is xtuc {1}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 2 }
xdsl2LineAlarmConfProfileXtucThresh15MinEs  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
     MAX-ACCESS  read-create
     STATUS      current
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     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MEs counter, when
      xdsl2PMLCurrUnit is xtuc {1}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 3 }
xdsl2LineAlarmConfProfileXtucThresh15MinSes  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MSes counter, when
      xdsl2PMLCurrUnit is xtuc {1}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 4 }
xdsl2LineAlarmConfProfileXtucThresh15MinLoss  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MLoss counter, when
      xdsl2PMLCurrUnit is xtuc {1}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 5 }
xdsl2LineAlarmConfProfileXtucThresh15MinUas  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MUas counter, when
      xdsl2PMLCurrUnit is xtuc {1}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
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   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 6 }
xdsl2LineAlarmConfProfileXturThresh15MinFecs  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MFecs counter, when
      xdsl2PMLCurrUnit is xtur {2}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 7 }
xdsl2LineAlarmConfProfileXturThresh15MinEs  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MEs counter, when
      xdsl2PMLCurrUnit is xtur {2}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 8 }
xdsl2LineAlarmConfProfileXturThresh15MinSes  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MSes counter, when
      xdsl2PMLCurrUnit is xtur {2}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 9 }
xdsl2LineAlarmConfProfileXturThresh15MinLoss  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
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     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MLoss counter, when
      xdsl2PMLCurrUnit is xtur {2}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 10 }
xdsl2LineAlarmConfProfileXturThresh15MinUas  OBJECT-TYPE
     SYNTAX      HCPerfIntervalThreshold
     UNITS       "seconds"
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLCurr15MUas counter, when
      xdsl2PMLCurrUnit is xtur {2}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 11 }
xdsl2LineAlarmConfProfileThresh15MinFailedFullInt  OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLInitCurr15MfailedFullInits
      counter.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 12 }
xdsl2LineAlarmConfProfileThresh15MinFailedShrtInt  OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMLInitCurr15MFailedShortInits
      counter.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
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   DEFVAL       { 0 }
     ::= { xdsl2LineAlarmConfProfileEntry 13 }
xdsl2LineAlarmConfProfileRowStatus  OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
      "This object is used to create a new row or to modify or
       delete an existing row in this table.
       A profile is activated by setting this object to 'active'.
       When 'active' is set, the system will validate the profile.
       Before a profile can be deleted or taken out of service (by
       setting this object to 'destroy' or 'notInService'), it MUST be
       first unreferenced from all associated templates."
     ::= { xdsl2LineAlarmConfProfileEntry 14 }
------------------------------------------------
--       xdsl2ChAlarmConfProfileTable         --
------------------------------------------------
xdsl2ChAlarmConfProfileTable  OBJECT-TYPE
     SYNTAX      SEQUENCE  OF  Xdsl2ChAlarmConfProfileEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
      "The table xdsl2ChAlarmConfProfileTable contains DSL channel
       PM thresholds profiles.
       Entries in this table MUST be maintained in a persistent
       manner."
     ::= { xdsl2ProfileAlarmConf 3 }
xdsl2ChAlarmConfProfileEntry  OBJECT-TYPE
     SYNTAX      Xdsl2ChAlarmConfProfileEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
      "The table xdsl2ChAlarmConfProfileTable contains DSL channel
       PM thresholds profiles.
       A default profile with an index of 'DEFVAL' will always exist and
       its parameters will be set to vendor-specific values, unless
       otherwise specified in this document."
     INDEX  { xdsl2ChAlarmConfProfileName }
     ::= { xdsl2ChAlarmConfProfileTable 1 }
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Xdsl2ChAlarmConfProfileEntry ::=
     SEQUENCE {
     xdsl2ChAlarmConfProfileName
                                                     SnmpAdminString,
     xdsl2ChAlarmConfProfileXtucThresh15MinCodingViolations
                                                     Unsigned32,
     xdsl2ChAlarmConfProfileXtucThresh15MinCorrected Unsigned32,
     xdsl2ChAlarmConfProfileXturThresh15MinCodingViolations
                                                     Unsigned32,
     xdsl2ChAlarmConfProfileXturThresh15MinCorrected Unsigned32,
     xdsl2ChAlarmConfProfileRowStatus                RowStatus
     }
xdsl2ChAlarmConfProfileName  OBJECT-TYPE
     SYNTAX      SnmpAdminString (SIZE(1..32))
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
     "This object identifies a row in this table."
     ::= { xdsl2ChAlarmConfProfileEntry 1 }
xdsl2ChAlarmConfProfileXtucThresh15MinCodingViolations OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMChCurr15MCodingViolations
      counter, when xdsl2PMChCurrUnit is xtuc {1}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2ChAlarmConfProfileEntry 2 }
xdsl2ChAlarmConfProfileXtucThresh15MinCorrected  OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMChCurr15MCorrectedBlocks
      counter, when xdsl2PMChCurrUnit is xtuc {1}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2ChAlarmConfProfileEntry 3 }
xdsl2ChAlarmConfProfileXturThresh15MinCodingViolations  OBJECT-TYPE
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     SYNTAX      Unsigned32
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMChCurr15MCodingViolations
      counter, when xdsl2PMChCurrUnit is xtur {2}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2ChAlarmConfProfileEntry 4 }
xdsl2ChAlarmConfProfileXturThresh15MinCorrected  OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
     "A threshold for the xdsl2PMChCurr15MCorrectedBlocks
      counter, when xdsl2PMChCurrUnit is xtur {2}.
      The value 0 means that no threshold is specified for the
      associated counter."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.7.2"
   DEFVAL       { 0 }
     ::= { xdsl2ChAlarmConfProfileEntry 5 }
xdsl2ChAlarmConfProfileRowStatus  OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
      "This object is used to create a new row or to modify or
       delete an existing row in this table.
       A profile is activated by setting this object to 'active'.
       When 'active' is set, the system will validate the profile.
       Before a profile can be deleted or taken out of service (by
       setting this object to 'destroy' or 'notInService'), it MUST be
       first unreferenced from all associated templates."
     ::= { xdsl2ChAlarmConfProfileEntry 6 }
------------------------------------------------
--          PM line current counters          --
------------------------------------------------
xdsl2PMLineCurrTable  OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2PMLineCurrEntry
   MAX-ACCESS  not-accessible
   STATUS      current
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   DESCRIPTION
      "The table xdsl2PMLineCurrTable contains current Performance
       Monitoring results for DSL lines."
   ::= { xdsl2PMLine 1 }
xdsl2PMLineCurrEntry  OBJECT-TYPE
   SYNTAX      Xdsl2PMLineCurrEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineCurrTable contains current Performance
       Monitoring results for DSL lines.
       The index of this table is an interface index, where the
       interface has an ifType of vdsl2(xxx), together with a
       termination
       unit."
   INDEX  { ifIndex, xdsl2PMLCurrUnit }
   ::= { xdsl2PMLineCurrTable 1 }
Xdsl2PMLineCurrEntry  ::=
   SEQUENCE {
      xdsl2PMLCurrUnit                    Xdsl2Unit,
      xdsl2PMLCurr15MValidIntervals       Unsigned32,
      xdsl2PMLCurr15MInvalidIntervals     Unsigned32,
      xdsl2PMLCurr15MTimeElapsed          HCPerfTimeElapsed,
      xdsl2PMLCurr15MFecs                 Counter32,
      xdsl2PMLCurr15MEs                   Counter32,
      xdsl2PMLCurr15MSes                  Counter32,
      xdsl2PMLCurr15MLoss                 Counter32,
      xdsl2PMLCurr15MUas                  Counter32,
      xdsl2PMLCurr1DayValidIntervals      Unsigned32,
      xdsl2PMLCurr1DayInvalidIntervals    Unsigned32,
      xdsl2PMLCurr1DayTimeElapsed         HCPerfTimeElapsed,
      xdsl2PMLCurr1DayFecs                Counter32,
      xdsl2PMLCurr1DayEs                  Counter32,
      xdsl2PMLCurr1DaySes                 Counter32,
      xdsl2PMLCurr1DayLoss                Counter32,
      xdsl2PMLCurr1DayUas                 Counter32
   }
xdsl2PMLCurrUnit  OBJECT-TYPE
   SYNTAX      Xdsl2Unit
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The termination unit xtuc{1} or xtur{2}."
   ::= { xdsl2PMLineCurrEntry 1 }
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xdsl2PMLCurr15MValidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Valid intervals."
   ::= { xdsl2PMLineCurrEntry 2 }
xdsl2PMLCurr15MInvalidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Invalid intervals."
   ::= { xdsl2PMLineCurrEntry 3 }
xdsl2PMLCurr15MTimeElapsed  OBJECT-TYPE
   SYNTAX      HCPerfTimeElapsed
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total elapsed seconds in this interval."
   ::= { xdsl2PMLineCurrEntry 4 }
xdsl2PMLCurr15MFecs  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was at
       least one FEC correction event for one or more bearer channels in
       this line.  This parameter is inhibited during UAS or SES."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.1 (FECS-L)
                 and paragraph #7.2.1.2.1 (FECS-LFE)"
   ::= { xdsl2PMLineCurrEntry 5 }
xdsl2PMLCurr15MEs  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was:
          xTU-C: CRC-8 >= 1 for one or more bearer channels OR
                 LOS >= 1 OR SEF >=1 OR LPR >= 1
          xTU-R: FEBE >= 1 for one or more bearer channels OR
Morgenstern, et al.      Expires January 8, 2009              [Page 167]
Internet-Draft               VDSL2-LINE MIB                    July 2008
                 LOS-FE >=1 OR RDI >=1 OR LPR-FE >=1 .
       This parameter is inhibited during UAS."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.2 (ES-L)
                 and paragraph #7.2.1.2.2 (ES-LFE)"
   ::= { xdsl2PMLineCurrEntry 6 }
xdsl2PMLCurr15MSes  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was:
          xTU-C: (CRC-8 anomalies in one or more of the
                 received bearer channels) >= 18 OR LOS >= 1
                 OR SEF >= 1 OR LPR >= 1
          xTU-R: (FEBE anomalies in one or more of the
                 received bearer channels) >= 18 OR LOS-FE >= 1
                 OR RDI >= 1 OR LPR-FE >= 1 .
       This parameter is inhibited during UAS."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.3 (SES-L)
                 and paragraph #7.2.1.2.3 (SES-LFE)"
   ::= { xdsl2PMLineCurrEntry 7 }
xdsl2PMLCurr15MLoss  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was LOS (or
       LOS-FE for xTU-R)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.4 (LOSS-L)
                 and paragraph #7.2.1.2.4 (LOSS-LFE)"
   ::= { xdsl2PMLineCurrEntry 8 }
xdsl2PMLCurr15MUas  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds in Unavailability State during this
       interval.  Unavailability begins at the onset of 10 contiguous
       severely-errored seconds, and ends at the onset of 10 contiguous
       seconds with no severely-errored seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.5 (UAS-L)
                 and paragraph #7.2.1.2.5 (UAS-LFE)"
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   ::= { xdsl2PMLineCurrEntry 9 }
xdsl2PMLCurr1DayValidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Valid intervals."
   ::= { xdsl2PMLineCurrEntry 10 }
xdsl2PMLCurr1DayInvalidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Invalid intervals."
   ::= { xdsl2PMLineCurrEntry 11 }
xdsl2PMLCurr1DayTimeElapsed  OBJECT-TYPE
   SYNTAX      HCPerfTimeElapsed
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total elapsed seconds in this interval."
   ::= { xdsl2PMLineCurrEntry 12 }
xdsl2PMLCurr1DayFecs  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was at
       least one FEC correction event for one or more bearer channels in
       this line.  This parameter is inhibited during UAS or SES."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.1 (FECS-L)
                 and paragraph #7.2.1.2.1 (FECS-LFE)"
   ::= { xdsl2PMLineCurrEntry 13 }
xdsl2PMLCurr1DayEs  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was:
          xTU-C: CRC-8 >= 1 for one or more bearer channels OR
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                 LOS >= 1 OR SEF >= 1 OR LPR >= 1
          xTU-R: FEBE >= 1 for one or more bearer channels OR
                 LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1.
       This parameter is inhibited during UAS."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.2 (ES-L)
                 and paragraph #7.2.1.2.2 (ES-LFE)"
   ::= { xdsl2PMLineCurrEntry 14 }
xdsl2PMLCurr1DaySes  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was:
          xTU-C: (CRC-8 anomalies in one or more of the
                 received bearer channels) >= 18 OR LOS >= 1
                 OR SEF >= 1 OR LPR >= 1
          xTU-R: (FEBE anomalies in one or more of the
                 received bearer channels) >= 18 OR LOS-FE >= 1
                 OR RDI >= 1 OR LPR-FE >= 1 .
       This parameter is inhibited during UAS."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.3 (SES-L)
                 and paragraph #7.2.1.2.3 (SES-LFE)"
   ::= { xdsl2PMLineCurrEntry 15 }
xdsl2PMLCurr1DayLoss  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was LOS (or
       LOS-FE for xTU-R)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.4 (LOSS-L)
                 and paragraph #7.2.1.2.4 (LOSS-LFE)"
   ::= { xdsl2PMLineCurrEntry 16 }
xdsl2PMLCurr1DayUas  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds in Unavailability State during this
       interval.
       Unavailability begins at the onset of 10 contiguous severely-
       errored seconds, and ends at the onset of 10 contiguous seconds
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       with no severely-errored seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.5 (UAS-L)
                 and paragraph #7.2.1.2.5 (UAS-LFE)"
   ::= { xdsl2PMLineCurrEntry 17 }
------------------------------------------------
--          PM line init current counters     --
------------------------------------------------
xdsl2PMLineInitCurrTable   OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2PMLineInitCurrEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineInitCurrTable contains current
       initialization counters for DSL lines."
   ::= { xdsl2PMLine 2 }
xdsl2PMLineInitCurrEntry  OBJECT-TYPE
   SYNTAX      Xdsl2PMLineInitCurrEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineInitCurrTable contains current
       initialization counters for DSL lines.
       The index of this table is an interface index, where the
       interface has an ifType of vdsl2(xxx), and a termination
       unit."
   INDEX  { ifIndex }
   ::= { xdsl2PMLineInitCurrTable 1 }
Xdsl2PMLineInitCurrEntry  ::=
   SEQUENCE {
      xdsl2PMLInitCurr15MValidIntervals       Unsigned32,
      xdsl2PMLInitCurr15MInvalidIntervals     Unsigned32,
      xdsl2PMLInitCurr15MTimeElapsed          Unsigned32,
      xdsl2PMLInitCurr15MFullInits            Unsigned32,
      xdsl2PMLInitCurr15MFailedFullInits      Unsigned32,
      xdsl2PMLInitCurr15MShortInits           Unsigned32,
      xdsl2PMLInitCurr15MFailedShortInits     Unsigned32,
      xdsl2PMLInitCurr1DayValidIntervals      Unsigned32,
      xdsl2PMLInitCurr1DayInvalidIntervals    Unsigned32,
      xdsl2PMLInitCurr1DayTimeElapsed         Unsigned32,
      xdsl2PMLInitCurr1DayFullInits           Unsigned32,
      xdsl2PMLInitCurr1DayFailedFullInits     Unsigned32,
      xdsl2PMLInitCurr1DayShortInits          Unsigned32,
      xdsl2PMLInitCurr1DayFailedShortInits    Unsigned32
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   }
xdsl2PMLInitCurr15MValidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Valid intervals."
   ::= { xdsl2PMLineInitCurrEntry 1 }
xdsl2PMLInitCurr15MInvalidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Invalid intervals."
   ::= { xdsl2PMLineInitCurrEntry 2 }
xdsl2PMLInitCurr15MTimeElapsed  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total elapsed seconds in this interval."
   ::= { xdsl2PMLineInitCurrEntry 3 }
xdsl2PMLInitCurr15MFullInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of full initializations attempted on the line
       (successful and failed) during this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.1"
   ::= { xdsl2PMLineInitCurrEntry 4 }
xdsl2PMLInitCurr15MFailedFullInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of failed full initializations on the line during this
       interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.2"
   ::= { xdsl2PMLineInitCurrEntry 5 }
xdsl2PMLInitCurr15MShortInits  OBJECT-TYPE
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   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of short initializations attempted on the line
       (successful and failed) during this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.3"
   ::= { xdsl2PMLineInitCurrEntry 6 }
xdsl2PMLInitCurr15MFailedShortInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of failed short initializations on the line during
       this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.4"
   ::= { xdsl2PMLineInitCurrEntry 7 }
xdsl2PMLInitCurr1DayValidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Valid intervals."
   ::= { xdsl2PMLineInitCurrEntry 8 }
xdsl2PMLInitCurr1DayInvalidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Invalid intervals."
   ::= { xdsl2PMLineInitCurrEntry 9 }
xdsl2PMLInitCurr1DayTimeElapsed  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total elapsed seconds in this interval."
   ::= { xdsl2PMLineInitCurrEntry 10 }
xdsl2PMLInitCurr1DayFullInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
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   DESCRIPTION
      "Count of full initializations attempted on the line
       (successful and failed) during this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.1"
   ::= { xdsl2PMLineInitCurrEntry 11 }
xdsl2PMLInitCurr1DayFailedFullInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of failed full initializations on the line during this
       interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.2"
   ::= { xdsl2PMLineInitCurrEntry 12 }
xdsl2PMLInitCurr1DayShortInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of short initializations attempted on the line
       (successful and failed) during this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.3"
   ::= { xdsl2PMLineInitCurrEntry 13 }
xdsl2PMLInitCurr1DayFailedShortInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of failed short initializations on the line during
       this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.4"
   ::= { xdsl2PMLineInitCurrEntry 14 }
-------------------------------------------
--       PM line history 15 Minutes      --
-------------------------------------------
xdsl2PMLineHist15MinTable    OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2PMLineHist15MinEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineHist15MinTable contains PM line history
       for 15min intervals of DSL line."
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   ::= { xdsl2PMLine 3 }
xdsl2PMLineHist15MinEntry  OBJECT-TYPE
   SYNTAX      Xdsl2PMLineHist15MinEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineHist15MinTable contains PM line history
       for 15min intervals of DSL line.
       The index of this table is an interface index, where the
       interface
       has an ifType of vdsl2(xxx), together with a termination unit and
       an
       interval number."
   INDEX  { ifIndex,
            xdsl2PMLHist15MUnit,
            xdsl2PMLHist15MInterval }
   ::= { xdsl2PMLineHist15MinTable 1 }
Xdsl2PMLineHist15MinEntry  ::=
   SEQUENCE {
      xdsl2PMLHist15MUnit                 Xdsl2Unit,
      xdsl2PMLHist15MInterval             Unsigned32,
      xdsl2PMLHist15MMonitoredTime        Unsigned32,
      xdsl2PMLHist15MFecs                 Counter32,
      xdsl2PMLHist15MEs                   Counter32,
      xdsl2PMLHist15MSes                  Counter32,
      xdsl2PMLHist15MLoss                 Counter32,
      xdsl2PMLHist15MUas                  Counter32,
      xdsl2PMLHist15MValidInterval        TruthValue
   }
xdsl2PMLHist15MUnit  OBJECT-TYPE
   SYNTAX      Xdsl2Unit
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The termination unit xtuc{1} or xtur{2}."
   ::= { xdsl2PMLineHist15MinEntry 1 }
xdsl2PMLHist15MInterval  OBJECT-TYPE
   SYNTAX      Unsigned32 (1..96)
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The interval number."
   ::= { xdsl2PMLineHist15MinEntry 2 }
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xdsl2PMLHist15MMonitoredTime  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total seconds monitored in this interval."
   ::= { xdsl2PMLineHist15MinEntry 3 }
xdsl2PMLHist15MFecs  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was at
       least one FEC correction event for one or more bearer channels in
       this line.  This parameter is inhibited during UAS or SES."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.1 (FECS-L)
                 and paragraph #7.2.1.2.1 (FECS-LFE)"
   ::= { xdsl2PMLineHist15MinEntry 4 }
xdsl2PMLHist15MEs  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was:
          xTU-C: CRC-8 >= 1 for one or more bearer channels OR
                 LOS >= 1 OR SEF >= 1 OR LPR >= 1
          xTU-R: FEBE >= 1 for one or more bearer channels OR
                 LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1.
       This parameter is inhibited during UAS."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.2 (ES-L)
                 and paragraph #7.2.1.2.2 (ES-LFE)"
   ::= { xdsl2PMLineHist15MinEntry 5 }
xdsl2PMLHist15MSes  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was:
          xTU-C: (CRC-8 anomalies in one or more of the
                 received bearer channels) >= 18 OR LOS >= 1
                 OR SEF >= 1 OR LPR >= 1
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          xTU-R: (FEBE anomalies in one or more of the
                 received bearer channels) >= 18 OR LOS-FE >= 1
                 OR RDI >= 1 OR LPR-FE >= 1 .
       This parameter is inhibited during UAS."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.3 (SES-L)
                 and paragraph #7.2.1.2.3 (SES-LFE)"
   ::= { xdsl2PMLineHist15MinEntry 6 }
xdsl2PMLHist15MLoss  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was LOS (or
       LOS-FE for xTU-R)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.4 (LOSS-L)
                 and paragraph #7.2.1.2.4 (LOSS-LFE)"
   ::= { xdsl2PMLineHist15MinEntry 7 }
xdsl2PMLHist15MUas  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds in Unavailability State during this
       interval.
       Unavailability begins at the onset of 10 contiguous severely-
       errored seconds, and ends at the onset of 10 contiguous seconds
       with no severely-errored seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.5 (UAS-L)
                 and paragraph #7.2.1.2.5 (UAS-LFE)"
   ::= { xdsl2PMLineHist15MinEntry 8 }
xdsl2PMLHist15MValidInterval  OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This variable indicates if the data for this interval is
       valid."
   ::= { xdsl2PMLineHist15MinEntry 9 }
---------------------------------------
--       PM line history 1 Day       --
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---------------------------------------
xdsl2PMLineHist1DayTable     OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2PMLineHist1DayEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineHist1DayTable contains PM line history
       for 24-hour intervals of DSL line."
   ::= { xdsl2PMLine 4 }
xdsl2PMLineHist1DayEntry  OBJECT-TYPE
   SYNTAX      Xdsl2PMLineHist1DayEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineHist1DayTable contains PM line history
       for 24-hour intervals of DSL line.
       The index of this table is an interface index, where the
       interface has an ifType of vdsl2(xxx), together with a
       termination unit and
       an interval number."
   INDEX  { ifIndex,
            xdsl2PMLHist1DUnit,
            xdsl2PMLHist1DInterval }
   ::= { xdsl2PMLineHist1DayTable 1 }
Xdsl2PMLineHist1DayEntry  ::=
   SEQUENCE {
      xdsl2PMLHist1DUnit              Xdsl2Unit,
      xdsl2PMLHist1DInterval          Unsigned32,
      xdsl2PMLHist1DMonitoredTime     Unsigned32,
      xdsl2PMLHist1DFecs              Counter32,
      xdsl2PMLHist1DEs                Counter32,
      xdsl2PMLHist1DSes               Counter32,
      xdsl2PMLHist1DLoss              Counter32,
      xdsl2PMLHist1DUas               Counter32,
      xdsl2PMLHist1DValidInterval     TruthValue
   }
xdsl2PMLHist1DUnit  OBJECT-TYPE
   SYNTAX      Xdsl2Unit
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The termination unit."
   ::= { xdsl2PMLineHist1DayEntry 1 }
xdsl2PMLHist1DInterval  OBJECT-TYPE
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   SYNTAX      Unsigned32 (1..30)
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The interval number."
   ::= { xdsl2PMLineHist1DayEntry 2 }
xdsl2PMLHist1DMonitoredTime  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total seconds monitored in this interval."
   ::= { xdsl2PMLineHist1DayEntry 3 }
xdsl2PMLHist1DFecs  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was at
       least one FEC correction event for one or more bearer channels in
       this line.  This parameter is inhibited during UAS or SES."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.1 (FECS-L)
                 and paragraph #7.2.1.2.1 (FECS-LFE)"
   ::= { xdsl2PMLineHist1DayEntry 4 }
xdsl2PMLHist1DEs  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was:
          xTU-C: CRC-8 >= 1 for one or more bearer channels OR
                 LOS >= 1 OR SEF >= 1 OR LPR >= 1
          xTU-R: FEBE >= 1 for one or more bearer channels OR
                 LOS-FE >= 1 OR RDI >= 1 OR LPR-FE >= 1.
       This parameter is inhibited during UAS."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.2 (ES-L)
                 and paragraph #7.2.1.2.2 (ES-LFE)"
   ::= { xdsl2PMLineHist1DayEntry 5 }
xdsl2PMLHist1DSes  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
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   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was:
          xTU-C: (CRC-8 anomalies in one or more of the
                 received bearer channels) >= 18 OR LOS >= 1
                 OR SEF >= 1 OR LPR >= 1
          xTU-R: (FEBE anomalies in one or more of the
                 received bearer channels) >= 18 OR LOS-FE >= 1
                 OR RDI >= 1 OR LPR-FE >= 1 .
       This parameter is inhibited during UAS."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.3 (SES-L)
                 and paragraph #7.2.1.2.3 (SES-LFE)"
   ::= { xdsl2PMLineHist1DayEntry 6 }
xdsl2PMLHist1DLoss  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds during this interval that there was LOS (or
       LOS-FE for xTU-R)."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.4 (LOSS-L)
                 and paragraph #7.2.1.2.4 (LOSS-LFE)"
   ::= { xdsl2PMLineHist1DayEntry 7 }
xdsl2PMLHist1DUas  OBJECT-TYPE
   SYNTAX      Counter32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of seconds in Unavailability State during this
       interval.
       Unavailability begins at the onset of 10 contiguous severely-
       errored seconds, and ends at the onset of 10 contiguous seconds
       with no severely-errored seconds."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.1.5 (UAS-L)
                 and paragraph #7.2.1.2.5 (UAS-LFE)"
   ::= { xdsl2PMLineHist1DayEntry 8 }
xdsl2PMLHist1DValidInterval  OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This variable indicates if the data for this interval is
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       valid."
   ::= { xdsl2PMLineHist1DayEntry 9 }
-------------------------------------------
--     PM line init history 15 Minutes   --
-------------------------------------------
xdsl2PMLineInitHist15MinTable      OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2PMLineInitHist15MinEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineInitHist15MinTable contains PM line
       initialization history for 15-minutes intervals of DSL
       line."
   ::= { xdsl2PMLine 5 }
xdsl2PMLineInitHist15MinEntry  OBJECT-TYPE
   SYNTAX      Xdsl2PMLineInitHist15MinEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineInitHist15MinTable contains PM line
       initialization history for 15-minute intervals for DSL
       lines.
       The index of this table is an interface index, where the
       interface
       has an ifType of vdsl2(xxx), and an interval number."
   INDEX  { ifIndex,
            xdsl2PMLInitHist15MInterval }
   ::= { xdsl2PMLineInitHist15MinTable 1 }
Xdsl2PMLineInitHist15MinEntry  ::=
   SEQUENCE {
      xdsl2PMLInitHist15MInterval              Unsigned32,
      xdsl2PMLInitHist15MMonitoredTime         Unsigned32,
      xdsl2PMLInitHist15MFullInits             Unsigned32,
      xdsl2PMLInitHist15MFailedFullInits       Unsigned32,
      xdsl2PMLInitHist15MShortInits            Unsigned32,
      xdsl2PMLInitHist15MFailedShortInits      Unsigned32,
      xdsl2PMLInitHist15MValidInterval         TruthValue
   }
xdsl2PMLInitHist15MInterval  OBJECT-TYPE
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   SYNTAX      Unsigned32 (1..96)
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The interval number."
   ::= { xdsl2PMLineInitHist15MinEntry 1 }
xdsl2PMLInitHist15MMonitoredTime  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total seconds monitored in this interval."
   ::= { xdsl2PMLineInitHist15MinEntry 2 }
xdsl2PMLInitHist15MFullInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of full initializations attempted on the line
       (successful and failed) during this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.1"
   ::= { xdsl2PMLineInitHist15MinEntry 3 }
xdsl2PMLInitHist15MFailedFullInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of failed full initializations on the line during this
       interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.2"
   ::= { xdsl2PMLineInitHist15MinEntry 4 }
xdsl2PMLInitHist15MShortInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of short initializations attempted on the line
       (successful and failed) during this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.3"
   ::= { xdsl2PMLineInitHist15MinEntry 5 }
xdsl2PMLInitHist15MFailedShortInits  OBJECT-TYPE
   SYNTAX      Unsigned32
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   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of failed short initializations on the line during
       this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.4"
   ::= { xdsl2PMLineInitHist15MinEntry 6 }
xdsl2PMLInitHist15MValidInterval  OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This variable indicates if the data for this interval is
       valid."
   ::= { xdsl2PMLineInitHist15MinEntry 7 }
-------------------------------------------
--       PM line init history 1 Day      --
-------------------------------------------
xdsl2PMLineInitHist1DayTable       OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2PMLineInitHist1DayEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineInitHist1DayTable contains PM line
       initialization history for 24-hour intervals for DSL
       lines."
   ::= { xdsl2PMLine 6 }
xdsl2PMLineInitHist1DayEntry  OBJECT-TYPE
   SYNTAX      Xdsl2PMLineInitHist1DayEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMLineInitHist1DayTable contains PM line
       initialization history for 24-hour intervals for DSL
       lines.
       The index of this table is an interface index, where the
       interface has an ifType of vdsl2(xxx), together with an interval
       number."
   INDEX  { ifIndex,
            xdsl2PMLInitHist1DInterval }
   ::= { xdsl2PMLineInitHist1DayTable 1 }
Xdsl2PMLineInitHist1DayEntry  ::=
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   SEQUENCE {
      xdsl2PMLInitHist1DInterval              Unsigned32,
      xdsl2PMLInitHist1DMonitoredTime         Unsigned32,
      xdsl2PMLInitHist1DFullInits             Unsigned32,
      xdsl2PMLInitHist1DFailedFullInits       Unsigned32,
      xdsl2PMLInitHist1DShortInits            Unsigned32,
      xdsl2PMLInitHist1DFailedShortInits      Unsigned32,
      xdsl2PMLInitHist1DValidInterval         TruthValue
   }
xdsl2PMLInitHist1DInterval  OBJECT-TYPE
   SYNTAX      Unsigned32 (1..30)
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The interval number."
   ::= { xdsl2PMLineInitHist1DayEntry 1 }
xdsl2PMLInitHist1DMonitoredTime  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total seconds monitored in this interval."
   ::= { xdsl2PMLineInitHist1DayEntry 2 }
xdsl2PMLInitHist1DFullInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of full initializations attempted on the line
       (successful and failed) during this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.1"
    ::= { xdsl2PMLineInitHist1DayEntry 3 }
xdsl2PMLInitHist1DFailedFullInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of failed full initializations on the line during this
       interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.2"
   ::= { xdsl2PMLineInitHist1DayEntry 4 }
xdsl2PMLInitHist1DShortInits  OBJECT-TYPE
Morgenstern, et al.      Expires January 8, 2009              [Page 184]
Internet-Draft               VDSL2-LINE MIB                    July 2008
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of short initializations attempted on the line
       (successful and failed) during this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.3"
   ::= { xdsl2PMLineInitHist1DayEntry 5 }
xdsl2PMLInitHist1DFailedShortInits  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of failed short initializations on the line during
       this interval."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.1.3.4"
   ::= { xdsl2PMLineInitHist1DayEntry 6 }
xdsl2PMLInitHist1DValidInterval  OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This variable indicates if the data for this interval is
       valid."
   ::= { xdsl2PMLineInitHist1DayEntry 7 }
---------------------------------------------------
--          PM channel current counters          --
---------------------------------------------------
xdsl2PMChCurrTable        OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2PMChCurrEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMChCurrTable contains current Performance
       Monitoring results for DSL channels."
   ::= { xdsl2PMChannel 1 }
xdsl2PMChCurrEntry  OBJECT-TYPE
   SYNTAX      Xdsl2PMChCurrEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMChCurrTable contains current Performance
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       Monitoring results for DSL channels.
       The index of this table is an interface index, where the
       interface has an ifType value which is applicable for a DSL
       channel, together with a termination unit."
   INDEX  { ifIndex, xdsl2PMChCurrUnit }
   ::= { xdsl2PMChCurrTable 1 }
Xdsl2PMChCurrEntry  ::=
   SEQUENCE {
      xdsl2PMChCurrUnit                     Xdsl2Unit,
      xdsl2PMChCurr15MValidIntervals        Unsigned32,
      xdsl2PMChCurr15MInvalidIntervals      Unsigned32,
      xdsl2PMChCurr15MTimeElapsed           HCPerfTimeElapsed,
      xdsl2PMChCurr15MCodingViolations      Unsigned32,
      xdsl2PMChCurr15MCorrectedBlocks       Unsigned32,
      xdsl2PMChCurr1DayValidIntervals       Unsigned32,
      xdsl2PMChCurr1DayInvalidIntervals     Unsigned32,
      xdsl2PMChCurr1DayTimeElapsed          HCPerfTimeElapsed,
      xdsl2PMChCurr1DayCodingViolations     Unsigned32,
      xdsl2PMChCurr1DayCorrectedBlocks      Unsigned32
   }
xdsl2PMChCurrUnit  OBJECT-TYPE
   SYNTAX      Xdsl2Unit
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
   "The termination unit."
   ::= { xdsl2PMChCurrEntry 1 }
xdsl2PMChCurr15MValidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Valid intervals."
   ::= { xdsl2PMChCurrEntry 2 }
xdsl2PMChCurr15MInvalidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Invalid intervals."
    ::= { xdsl2PMChCurrEntry 3 }
xdsl2PMChCurr15MTimeElapsed  OBJECT-TYPE
   SYNTAX      HCPerfTimeElapsed
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   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total elapsed seconds in this interval."
   ::= { xdsl2PMChCurrEntry 4 }
xdsl2PMChCurr15MCodingViolations  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of CRC-8 (FEBE for xTU-R) anomalies occurring in the
       channel during the interval.  This parameter is inhibited during
       UAS or SES.  If the CRC is applied over multiple channels, then
       each related CRC-8 (or FEBE) anomaly SHOULD increment each of the
       counters related to the individual channels."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.2.1.1 (CV-C)
                 and paragraph #7.2.2.2.1 (CV-CFE)"
  ::= { xdsl2PMChCurrEntry 5 }
xdsl2PMChCurr15MCorrectedBlocks  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of FEC (FFEC for xTU-R) anomalies (corrected code
       words) occurring in the channel during the interval.  This
       parameter is inhibited during UAS or SES.  If the FEC is applied
       over multiple channels, then each related FEC (or FFEC) anomaly
       SHOULD increment each of the counters related to the individual
       channels."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.2.1.2 (FEC-C)
                 and paragraph #7.2.2.2.2 (FEC-CFE)"
   ::= { xdsl2PMChCurrEntry 6 }
xdsl2PMChCurr1DayValidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Valid intervals."
   ::= { xdsl2PMChCurrEntry 7 }
xdsl2PMChCurr1DayInvalidIntervals  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
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   DESCRIPTION
      "Invalid intervals."
   ::= { xdsl2PMChCurrEntry 8 }
xdsl2PMChCurr1DayTimeElapsed  OBJECT-TYPE
   SYNTAX      HCPerfTimeElapsed
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total elapsed seconds in this interval."
   ::= { xdsl2PMChCurrEntry 9 }
xdsl2PMChCurr1DayCodingViolations  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of CRC-8 (FEBE for xTU-R) anomalies occurring in the
       channel during the interval.  This parameter is inhibited during
       UAS or SES.  If the CRC is applied over multiple channels, then
       each related CRC-8 (or FEBE) anomaly SHOULD increment each of the
       counters related to the individual channels."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.2.1.1 (CV-C)
                 and paragraph #7.2.2.2.1 (CV-CFE)"
   ::= { xdsl2PMChCurrEntry 10 }
xdsl2PMChCurr1DayCorrectedBlocks  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of FEC (FFEC for xTU-R) anomalies (corrected code
       words) occurring in the channel during the interval.  This
       parameter is inhibited during UAS or SES.  If the FEC is applied
       over multiple channels, then each related FEC (or FFEC) anomaly
       SHOULD increment each of the counters related to the individual
       channels."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.2.1.2 (FEC-C)
                 and paragraph #7.2.2.2.2 (FEC-CFE)"
   ::= { xdsl2PMChCurrEntry 11 }
-------------------------------------------
--    PM channel history 15 Minutes      --
-------------------------------------------
xdsl2PMChHist15MinTable         OBJECT-TYPE
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   SYNTAX      SEQUENCE  OF  Xdsl2PMChHist15MinEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMChHist15MinTable contains Performance
       Monitoring (PM) history for 15-minute intervals for DSL channels
       PM."
   ::= { xdsl2PMChannel 2 }
xdsl2PMChHist15MinEntry  OBJECT-TYPE
   SYNTAX      Xdsl2PMChHist15MinEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMChHist15MinTable contains Performance
       Monitoring (PM) history for 15-minute intervals for DSL channels
       PM.
       The index of this table is an interface index, where the
       interface has an ifType value which is applicable for a DSL
       channel, together with a termination unit and an interval
       number."
   INDEX  { ifIndex,
            xdsl2PMChHist15MUnit,
            xdsl2PMChHist15MInterval }
   ::= { xdsl2PMChHist15MinTable 1 }
Xdsl2PMChHist15MinEntry  ::=
   SEQUENCE {
      xdsl2PMChHist15MUnit                     Xdsl2Unit,
      xdsl2PMChHist15MInterval                 Unsigned32,
      xdsl2PMChHist15MMonitoredTime            Unsigned32,
      xdsl2PMChHist15MCodingViolations         Unsigned32,
      xdsl2PMChHist15MCorrectedBlocks          Unsigned32,
      xdsl2PMChHist15MValidInterval            TruthValue
   }
xdsl2PMChHist15MUnit  OBJECT-TYPE
   SYNTAX      Xdsl2Unit
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The termination unit."
   ::= { xdsl2PMChHist15MinEntry 1 }
xdsl2PMChHist15MInterval  OBJECT-TYPE
   SYNTAX      Unsigned32 (1..96)
   MAX-ACCESS  not-accessible
   STATUS      current
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   DESCRIPTION
      "The interval number."
   ::= { xdsl2PMChHist15MinEntry 2 }
xdsl2PMChHist15MMonitoredTime  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total seconds monitored in this interval."
   ::= { xdsl2PMChHist15MinEntry 3 }
xdsl2PMChHist15MCodingViolations  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of CRC-8 (FEBE for xTU-R) anomalies occurring in the
       channel during the interval.  This parameter is inhibited during
       UAS or SES.  If the CRC is applied over multiple channels, then
       each related CRC-8 (or FEBE) anomaly SHOULD increment each of the
       counters related to the individual channels."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.2.1.1 (CV-C)
                 and paragraph #7.2.2.2.1 (CV-CFE)"
  ::= { xdsl2PMChHist15MinEntry 4 }
xdsl2PMChHist15MCorrectedBlocks  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of FEC (FFEC for xTU-R) anomalies (corrected code
       words) occurring in the channel during the interval.  This
       parameter is inhibited during UAS or SES.  If the FEC is applied
       over multiple channels, then each related FEC (or FFEC) anomaly
       SHOULD increment each of the counters related to the individual
       channels."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.2.1.2 (FEC-C)
                 and paragraph #7.2.2.2.2 (FEC-CFE)"
   ::= { xdsl2PMChHist15MinEntry 5 }
xdsl2PMChHist15MValidInterval  OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This variable indicates if the data for this interval is
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       valid."
   ::= { xdsl2PMChHist15MinEntry 6 }
------------------------------------------
--        PM channel history 1 Day      --
------------------------------------------
xdsl2PMChHist1DTable         OBJECT-TYPE
   SYNTAX      SEQUENCE  OF  Xdsl2PMChHist1DEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMChHist1DTable contains Performance
       Monitoring (PM) history for 1-day intervals for DSL channels
       PM."
   ::= { xdsl2PMChannel 3 }
xdsl2PMChHist1DEntry  OBJECT-TYPE
   SYNTAX      Xdsl2PMChHist1DEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The table xdsl2PMChHist1DTable contains Performance
       Monitoring (PM) history for 1-day intervals for DSL channels PM.
       The index of this table is an interface index, where the
       interface has an ifType value which is applicable for a DSL
       channel, together with a termination unit and the interval
       number."
   INDEX  { ifIndex,
            xdsl2PMChHist1DUnit,
            xdsl2PMChHist1DInterval }
   ::= { xdsl2PMChHist1DTable 1 }
Xdsl2PMChHist1DEntry  ::=
   SEQUENCE {
      xdsl2PMChHist1DUnit                      Xdsl2Unit,
      xdsl2PMChHist1DInterval                  Unsigned32,
      xdsl2PMChHist1DMonitoredTime             Unsigned32,
      xdsl2PMChHist1DCodingViolations          Unsigned32,
      xdsl2PMChHist1DCorrectedBlocks           Unsigned32,
      xdsl2PMChHist1DValidInterval             TruthValue
   }
xdsl2PMChHist1DUnit  OBJECT-TYPE
   SYNTAX      Xdsl2Unit
   MAX-ACCESS  not-accessible
   STATUS      current
Morgenstern, et al.      Expires January 8, 2009              [Page 191]
Internet-Draft               VDSL2-LINE MIB                    July 2008
   DESCRIPTION
      "The termination unit."
    ::= { xdsl2PMChHist1DEntry 1 }
xdsl2PMChHist1DInterval  OBJECT-TYPE
   SYNTAX      Unsigned32 (1..30)
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
      "The interval number."
   ::= { xdsl2PMChHist1DEntry 2 }
xdsl2PMChHist1DMonitoredTime  OBJECT-TYPE
   SYNTAX      Unsigned32
   UNITS       "seconds"
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Total seconds monitored in this interval."
   ::= { xdsl2PMChHist1DEntry 3 }
xdsl2PMChHist1DCodingViolations  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of CRC-8 (FEBE for xTU-R) anomalies occurring in the
       channel during the interval.  This parameter is inhibited during
       UAS or SES.  If the CRC is applied over multiple channels, then
       each related CRC-8 (or FEBE) anomaly SHOULD increment each of the
       counters related to the individual channels."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.2.1.1 (CV-C)
                 and paragraph #7.2.2.2.1 (CV-CFE)"
   ::= { xdsl2PMChHist1DEntry 4 }
xdsl2PMChHist1DCorrectedBlocks  OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "Count of FEC (FFEC for xTU-R) anomalies (corrected code
       words) occurring in the channel during the interval.  This
       parameter is inhibited during UAS or SES.  If the FEC is applied
       over multiple channels, then each related FEC (or FFEC) anomaly
       SHOULD increment each of the counters related to the individual
       channels."
   REFERENCE    "ITU-T G.997.1, paragraph #7.2.2.1.2 (FEC-C)
                 and paragraph #7.2.2.2.2 (FEC-CFE)"
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   ::= { xdsl2PMChHist1DEntry 5 }
xdsl2PMChHist1DValidInterval  OBJECT-TYPE
   SYNTAX      TruthValue
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This variable indicates if the data for this interval is
       valid."
   ::= { xdsl2PMChHist1DEntry 6 }
-------------------------------------------
--          Notifications Group          --
-------------------------------------------
xdsl2LinePerfFECSThreshXtuc NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MFecs,
   xdsl2LineAlarmConfProfileXtucThresh15MinFecs
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the FEC seconds threshold
      has been reached/exceeded for the referred xTU-C."
   ::= { xdsl2Notifications 1 }
xdsl2LinePerfFECSThreshXtur NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MFecs,
   xdsl2LineAlarmConfProfileXturThresh15MinFecs
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the FEC seconds threshold
      has been reached/exceeded for the referred xTU-R."
   ::= { xdsl2Notifications 2 }
xdsl2LinePerfESThreshXtuc NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MEs,
   xdsl2LineAlarmConfProfileXtucThresh15MinEs
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the errored seconds
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      threshold has been reached/exceeded for the referred xTU-C."
   ::= { xdsl2Notifications 3 }
xdsl2LinePerfESThreshXtur NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MEs,
   xdsl2LineAlarmConfProfileXturThresh15MinEs
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the errored seconds
      threshold has been reached/exceeded for the referred xTU-R."
   ::= { xdsl2Notifications 4 }
xdsl2LinePerfSESThreshXtuc NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MSes,
   xdsl2LineAlarmConfProfileXtucThresh15MinSes
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the severely-errored seconds
      threshold has been reached/exceeded for the referred xTU-C."
   ::= { xdsl2Notifications 5 }
xdsl2LinePerfSESThreshXtur NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MSes,
   xdsl2LineAlarmConfProfileXturThresh15MinSes
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the severely-errored seconds
      threshold has been reached/exceeded for the referred xTU-R."
   ::= { xdsl2Notifications 6 }
xdsl2LinePerfLOSSThreshXtuc NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MLoss,
   xdsl2LineAlarmConfProfileXtucThresh15MinLoss
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the LOS seconds
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      threshold has been reached/exceeded for the referred xTU-C."
   ::= { xdsl2Notifications 7 }
xdsl2LinePerfLOSSThreshXtur NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MLoss,
   xdsl2LineAlarmConfProfileXturThresh15MinLoss
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the LOS seconds
      threshold has been reached/exceeded for the referred xTU-R."
   ::= { xdsl2Notifications 8 }
xdsl2LinePerfUASThreshXtuc NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MUas,
   xdsl2LineAlarmConfProfileXtucThresh15MinUas
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the unavailable seconds
      threshold has been reached/exceeded for the referred xTU-C."
   ::= { xdsl2Notifications 9 }
xdsl2LinePerfUASThreshXtur NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLCurr15MUas,
   xdsl2LineAlarmConfProfileXturThresh15MinUas
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the unavailable seconds
      threshold has been reached/exceeded for the referred xTU-R."
   ::= { xdsl2Notifications 10 }
xdsl2LinePerfCodingViolationsThreshXtuc NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMChCurr15MCodingViolations,
   xdsl2ChAlarmConfProfileXtucThresh15MinCodingViolations
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the coding violations
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      threshold has been reached/exceeded for the referred xTU-C."
   ::= { xdsl2Notifications 11 }
xdsl2LinePerfCodingViolationsThreshXtur NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMChCurr15MCodingViolations,
   xdsl2ChAlarmConfProfileXturThresh15MinCodingViolations
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the coding violations
      threshold has been reached/exceeded for the referred xTU-R."
   ::= { xdsl2Notifications 12 }
xdsl2LinePerfCorrectedThreshXtuc NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMChCurr15MCorrectedBlocks,
   xdsl2ChAlarmConfProfileXtucThresh15MinCorrected
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the corrected blocks
      (FEC events) threshold has been reached/exceeded for the
      referred xTU-C."
   ::= { xdsl2Notifications 13 }
xdsl2LinePerfCorrectedThreshXtur NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMChCurr15MCorrectedBlocks,
   xdsl2ChAlarmConfProfileXturThresh15MinCorrected
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the corrected blocks
      (FEC events) threshold has been reached/exceeded for the
      referred xTU-R."
   ::= { xdsl2Notifications 14 }
xdsl2LinePerfFailedFullInitThresh NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLInitCurr15MFailedFullInits,
   xdsl2LineAlarmConfProfileThresh15MinFailedFullInt
   }
   STATUS     current
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   DESCRIPTION
     "This notification indicates that the failed full
      initializations threshold has been reached/exceeded for the
      referred ADSL/ADSL2 or ADSL2 line."
   ::= { xdsl2Notifications 15 }
xdsl2LinePerfFailedShortInitThresh NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2PMLInitCurr15MFailedShortInits,
   xdsl2LineAlarmConfProfileThresh15MinFailedShrtInt
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that the failed short
      initializations threshold has been reached/exceeded for the
      referred VDSL2/ADSL/ADSL2 or ADSL2+ line."
   ::= { xdsl2Notifications 16 }
xdsl2LineStatusChangeXtuc NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2LineStatusXtuc
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that a status change is
      detected for the referred xTU-C."
   ::= { xdsl2Notifications 17 }
xdsl2LineStatusChangeXtur NOTIFICATION-TYPE
   OBJECTS
   {
   xdsl2LineStatusXtur
   }
   STATUS     current
   DESCRIPTION
     "This notification indicates that a status change is
      detected for the referred xTU-R."
   ::= { xdsl2Notifications 18 }
   -- conformance information
   xdsl2Groups OBJECT IDENTIFIER ::= { xdsl2Conformance 1 }
   xdsl2Compliances OBJECT IDENTIFIER ::= { xdsl2Conformance 2 }
   xdsl2LineMibCompliance MODULE-COMPLIANCE
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      STATUS  current
      DESCRIPTION
         "The compliance statement for SNMP entities which
          manage VDSL2/ADSL/ADSL2 and ADSL2+ interfaces."
      MODULE  -- this module
      MANDATORY-GROUPS
          {
          xdsl2LineGroup,
          xdsl2ChannelStatusGroup,
          xdsl2SCStatusGroup,
          xdsl2LineInventoryGroup,
          xdsl2LineConfTemplateGroup,
          xdsl2LineConfProfGroup,
          xdsl2LineConfProfModeSpecGroup,
          xdsl2LineConfProfModeSpecBandUsGroup,
          xdsl2ChConfProfileGroup,
          xdsl2LineAlarmConfTemplateGroup,
          xdsl2PMLineCurrGroup,
          xdsl2PMLineInitCurrGroup,
          xdsl2PMLineHist15MinGroup,
          xdsl2PMLineHist1DayGroup,
          xdsl2PMLineInitHist15MinGroup,
          xdsl2PMLineInitHist1DayGroup,
          xdsl2PMChCurrGroup,
          xdsl2PMChHist15MinGroup,
          xdsl2PMChHist1DGroup
          }
   GROUP  xdsl2LineFallbackGroup
      DESCRIPTION
        "The group of configuration, status, and commands
         objects on the line level that are associated with the fallback
         feature."
   GROUP  xdsl2LineBpscGroup
      DESCRIPTION
        "The group of configuration, status, and commands objects
         on the line level that are associated with requesting a bits
         per subcarrier measurement."
   GROUP  xdsl2LineSegmentGroup
      DESCRIPTION
        "The group of status, and commands objects on the line
         level that are used to hold the results of the bits per
         subcarrier measurement."
   GROUP  xdsl2ChannelStatusAtmGroup
      DESCRIPTION
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        "The group of status objects required when the data path
         is ATM."
   GROUP  xdsl2ChannelStatusPtmGroup
      DESCRIPTION
        "The group of status objects required when the data path
         is PTM."
   GROUP  xdsl2LineConfProfRaGroup
      DESCRIPTION
        "The group of objects required for controlling the
         rate-adaptive behavior of the line."
   GROUP  xdsl2LineConfProfMsgMinGroup
      DESCRIPTION
        "The group of objects required for controlling the rate
         reserved for Overhead traffic."
   GROUP  xdsl2LineAlarmConfProfileGroup
      DESCRIPTION
        "The group of objects that define the alarm thresholds
         on line level PM counters."
   GROUP  xdsl2ChAlarmConfProfileGroup
      DESCRIPTION
        "The group of objects that define the alarm thresholds
        on channel-level PM counters."
   GROUP  xdsl2ChConfProfileAtmGroup
      DESCRIPTION
        "The group of configuration objects required when the data
         path is ATM."
   GROUP  xdsl2ChConfProfileMinResGroup
      DESCRIPTION
        "The group of configuration objects required for the
         reserved data rate."
   GROUP  xdsl2ChConfProfileOptAttrGroup
      DESCRIPTION
        "The group of various optional channel configuration
        objects."
   GROUP  xdsl2PMLineInitCurrShortGroup
      DESCRIPTION
        "The group of PM counters for the current intervals short
         initializations."
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   GROUP  xdsl2PMLineInitHist15MinShortGroup
      DESCRIPTION
        "The group of PM counters for the previous 15-minutes
         intervals short initializations."
   GROUP  xdsl2PMLineInitHist1DayShortGroup
      DESCRIPTION
        "The group of PM counters for the previous 24-hour
         intervals short initializations."
   GROUP  xdsl2ScalarSCGroup
      DESCRIPTION
        "The group of objects that report the available memory
         resources for DELT processes."
   GROUP  xdsl2ThreshNotificationGroup
      DESCRIPTION
        "The group of thresholds crossing notifications."
   GROUP  xdsl2StatusChangeNotificationGroup
      DESCRIPTION
        "The group of status change notifications."
      ::= { xdsl2Compliances 1 }
   -- units of conformance
   xdsl2LineGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LineCnfgTemplate,
          xdsl2LineAlarmCnfgTemplate,
          xdsl2LineCmndConfPmsf,
          xdsl2LineCmndConfLdsf,
          xdsl2LineCmndConfLdsfFailReason,
          xdsl2LineCmndAutomodeColdStart,
          xdsl2LineCmndConfReset,
          xdsl2LineStatusXtuTransSys,
          xdsl2LineStatusPwrMngState,
          xdsl2LineStatusInitResult,
          xdsl2LineStatusLastStateDs,
          xdsl2LineStatusLastStateUs,
          xdsl2LineStatusXtur,
          xdsl2LineStatusXtuc,
          xdsl2LineStatusAttainableRateDs,
          xdsl2LineStatusAttainableRateUs,
          xdsl2LineStatusActPsdDs,
          xdsl2LineStatusActPsdUs,
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          xdsl2LineStatusActAtpDs,
          xdsl2LineStatusActAtpUs,
          xdsl2LineStatusActProfile,
          xdsl2LineStatusActLimitMask,
          xdsl2LineStatusActUs0Mask,
          xdsl2LineStatusActSnrModeDs,
          xdsl2LineStatusActSnrModeUs,
          xdsl2LineStatusElectricalLength,
          xdsl2LineStatusTssiDs,
          xdsl2LineStatusTssiUs,
          xdsl2LineStatusMrefPsdDs,
          xdsl2LineStatusMrefPsdUs,
          xdsl2LineStatusTrellisDs,
          xdsl2LineStatusTrellisUs,
          xdsl2LineStatusActualCe,
          xdsl2LineBandStatusLnAtten,
          xdsl2LineBandStatusSigAtten,
          xdsl2LineBandStatusSnrMargin
           }
      STATUS     current
      DESCRIPTION
         "The group of configuration, status, and commands objects
          on the line level."
      ::= { xdsl2Groups 1 }
   xdsl2LineFallbackGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LineCnfgFallbackTemplate,
          xdsl2LineStatusActTemplate
           }
      STATUS     current
      DESCRIPTION
         "The group of configuration, status, and commands
          objects on the line level that are associated with the
          fallback feature."
      ::= { xdsl2Groups 2 }
   xdsl2LineBpscGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LineCmndConfBpsc,
          xdsl2LineCmndConfBpscFailReason,
          xdsl2LineCmndConfBpscReqCount
           }
      STATUS     current
      DESCRIPTION
         "The group of configuration, status, and commands
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          objects on the line level that are associated with requesting
          a bits per subcarrier measurement."
      ::= { xdsl2Groups 3 }
   xdsl2LineSegmentGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LineSegmentBitsAlloc,
          xdsl2LineSegmentRowStatus
           }
      STATUS     current
      DESCRIPTION
         "The group of status, and commands objects on the line
          level that are used to hold the results of the bits per
          subcarrier measurement."
      ::= { xdsl2Groups 4 }
   xdsl2ChannelStatusGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2ChStatusActDataRate,
          xdsl2ChStatusPrevDataRate,
          xdsl2ChStatusActDelay,
          xdsl2ChStatusActInp,
          xdsl2ChStatusInpReport,
          xdsl2ChStatusNFec,
          xdsl2ChStatusRFec,
          xdsl2ChStatusLSymb,
          xdsl2ChStatusIntlvDepth,
          xdsl2ChStatusIntlvBlock,
          xdsl2ChStatusLPath
          }
      STATUS     current
      DESCRIPTION
          "The group of status objects on the channel level."
      ::= { xdsl2Groups 5 }
   xdsl2ChannelStatusAtmGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2ChStatusAtmStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of status objects on the data path level
          when it is ATM."
      ::= { xdsl2Groups 6 }
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   xdsl2ChannelStatusPtmGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2ChStatusPtmStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of status objects on the data path level
          when it is PTM."
      ::= { xdsl2Groups 7 }
   xdsl2SCStatusGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2SCStatusLinScale,
          xdsl2SCStatusLinScGroupSize,
          xdsl2SCStatusLogMt,
          xdsl2SCStatusLogScGroupSize,
          xdsl2SCStatusQlnMt,
          xdsl2SCStatusQlnScGroupSize,
          xdsl2SCStatusSnrMtime,
          xdsl2SCStatusSnrScGroupSize,
          xdsl2SCStatusBandLnAtten,
          xdsl2SCStatusBandSigAtten,
          xdsl2SCStatusAttainableRate,
          xdsl2SCStatusRowStatus,
          xdsl2SCStatusSegmentLinReal,
          xdsl2SCStatusSegmentLinImg,
          xdsl2SCStatusSegmentLog,
          xdsl2SCStatusSegmentQln,
          xdsl2SCStatusSegmentSnr,
          xdsl2SCStatusSegmentBitsAlloc,
          xdsl2SCStatusSegmentGainAlloc
          }
      STATUS     current
      DESCRIPTION
         "The group of status objects on the subcarrier level.
          They are updated as a result of a DELT process."
      ::= { xdsl2Groups 8 }
   xdsl2LineInventoryGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LInvG994VendorId,
          xdsl2LInvSystemVendorId,
          xdsl2LInvVersionNumber,
          xdsl2LInvSerialNumber,
          xdsl2LInvSelfTestResult,
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          xdsl2LInvTransmissionCapabilities
          }
      STATUS     current
      DESCRIPTION
          "The group of inventory objects per xTU."
      ::= { xdsl2Groups 9 }
   xdsl2LineConfTemplateGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LConfTempLineProfile,
          xdsl2LConfTempChan1ConfProfile,
          xdsl2LConfTempChan1RaRatioDs,
          xdsl2LConfTempChan1RaRatioUs,
          xdsl2LConfTempChan2ConfProfile,
          xdsl2LConfTempChan2RaRatioDs,
          xdsl2LConfTempChan2RaRatioUs,
          xdsl2LConfTempChan3ConfProfile,
          xdsl2LConfTempChan3RaRatioDs,
          xdsl2LConfTempChan3RaRatioUs,
          xdsl2LConfTempChan4ConfProfile,
          xdsl2LConfTempChan4RaRatioDs,
          xdsl2LConfTempChan4RaRatioUs,
          xdsl2LConfTempRowStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of objects in a line configuration
          template."
      ::= { xdsl2Groups 10 }
   xdsl2LineConfProfGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LConfProfScMaskDs,
          xdsl2LConfProfScMaskUs,
          xdsl2LConfProfVdsl2CarMask,
          xdsl2LConfProfRfiBands,
          xdsl2LConfProfRaModeDs,
          xdsl2LConfProfRaModeUs,
          xdsl2LConfProfTargetSnrmDs,
          xdsl2LConfProfTargetSnrmUs,
          xdsl2LConfProfMaxSnrmDs,
          xdsl2LConfProfMaxSnrmUs,
          xdsl2LConfProfMinSnrmDs,
          xdsl2LConfProfMinSnrmUs,
          xdsl2LConfProfCeFlag,
          xdsl2LConfProfSnrModeDs,
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          xdsl2LConfProfSnrModeUs,
          xdsl2LConfProfTxRefVnDs,
          xdsl2LConfProfTxRefVnUs,
          xdsl2LConfProfXtuTransSysEna,
          xdsl2LConfProfPmMode,
          xdsl2LConfProfL0Time,
          xdsl2LConfProfL2Time,
          xdsl2LConfProfL2Atpr,
          xdsl2LConfProfL2Atprt,
          xdsl2LConfProfProfiles,
          xdsl2LConfProfDpboEPsd,
          xdsl2LConfProfDpboEsEL,
          xdsl2LConfProfDpboEsCableModelA,
          xdsl2LConfProfDpboEsCableModelB,
          xdsl2LConfProfDpboEsCableModelC,
          xdsl2LConfProfDpboMus,
          xdsl2LConfProfDpboFMin,
          xdsl2LConfProfDpboFMax,
          xdsl2LConfProfUpboKL,
          xdsl2LConfProfUpboKLF,
          xdsl2LConfProfUs0Mask,
          xdsl2LConfProfForceInp,
          xdsl2LConfProfRowStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of objects in a line configuration
          profile."
      ::= { xdsl2Groups 11 }
   xdsl2LineConfProfRaGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LConfProfRaUsNrmDs,
          xdsl2LConfProfRaUsNrmUs,
          xdsl2LConfProfRaUsTimeDs,
          xdsl2LConfProfRaUsTimeUs,
          xdsl2LConfProfRaDsNrmDs,
          xdsl2LConfProfRaDsNrmUs,
          xdsl2LConfProfRaDsTimeDs,
          xdsl2LConfProfRaDsTimeUs
          }
      STATUS     current
      DESCRIPTION
         "The group of objects required for controlling the
          rate-adaptive behavior of the line."
      ::= { xdsl2Groups 12 }
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   xdsl2LineConfProfMsgMinGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LConfProfMsgMinUs,
          xdsl2LConfProfMsgMinDs
          }
      STATUS     current
      DESCRIPTION
         "The group of objects required for controlling the rate
          reserved for Overhead traffic."
      ::= { xdsl2Groups 13 }
   xdsl2LineConfProfModeSpecGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LConfProfMaxNomPsdDs,
          xdsl2LConfProfMaxNomPsdUs,
          xdsl2LConfProfMaxNomAtpDs,
          xdsl2LConfProfMaxNomAtpUs,
          xdsl2LConfProfMaxAggRxPwrUs,
          xdsl2LConfProfPsdMaskDs,
          xdsl2LConfProfPsdMaskUs,
          xdsl2LConfProfPsdMaskSelectUs,
          xdsl2LConfProfClassMask,
          xdsl2LConfProfLimitMask,
          xdsl2LConfProfUs0Disable,
          xdsl2LConfProfModeSpecRowStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of objects in a line configuration profile
          that have an instance for each operation mode allowed."
      ::= { xdsl2Groups 14 }
   xdsl2LineConfProfModeSpecBandUsGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LConfProfUpboPsdA,
          xdsl2LConfProfUpboPsdB,
          xdsl2LConfProfModeSpecBandUsRowStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of objects in a line configuration profile
          that have several per-upstream-band instances for each
          operation mode allowed."
      ::= { xdsl2Groups 15 }
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   xdsl2ChConfProfileGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2ChConfProfMinDataRateDs,
          xdsl2ChConfProfMinDataRateUs,
          xdsl2ChConfProfMaxDataRateDs,
          xdsl2ChConfProfMaxDataRateUs,
          xdsl2ChConfProfMinDataRateLowPwrDs,
          xdsl2ChConfProfMinDataRateLowPwrUs,
          xdsl2ChConfProfMaxDelayDs,
          xdsl2ChConfProfMaxDelayUs,
          xdsl2ChConfProfMinProtectionDs,
          xdsl2ChConfProfMinProtectionUs,
          xdsl2ChConfProfMinProtection8Ds,
          xdsl2ChConfProfMinProtection8Us,
          xdsl2ChConfProfMaxBerDs,
          xdsl2ChConfProfMaxBerUs,
          xdsl2ChConfProfUsDataRateDs,
          xdsl2ChConfProfDsDataRateDs,
          xdsl2ChConfProfUsDataRateUs,
          xdsl2ChConfProfDsDataRateUs,
          xdsl2ChConfProfRowStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of objects in a channel configuration
          profile."
      ::= { xdsl2Groups 16 }
   xdsl2ChConfProfileAtmGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2ChConfProfImaEnabled,
          xdsl2ChStatusAtmStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of configuration objects required when the data
          path is ATM."
      ::= { xdsl2Groups 17 }
   xdsl2ChConfProfileMinResGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2ChConfProfMinResDataRateDs,
          xdsl2ChConfProfMinResDataRateUs
          }
      STATUS     current
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      DESCRIPTION
         "The group of configuration objects required for the
          reserved data rate."
      ::= { xdsl2Groups 18 }
   xdsl2ChConfProfileOptAttrGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2ChConfProfMaxDelayVar,
          xdsl2ChConfProfInitPolicy
          }
      STATUS     current
      DESCRIPTION
         "The group of various optional channel configuration
          parameters."
      ::= { xdsl2Groups 19 }
   xdsl2LineAlarmConfTemplateGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LAlarmConfTempLineProfile,
          xdsl2LAlarmConfTempChan1ConfProfile,
          xdsl2LAlarmConfTempChan2ConfProfile,
          xdsl2LAlarmConfTempChan3ConfProfile,
          xdsl2LAlarmConfTempChan4ConfProfile,
          xdsl2LAlarmConfTempRowStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of objects in a line alarm template."
      ::= { xdsl2Groups 20 }
   xdsl2LineAlarmConfProfileGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2LineAlarmConfProfileXtucThresh15MinFecs,
          xdsl2LineAlarmConfProfileXtucThresh15MinEs,
          xdsl2LineAlarmConfProfileXtucThresh15MinSes,
          xdsl2LineAlarmConfProfileXtucThresh15MinLoss,
          xdsl2LineAlarmConfProfileXtucThresh15MinUas,
          xdsl2LineAlarmConfProfileXturThresh15MinFecs,
          xdsl2LineAlarmConfProfileXturThresh15MinEs,
          xdsl2LineAlarmConfProfileXturThresh15MinSes,
          xdsl2LineAlarmConfProfileXturThresh15MinLoss,
          xdsl2LineAlarmConfProfileXturThresh15MinUas,
          xdsl2LineAlarmConfProfileThresh15MinFailedFullInt,
          xdsl2LineAlarmConfProfileThresh15MinFailedShrtInt,
          xdsl2LineAlarmConfProfileRowStatus
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          }
      STATUS     current
      DESCRIPTION
         "The group of objects in a line alarm profile."
      ::= { xdsl2Groups 21 }
   xdsl2ChAlarmConfProfileGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2ChAlarmConfProfileXtucThresh15MinCodingViolations,
          xdsl2ChAlarmConfProfileXtucThresh15MinCorrected,
          xdsl2ChAlarmConfProfileXturThresh15MinCodingViolations,
          xdsl2ChAlarmConfProfileXturThresh15MinCorrected,
          xdsl2ChAlarmConfProfileRowStatus
          }
      STATUS     current
      DESCRIPTION
         "The group of objects in a channel alarm profile."
      ::= { xdsl2Groups 22 }
   xdsl2PMLineCurrGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMLCurr15MValidIntervals,
          xdsl2PMLCurr15MInvalidIntervals,
          xdsl2PMLCurr15MTimeElapsed,
          xdsl2PMLCurr15MFecs,
          xdsl2PMLCurr15MEs,
          xdsl2PMLCurr15MSes,
          xdsl2PMLCurr15MLoss,
          xdsl2PMLCurr15MUas,
          xdsl2PMLCurr1DayValidIntervals,
          xdsl2PMLCurr1DayInvalidIntervals,
          xdsl2PMLCurr1DayTimeElapsed,
          xdsl2PMLCurr1DayFecs,
          xdsl2PMLCurr1DayEs,
          xdsl2PMLCurr1DaySes,
          xdsl2PMLCurr1DayLoss,
          xdsl2PMLCurr1DayUas
          }
      STATUS     current
      DESCRIPTION
         "The group of objects that report the line-level
          counters for current PM intervals."
      ::= { xdsl2Groups 23 }
   xdsl2PMLineInitCurrGroup OBJECT-GROUP
      OBJECTS
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          {
          xdsl2PMLInitCurr15MValidIntervals,
          xdsl2PMLInitCurr15MInvalidIntervals,
          xdsl2PMLInitCurr15MTimeElapsed,
          xdsl2PMLInitCurr15MFullInits,
          xdsl2PMLInitCurr15MFailedFullInits,
          xdsl2PMLInitCurr1DayValidIntervals,
          xdsl2PMLInitCurr1DayInvalidIntervals,
          xdsl2PMLInitCurr1DayTimeElapsed,
          xdsl2PMLInitCurr1DayFullInits,
          xdsl2PMLInitCurr1DayFailedFullInits
          }
      STATUS     current
      DESCRIPTION
         "The group of objects that report the full
          initializations counters for current PM intervals."
      ::= { xdsl2Groups 24 }
   xdsl2PMLineInitCurrShortGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMLInitCurr15MShortInits,
          xdsl2PMLInitCurr15MFailedShortInits,
          xdsl2PMLInitCurr1DayShortInits,
          xdsl2PMLInitCurr1DayFailedShortInits
          }
      STATUS     current
      DESCRIPTION
         "The group of objects that report the short
          initializations counters for current PM intervals."
      ::= { xdsl2Groups 25 }
   xdsl2PMLineHist15MinGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMLHist15MMonitoredTime,
          xdsl2PMLHist15MFecs,
          xdsl2PMLHist15MEs,
          xdsl2PMLHist15MSes,
          xdsl2PMLHist15MLoss,
          xdsl2PMLHist15MUas,
          xdsl2PMLHist15MValidInterval
          }
      STATUS     current
      DESCRIPTION
         "The group of line-level PM counters for the previous
          15 minutes intervals."
      ::= { xdsl2Groups 26 }
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   xdsl2PMLineHist1DayGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMLHist1DMonitoredTime,
          xdsl2PMLHist1DFecs,
          xdsl2PMLHist1DEs,
          xdsl2PMLHist1DSes,
          xdsl2PMLHist1DLoss,
          xdsl2PMLHist1DUas,
          xdsl2PMLHist1DValidInterval
          }
      STATUS     current
      DESCRIPTION
         "The group of line-level PM counters for the previous
          24-hour intervals."
      ::= { xdsl2Groups 27 }
   xdsl2PMLineInitHist15MinGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMLInitHist15MMonitoredTime,
          xdsl2PMLInitHist15MFullInits,
          xdsl2PMLInitHist15MFailedFullInits,
          xdsl2PMLInitHist15MValidInterval
          }
      STATUS     current
      DESCRIPTION
         "The group of PM counters for the previous 15-minutes
          intervals full initializations."
      ::= { xdsl2Groups 28 }
   xdsl2PMLineInitHist15MinShortGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMLInitHist15MShortInits,
          xdsl2PMLInitHist15MFailedShortInits
          }
      STATUS     current
      DESCRIPTION
         "The group of PM counters for the previous 15-minutes
          intervals short initializations."
      ::= { xdsl2Groups 29 }
   xdsl2PMLineInitHist1DayGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMLInitHist1DMonitoredTime,
          xdsl2PMLInitHist1DFullInits,
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          xdsl2PMLInitHist1DFailedFullInits,
          xdsl2PMLInitHist1DValidInterval
          }
      STATUS     current
      DESCRIPTION
         "The group of PM counters for the previous 24-hour
          intervals full initializations."
      ::= { xdsl2Groups 30 }
   xdsl2PMLineInitHist1DayShortGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMLInitHist1DShortInits,
          xdsl2PMLInitHist1DFailedShortInits
          }
      STATUS     current
      DESCRIPTION
         "The group of PM counters for the previous 24-hour
          intervals short initializations."
      ::= { xdsl2Groups 31 }
   xdsl2PMChCurrGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMChCurr15MValidIntervals,
          xdsl2PMChCurr15MInvalidIntervals,
          xdsl2PMChCurr15MTimeElapsed,
          xdsl2PMChCurr15MCodingViolations,
          xdsl2PMChCurr15MCorrectedBlocks,
          xdsl2PMChCurr1DayValidIntervals,
          xdsl2PMChCurr1DayInvalidIntervals,
          xdsl2PMChCurr1DayTimeElapsed,
          xdsl2PMChCurr1DayCodingViolations,
          xdsl2PMChCurr1DayCorrectedBlocks
          }
      STATUS     current
      DESCRIPTION
         "The group of objects that report the channel-level
          counters for current PM intervals."
      ::= { xdsl2Groups 32 }
   xdsl2PMChHist15MinGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMChHist15MMonitoredTime,
          xdsl2PMChHist15MCodingViolations,
          xdsl2PMChHist15MCorrectedBlocks,
          xdsl2PMChHist15MValidInterval
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          }
      STATUS     current
      DESCRIPTION
         "The group of objects that report the channel-level
          counters for previous 15 minutes PM intervals."
      ::= { xdsl2Groups 33 }
   xdsl2PMChHist1DGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2PMChHist1DMonitoredTime,
          xdsl2PMChHist1DCodingViolations,
          xdsl2PMChHist1DCorrectedBlocks,
          xdsl2PMChHist1DValidInterval
          }
      STATUS     current
      DESCRIPTION
        "The group of objects that report the channel-level
        counters for previous 24-hour PM intervals."
      ::= { xdsl2Groups 34 }
   xdsl2ScalarSCGroup OBJECT-GROUP
      OBJECTS
          {
          xdsl2ScalarSCMaxInterfaces,
          xdsl2ScalarSCAvailInterfaces
          }
      STATUS     current
      DESCRIPTION
         "The group of objects that report the available memory
          resources for DELT processes."
      ::= { xdsl2Groups 35 }
   xdsl2ThreshNotificationGroup NOTIFICATION-GROUP
      NOTIFICATIONS
      {
      xdsl2LinePerfFECSThreshXtuc,
      xdsl2LinePerfFECSThreshXtur,
      xdsl2LinePerfESThreshXtuc,
      xdsl2LinePerfESThreshXtur,
      xdsl2LinePerfSESThreshXtuc,
      xdsl2LinePerfSESThreshXtur,
      xdsl2LinePerfLOSSThreshXtuc,
      xdsl2LinePerfLOSSThreshXtur,
      xdsl2LinePerfUASThreshXtuc,
      xdsl2LinePerfUASThreshXtur,
      xdsl2LinePerfCodingViolationsThreshXtuc,
      xdsl2LinePerfCodingViolationsThreshXtur,
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      xdsl2LinePerfCorrectedThreshXtuc,
      xdsl2LinePerfCorrectedThreshXtur,
      xdsl2LinePerfFailedFullInitThresh,
      xdsl2LinePerfFailedShortInitThresh
      }
      STATUS      current
      DESCRIPTION
         "This group supports notifications of significant
          conditions associated with DSL lines."
      ::= { xdsl2Groups 36 }
   xdsl2StatusChangeNotificationGroup NOTIFICATION-GROUP
      NOTIFICATIONS
      {
      xdsl2LineStatusChangeXtuc,
      xdsl2LineStatusChangeXtur
      }
      STATUS      current
      DESCRIPTION
         "This group supports notifications of thresholds crossing
          associated with DSL lines."
      ::= { xdsl2Groups 37 }
END
4.  Implementation Analysis
   A management application intended to manage ADSL links (e.g.,
   G.992.1) with this MIB module MUST be modified to adapt itself to
   certain differences between RFC 2662 [RFC2662] and this MIB module,
   including the following aspects:
   o  Though the configuration templates/profiles allow referring to 1-4
      bearer channels, ADSL links are limited to 2 channels at most
   o  Though the channel configuration profile allows higher data rates,
      ADSL links are limited to downstream/upstream data rate as assumed
      in RFC 2662 [RFC2662]
   o  The Impulse Noise Protection (INP) configuration parameters are
      given by minimum protection and maximum delay parameters.
   o  The line configuration profile includes a sub-table that addresses
      mode-specific parameters.  For ADSL links, the management
      application SHOULD create a row in that table for the ADSL modes
      only.
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   o  The line configuration profile includes parameters that are
      irrelevant for ADSL links.  Similarly, many status parameters in
      the MIB are irrelevant for certain ADSL modes.  Therefore, it is
      advised to consult with ITU G.997.1 standard [G.997.1] regarding
      the scope and relevance of each parameter in this MIB.
5.  Security Considerations
   There are a number of management objects defined in this MIB module
   with a MAX-ACCESS clause of read-write and/or read-create.  Such
   objects may be considered sensitive or vulnerable in some network
   environments.  The support for SET operations in a non- secure
   environment without proper protection can have a negative effect on
   network operations.  These are the tables and objects and their
   sensitivity/vulnerability:
   o  xdsl2LineTable
      The table consists of the following objects that support SET
      operations:
      *  xdsl2LineCnfgTemplate
      *  xdsl2LineCnfgFallbackTemplate
      *  xdsl2LineAlarmCnfgTemplate
      *  xdsl2LineCmndConfPmsf
      *  xdsl2LineCmndConfLdsf
      *  xdsl2LineCmndConfBpsc
      *  xdsl2LineCmndAutomodeColdStart
      *  xdsl2LineCmndConfReset
      Unauthorized changes to xdsl2LineCnfgTemplate could have a major
      adverse operational effect on many lines simultaneously.
      Unauthorized changes to xdsl2LineCnfgFallbackTemplate could have a
      major adverse operational effect on many lines simultaneously.
      Unauthorized changes to xdsl2LineAlarmCnfgTemplate could have a
      contrary effect on notifications.
      Unauthorized changes to xdsl2LineCmndConfPmsf could have an
      adverse affect on the power consumption of a line and may disrupt
      an operational service.
      Unauthorized changes to xdsl2LineCmndConfLdsf could cause an
      unscheduled line test to be carried out on the line.
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      Unauthorized changes to xdsl2LineCmndConfBpsc could cause an
      unscheduled bits per subcarrier measurement to be carried out on
      the line.
      Unauthorized changes to xdsl2LineCmndAutomodeColdStart could cause
      an unscheduled cold reset to the line.
      Unauthorized changes to xdsl2LineCmndConfReset could cause a
      unscheduled retrain of a line.
   o  xdsl2LineSegmentTable
      This table contains one object, xdsl2LineSegmentRowStatus, that
      supports SET operations.  Unauthorized changes could result in
      measurement results being deleted prematurely.
   o  xdsl2SCStatusTable
      This table contains one object, xdsl2SCStatusRowStatus, that
      supports SET operations.  Unauthorized changes could result in
      line test results being deleted prematurely.
   o  xdsl2LineConfTemplateTable
      The table consists of the following objects that support SET
      operations:
      *  xdsl2LConfTempLineProfile
      *  xdsl2LConfTempChan1ConfProfile
      *  xdsl2LConfTempChan1RaRatioDs
      *  xdsl2LConfTempChan1RaRatioUs
      *  xdsl2LConfTempChan2ConfProfile
      *  xdsl2LConfTempChan2RaRatioDs
      *  xdsl2LConfTempChan2RaRatioUs
      *  xdsl2LConfTempChan3ConfProfile
      *  xdsl2LConfTempChan3RaRatioDs
      *  xdsl2LConfTempChan3RaRatioUs
      *  xdsl2LConfTempChan4ConfProfile
      *  xdsl2LConfTempChan4RaRatioDs
      *  xdsl2LConfTempChan4RaRatioUs
      *  xdsl2LConfTempRowStatus
      Unauthorized changes to xdsl2LConfTempLineProfile,
      xdsl2LConfTempChan1ConfProfile, xdsl2LConfTempChan2ConfProfile,
      xdsl2LConfTempChan3ConfProfile, or xdsl2LConfTempChan4ConfProfile
      could have an adverse operational effect on several lines; could
      change several lines over to running in unwanted levels of
      operation; or could result in several services undergoing changes
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      in the number of channels that carry the service.
      Unauthorized changes to xdsl2LConfTempChan1RaRatioDs,
      xdsl2LConfTempChan2RaRatioDs, xdsl2LConfTempChan3RaRatioDs, or
      xdsl2LConfTempChan4RaRatioDs, would alter the relative rate
      allocations among all channels belonging to a line.  This could
      have an adverse operational effect on several lines.
      Unauthorized changes to xdsl2LConfTempRowStatus could result in
      templates being created or brought into service prematurely; or
      could result in templates being inadvertently deleted or taken out
      of service.
   o  xdsl2LineConfProfTable
      The table consists of the following objects that support SET
      operations:
      *  xdsl2LConfProfScMaskDs
      *  xdsl2LConfProfScMaskUs
      *  xdsl2LConfProfRfiBandsDs
      *  xdsl2LConfProfRaModeDs
      *  xdsl2LConfProfRaModeUs
      *  xdsl2LConfProfRaUsNrmDs
      *  xdsl2LConfProfRaUsNrmUs
      *  xdsl2LConfProfRaUsTimeDs
      *  xdsl2LConfProfRaUsTimeUs
      *  xdsl2LConfProfRaDsNrmDs
      *  xdsl2LConfProfRaDsNrmUs
      *  xdsl2LConfProfRaDsTimeDs
      *  xdsl2LConfProfRaDsTimeUs
      *  xdsl2LConfProfTargetSnrmDs
      *  xdsl2LConfProfTargetSnrmUs
      *  xdsl2LConfProfMaxSnrmDs
      *  xdsl2LConfProfMaxSnrmUs
      *  xdsl2LConfProfMinSnrmDs
      *  xdsl2LConfProfMinSnrmUs
      *  xdsl2LConfProfMsgMinUs
      *  xdsl2LConfProfMsgMinDs
      *  xdsl2LConfProfCeFlag
      *  xdsl2LConfProfSnrModeDs
      *  xdsl2LConfProfSnrModeUs
      *  xdsl2LConfProfTxRefVnDs
      *  xdsl2LConfProfTxRefVnUs
      *  xdsl2LConfProfXtuTransSysEna
      *  xdsl2LConfProfPmMode
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      *  xdsl2LConfProfL0Time
      *  xdsl2LConfProfL2Time
      *  xdsl2LConfProfL2Atpr
      *  xdsl2LConfProfL2Atprt
      *  xdsl2LConfProfProfiles
      *  xdsl2LConfProfDpboEPsd
      *  xdsl2LConfProfDpboEsEL
      *  xdsl2LConfProfDpboEsCableModelA
      *  xdsl2LConfProfDpboEsCableModelB
      *  xdsl2LConfProfDpboEsCableModelC
      *  xdsl2LConfProfDpboMus
      *  xdsl2LConfProfDpboFMin
      *  xdsl2LConfProfDpboFMax
      *  xdsl2LConfProfUpboKL
      *  xdsl2LConfProfUpboKLF
      *  xdsl2LConfProfUs0Mask
      *  xdsl2LConfProfForceInp
      *  xdsl2LConfProfRowStatus
      Unauthorized changes resulting in the setting of any of the above
      objects to an incorrect value could have an adverse operational
      effect on several lines.
      Also, unauthorized changes to xdsl2LConfProfRowStatus could result
      in unwanted line profiles being created or brought into service
      prematurely; or could result in line profiles being inadvertently
      deleted or taken out of service.
   o  xdsl2LineConfProfModeSpecTable
      The table consists of the following objects that support SET
      operations:
      *  xdsl2LConfProfMaxNomPsdDs
      *  xdsl2LConfProfMaxNomPsdUs
      *  xdsl2LConfProfMaxNomAtpDs
      *  xdsl2LConfProfMaxNomAtpUs
      *  xdsl2LConfProfMaxAggRxPwrUs
      *  xdsl2LConfProfPsdMaskDs
      *  xdsl2LConfProfPsdMaskUs
      *  xdsl2LConfProfPsdMaskSelectUs
      *  xdsl2LConfProfClassMask
      *  xdsl2LConfProfLimitMask
      *  xdsl2LConfProfUs0Disable
      *  xdsl2LConfProfModeSpecRowStatus
      Unauthorized changes resulting in the setting of any of the above
      objects to an incorrect value could have an adverse operational
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      effect on several lines.
      Also, unauthorized changes to xdsl2LConfProfModeSpecRowStatus
      could result in unwanted PSD configurations being created or
      brought into service prematurely; or could result in PSD
      configurations being inadvertently deleted or taken out of
      service.
   o  xdsl2LineConfProfModeSpecBandUsTable
      The table consists of the following objects that support SET
      operations:
      *  xdsl2LConfProfUpboPsdA
      *  xdsl2LConfProfUpboPsdB
      *  xdsl2LConfProfModeSpecRowStatus
      Unauthorized changes resulting in the setting of any of the above
      objects to an incorrect value could have an adverse operational
      effect on several lines.
      Also, unauthorized changes to
      xdsl2LConfProfModeSpecBandUsRowStatus could result in unwanted PSD
      configurations being created or brought into service prematurely;
      or could result in PSD configurations being inadvertently deleted
      or taken out of service.
   o  xdsl2ChConfProfileTable
      The table consists of the following objects that support SET
      operations:
      *  xdsl2ChConfProfMinDataRateDs
      *  xdsl2ChConfProfMinDataRateUs
      *  xdsl2ChConfProfMinResDataRateDs
      *  xdsl2ChConfProfMinResDataRateUs
      *  xdsl2ChConfProfMaxDataRateDs
      *  xdsl2ChConfProfMaxDataRateUs
      *  xdsl2ChConfProfMinDataRateLowPwrDs
      *  xdsl2ChConfProfMinDataRateLowPwrUs
      *  xdsl2ChConfProfMaxDelayDs
      *  xdsl2ChConfProfMaxDelayUs
      *  xdsl2ChConfProfMinProtectionDs
      *  xdsl2ChConfProfMinProtectionUs
      *  xdsl2ChConfProfMinProtection8Ds
      *  xdsl2ChConfProfMinProtection8Us
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      *  xdsl2ChConfProfMaxBerDs
      *  xdsl2ChConfProfMaxBerUs
      *  xdsl2ChConfProfUsDataRateDs
      *  xdsl2ChConfProfDsDataRateDs
      *  xdsl2ChConfProfUsDataRateUs
      *  xdsl2ChConfProfDsDataRateUs
      *  xdsl2ChConfProfImaEnabled
      *  xdsl2ChConfProfMaxDelayVar
      *  xdsl2ChConfProfInitPolicy
      *  xdsl2ChConfProfRowStatus
      Unauthorized changes resulting in the setting of any of the above
      objects to an incorrect value could have an adverse operational
      effect on several lines.
      Also, unauthorized changes to xdsl2ChConfProfRowStatus could
      result in unwanted channel profiles being created or brought into
      service prematurely; or could result in channel profiles being
      inadvertently deleted or taken out of service.
   o  xdsl2LineAlarmConfTemplateTable
      The table consists of the following objects that support SET
      operations:
      *  xdsl2LAlarmConfTempLineProfile
      *  xdsl2LAlarmConfTempChan1ConfProfile
      *  xdsl2LalarmConfTempChan2ConfProfile
      *  xdsl2LalarmConfTempChan3ConfProfile
      *  xdsl2LalarmConfTempChan4ConfProfile
      *  xdsl2LAlarmConfTempRowStatus
      Unauthorized changes to xdsl2LAlarmConfTempLineProfile,
      xdsl2LAlarmConfTempChan1ConfProfile,
      xdsl2LAlarmConfTempChan2ConfProfile,
      xdsl2LAlarmConfTempChan3ConfProfile, or
      xdsl2LAlarmConfTempChan4ConfProfile could have an adverse effect
      on the management of notifications generated at the scope of
      several to many lines; or could change several to many lines over
      to running with unwanted management rates for generated
      notifications.
      Unauthorized changes to xdsl2LAlarmConfTempRowStatus could result
      in alarm templates being created or brought into service
      prematurely; or could result in alarm templates being
      inadvertently deleted or taken out of service.
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   o  xdsl2LineAlarmConfProfileTable
      The table consists of the following objects that support SET
      operations:
      *  xdsl2LineAlarmConfProfileXtucThresh15MinFecs
      *  xdsl2LineAlarmConfProfileXtucThresh15MinEs
      *  xdsl2LineAlarmConfProfileXtucThresh15MinSes
      *  xdsl2LineAlarmConfProfileXtucThresh15MinLoss
      *  xdsl2LineAlarmConfProfileXtucThresh15MinUas
      *  xdsl2LineAlarmConfProfileXturThresh15MinFecs
      *  xdsl2LineAlarmConfProfileXturThresh15MinEs
      *  xdsl2LineAlarmConfProfileXturThresh15MinSes
      *  xdsl2LineAlarmConfProfileXturThresh15MinLoss
      *  xdsl2LineAlarmConfProfileXturThresh15MinUas
      *  xdsl2LineAlarmConfProfileThresh15MinFailedFullInt
      *  xdsl2LineAlarmConfProfileThresh15MinFailedShrtInt
      *  xdsl2LineAlarmConfProfileRowStatus
      Increasing any of the threshold values could result in a
      notification being suppressed or deferred.  Setting a threshold to
      0 could result in a notification being suppressed.  Suppressing or
      deferring a notification could prevent the timely delivery of
      important diagnostic information.  Decreasing any of the threshold
      values could result in a notification being sent from the network
      falsely reporting a threshold crossing.
      Changing a threshold value could also have an impact on the amount
      of notifications the agent sends.  The Notifications Section of
      this document has a paragraph which provides general guidance on
      the rate-limiting of notifications.  Agent implementations not
      providing rate-limiting could result in notifications being
      generated at an uncontrolled rate.  Unauthorized changes to a
      threshold value could result in an undesired notification rate.
      Unauthorized changes to row status could result in unwanted line
      alarm profiles being created or brought into service.  Also,
      changes to the row status could result in line alarm profiles
      being inadvertently deleted or taken out of service.
   o  xdsl2ChAlarmConfProfileTable
      The table consists of the following objects that support SET
      operations:
      *  xdsl2ChAlarmConfProfileXtucThresh15MinCodingViol ations
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      *  xdsl2ChAlarmConfProfileXtucThresh15MinCorrected
      *  xdsl2ChAlarmConfProfileXturThresh15MinCodingViol ations
      *  xdsl2ChAlarmConfProfileXturThresh15MinCorrected
      *  xdsl2ChAlarmConfProfileRowStatus
      *  xdsl2LineAlarmConfProfileXturThresh15MinFecs
      *  xdsl2LineAlarmConfProfileXturThresh15MinEs
      *  xdsl2LineAlarmConfProfileXturThresh15MinSes
      *  xdsl2LineAlarmConfProfileXturThresh15MinLoss
      *  xdsl2LineAlarmConfProfileXturThresh15MinUas
      *  xdsl2LineAlarmConfProfileThresh15MinFailedFullInt
      *  xdsl2LineAlarmConfProfileThresh15MinFailedShrtInt
      *  xdsl2LineAlarmConfProfileRowStatus
      Increasing any of the threshold values could result in a
      notification being suppressed or deferred.  Setting a threshold to
      0 could result in a notification being suppressed.  Suppressing or
      deferring a notification could prevent the timely delivery of
      important diagnostic information.  Decreasing any of the threshold
      values could result in a notification being sent from the network
      falsely reporting a threshold crossing.
      Changing a threshold value could also have an impact on the amount
      of notifications the agent sends.  The Notifications Section of
      this document has a paragraph which provides general guidance on
      the rate-limiting of notifications.  Agent implementations not
      providing rate-limiting could result in notifications being
      generated at an uncontrolled rate.  Unauthorized changes to a
      threshold value could result in an undesired notification rate.
      Unauthorized changes to row status could result in unwanted
      channel alarm profiles being created or brought into service.
      Also, changes to the row status could result in channel alarm
      profiles being inadvertently deleted or taken out of service.
   Some of the readable objects in this MIB module (i.e., objects with a
   MAX-ACCESS other than not-accessible) may be considered sensitive or
   vulnerable in some network environments.  It is thus important to
   control even GET and/or NOTIFY access to these objects and possibly
   to even encrypt the values of these objects when sending them over
   the network via SNMP.  These are the tables and objects and their
   sensitivity/vulnerability:
   o  xdsl2LineInventoryTable
      Access to these objects would allow an intruder to obtain
      information about which vendor's equipment is in use on the
      network.  Further, such information is considered sensitive in
      many environments for competitive reasons.
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      *  xdsl2LInvG994VendorId
      *  xdsl2LInvSystemVendorId
      *  xdsl2LInvVersionNumber
      *  xdsl2LInvSerialNumber
      *  xdsl2LInvSelfTestResult
      *  xdsl2LInvTransmissionCapabilities
   SNMP versions prior to SNMPv3 did not include adequate security.
   Even if the network itself is secure (for example by using IPSec),
   even then, there is no control as to who on the secure network is
   allowed to access and GET/SET (read/change/create/delete) the objects
   in this MIB module.
   It is RECOMMENDED that implementers consider the security features as
   provided by the SNMPv3 framework (see [RFC3410], Section 8),
   including full support for the SNMPv3 cryptographic mechanisms (for
   authentication and privacy).
   It is RECOMMENDED to deploy SNMPv3 and to enable cryptographic
   security.  It is then a customer/operator responsibility to ensure
   that the SNMP entity giving access to an instance of this MIB module
   is properly configured to give access only to those objects whose
   principals (users) have legitimate rights to indeed GET or SET
   (change/create/delete) them.
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