vdslOtPhysCurrSnrMgn METANOIA 0 # Current UpStream Snr Mgn # 1
vdslOtPhysCurrLineRate METANOIA 0 # Current UpStream linerate # 1
vdslRtPhysCurrSnrMgn METANOIA 0 # Current DownStream Snr Mgn # 1
vdslRtPhysCurrLineRate METANOIA 0 # Current DownStream linerate # 1
vdslOtIntlvChanBadBlks METANOIA 0 # CRC counter # 1
vdslRtIntlvChanBadBlks METANOIA 0 # CRC counter # 1
vdslLineConfDownTargetSnrMgn METANOIA 0 # target DownStream Snr Mgn # 1
vdslLineConfUpTargetSnrMgn METANOIA 0 # target UpStream Snr Mgn # 1
vdslLineConfDownSlowMaxDataRate METANOIA 0 # DownStream Rate Limit # 1
vdslLineConfUpSlowMaxDataRate METANOIA 0 # UpStream Rate Limit # 1
vdslLineConfDownMaxInterDelay METANOIA 0 # DownStream Max network delay (0.5 ms) # 1
vdslLineConfUpMaxInterDelay METANOIA 0 # UpStream Max network delay(0.5 ms)  # 1
vdslLineConfDownTargetSlowBurst METANOIA 0 # DownStream IMP (us) # 1
vdslLineConfUpTargetSlowBurst METANOIA 0 # UpStream IMP (us) # 1
vdslFirmwareVer METANOIA 2 # # 1
vdslFirmwareDate METANOIA 2 # # 1
vdslFirmwareTime METANOIA 2 # # 1
vdslOtFirmwareVer METANOIA 2 # # 1
vdslOtFirmwareDate METANOIA 2 # # 1
vdslOtFirmwareTime METANOIA 2 # # 1
vdslRtFirmwareVer METANOIA 2 # # 1
vdslRtFirmwareDate METANOIA 2 # # 1
vdslRtFirmwareTime METANOIA 2 # # 1
vdslOtPerfDataInits METANOIA 0 # connection success counter # 1
vdslRtPerfDataInits METANOIA 0 # connection success counter # 1
MutRxFlushCntr ADVANCE 0 # Flush counter when packet buffer over flow # 1
vdslRtIntlvChanFixedOctets METANOIA 0 # error correct byte # 1
vdslOtIntlvChanFixedOctets METANOIA 0 # error correct byte # 1
vdslOtIntlvChanInterleaveDelay METANOIA 0 # interleave delay of downstream ( ms ) # 1
vdslOtIntlvChanCurrTxRate METANOIA 0 # unit of kbps, net data rate of downstream # 1
vdslOtIntlvChanCurrTxSlowBurstProtect ADVANCE 0 # unit of us, impulse noise protect of downstream, ~InterleaveDelay*(R/2N),R=16,N=160 # 1
xvdslMetanoiaDsDataRatio ADVANCE 0 # unit of %, ~DataRate/LineRata # 1
vdslRtIntlvChanInterleaveDelay METANOIA 0 #  interleave delay of upstream (ms) # 1
vdslRtIntlvChanCurrTxRate METANOIA 0 # unit of kbps, net data rate of upstream # 1
vdslRtIntlvChanCurrTxSlowBurstProtect ADVANCE 0 #  unit of us, impulse noise protect of upstream, ~InterleaveDelay*(R/2N),R=16,N=160 # 1
vdslMetanoiaUsDataRatio ADVANCE 0 # unit of %, ~DataRate/LineRata # 1
vdslRtPerfDataESs ADVANCE 0 # DownStream Error second # 1
vdslOtPerfDataESs ADVANCE 0 # UpStream Error second # 1
BinSelect ADVANCE 0 # # 1
CfgUsPbs BANDPLAN 0 # # 1
vdslLineMCMConfProfileRxBandStart1 BANDPLAN 0 # # 1
vdslLineMCMConfProfileRxBandStop1 BANDPLAN 0 # # 1
vdslLineMCMConfProfileRxBandStart2 BANDPLAN 0 # # 1
vdslLineMCMConfProfileRxBandStop2 BANDPLAN 0 # # 1
vdslLineMCMConfProfileRxBandStart3 BANDPLAN 0 # # 1
vdslLineMCMConfProfileRxBandStop3 BANDPLAN 0 # # 1
vdslLineMCMConfProfileRxBandStart4 BANDPLAN 0 # # 1
vdslLineMCMConfProfileRxBandStop4 BANDPLAN 0 # # 1
CfgUsPb4FirstTone BANDPLAN 0 # # 1
CfgUsPb4LastTone BANDPLAN 0 # # 1
CfgDsPbs BANDPLAN 0 # # 1
vdslLineMCMConfProfileTxBandStart1 BANDPLAN 0 # # 1
vdslLineMCMConfProfileTxBandStop1 BANDPLAN 0 # # 1
vdslLineMCMConfProfileTxBandStart2 BANDPLAN 0 # # 1
vdslLineMCMConfProfileTxBandStop2 BANDPLAN 0 # # 1
vdslLineMCMConfProfileTxBandStart3 BANDPLAN 0 # # 1
vdslLineMCMConfProfileTxBandStop3 BANDPLAN 0 # # 1
vdslLineMCMConfProfileTxBandStart4 BANDPLAN 0 # # 1
vdslLineMCMConfProfileTxBandStop4 BANDPLAN 0 # # 1
CfgDsPb4FirstTone BANDPLAN 0 # # 1
CfgDsPb4LastTone BANDPLAN 0 # # 1
ModemStatus ADVANCE 2 #
vdslLineDiagInit DEBUG 2 #
vdslLineDiagInitD DEBUG 2 # # 1
vdslLineDiagInitDD DEBUG 2 # # 1
vdslLineDiagTrn DEBUG 2 # # 1
vdslLineDiagTrnD DEBUG 2 # # 1
vdslLineDiagTrnDD DEBUG 2 # # 1
vdslLineDiagSt DEBUG 2 # # 1
vdslLineDiagStD DEBUG 2 # # 1
vdslLineDiagStDD DEBUG 2 # # 1
vdslLineDiagSt2 DEBUG 2 # # 1
vdslLineDiagSt2D DEBUG 2 # # 1
vdslLineDiagSt2DD DEBUG 2 # # 1
VdslLineFgndCntr DEBUG 2 # # 1
vdslLineTime250ms DEBUG 2 # # 1
vdslLineTime250msD DEBUG 2 # # 1
vdslLineTime250msDD DEBUG 2 # # 1
DRS_N ADVANCE 0 # codeword size of RS, suggest not change, capability<=255 # 1
DRS_R ADVANCE 0 # redundancy size of RS, suggest not change, capability=0,2,4,6,8,10,12,14 and 16 # 1
vdslVcxoValue ADVANCE 2 # clock setting reference # 1
vdslMetanoiaRtVcxo ADVANCE 2 # RT clock setting reference # 1
VcxoValue ADVANCE 2 # # 1
ElectricLen ADVANCE 0 # estimated line length # 1
RxPktCntr ADVANCE 0 # # 1
TxPktCntr ADVANCE 0 # # 1
vdslLinePauseFrmCntr ADVANCE 0 # 802.3 pause frame counter # 1
nO_DsFastPathRate ADVANCE 0 # Data rate ( unit is 64 kbps ) # 1
nO_UsFastPathRate ADVANCE 0 # Data rate ( unit is 64 kbps ) # 1
vdslTwConfig METANOIA 2 # bit 4: report packet activities in LED 0 # 1
SecondCnt ADVANCE 0 # when showtime, the value is seconds from showtime start # 1
SecondIntlvCntST ADVANCE 0 # total seconds of showtime # 1
DrsCwHistAccCorr ADVANCE 0 # success error correction count # 1
DrsCwHistAccUnCorr ADVANCE 0 # fail error correction count # 1
AocMinBin1Index ADVANCE 0 # minmal snr Bin # 1
AocMinBin2Index ADVANCE 0 # second minmal snr Bin # 1
AocMinMarg1 ADVANCE 0 # minmal snr Bin's snr # 1
AocMinMarg2 ADVANCE 0 # second minmal snr Bin's snr # 1
CfgBandPlan BANDPLAN 0 # # 1


