# print type:1=>dec type:2=>hex  3=>binary
######OT Setting###########
OT vdslOtPhysCurrLineRate 1
OT vdslRtPhysCurrLineRate 1
OT SystemFlag4 2
OT SystemFlagStk 2
OT RxPgaSelect 2
OT ElectricLen 2
OT vdslLineDiagInit 3
OT vdslLineDiagTrn 3
OT vdslLineDiagSt2 3
OT vdslLineDiagSt 3
OT vdslTerminal 3
OT ModemStatus 3
OT DebugFlag 3
######RT Setting###########
RT vdslOtPhysCurrLineRate 1
RT vdslRtPhysCurrLineRate 1
RT SystemFlag4 2
RT SystemFlagStk 2
RT RxPgaSelect 2
RT ElectricLen 2
RT vdslTerminal 3
RT vdslLineDiagInit 3
RT vdslLineDiagTrn 3
RT vdslLineDiagSt2 3
RT vdslLineDiagSt 3
RT ModemStatus 3
RT DebugFlag 3
RT vdslVcxoValue 2
