VDSL2 SOC message parser/interpreter v0.2
(c) 2008 Metanoia Communications Inc.

1024 bytes read

##################################################################################
 GHS Rx frame found at index 0, frame size 1
##################################################################################
 Frame #1
Frame data:
Decoding G.HS KICK message
This is a virtual received message, please ignore this!

Decoding G.HS message MS
GHS version: 0
Message segment index 0

Segmented messages are all parsed

##################################################################################
 GHS Tx frame found at index 1, frame size 56
##################################################################################
 Frame #2
Frame data:
03    01    B5    00    4D    45    54    41    
00    00    C0    80    84    00    00    00    
00    A0    40    31    43    3F    43    4D    
08    00    40    3F    0F    00    00    43    
07    C3    02    07    B5    00    4D    45    
54    41    01    0A    B5    00    4D    45    
54    41    00    00    00    3A    89    54    

Decoding G.HS message CLR
GHS version: 1
Country code: b500, Vendor ID: META, Vendor-specific info: 0000
Message segment index 0

c0
Identification NPar1 descriptions:
	Non-standard field

80
Identification SPar1 descriptions:
		No information in octet 1

Identification ends
84
Standard NPar1 descriptions:
	Silent period (Note 2)

00 00 00 00 a0
Standard SPar1 descriptions:
		No information in octet 1
		No information in octet 2
		No information in octet 3
		No information in octet 4
	G.993.2

SPar1 G.993.2
40
Standard NPar2 descriptions:
		No information in octet 1


31 43
SPar1 G.993.2
SPar2 active settings:
	Profiles
	Initial IDFT size (2N)
	CE Lengths
	Annex A US0
	Annex B US0

G.993.2 --> Profiles:  3f 43
	8a
	8b
	8c
	8d
	12a
	12b
	17a
	30a



G.993.2 --> Initial IDFT size (2N):  4d
	IDFT size 2N = 8192

G.993.2 --> CE Lengths:  08 00 40
	Length of CE (m = 5)
		No information in octet 2
		No information in octet 3


G.993.2 --> Annex A US0:  3f 0f 00 00 43
	EU-32
	EU-36
	EU-40
	EU-44
	EU-48
	EU-52
	EU-56
	EU-60
	EU-64
	EU-128
		No information in octet 3
		No information in octet 4
	US0 supported in profile 12b
	US0 supported in profile 17a


G.993.2 --> Annex B US0:  07 c3
	25-138 kHz (A)
	25-276 kHz (M)
	120-276 kHz (B)
	US0 supported in profile 12b
	US0 supported in profile 17a


Standard ends
Number of NS blocks: 2 

NS block #1 length 7

b5  00  4d  45  54  41  01  

NS block #2 length 10

b5  00  4d  45  54  41  00  00  00  3a  

Nonstandard info ends

Segmented messages are all parsed

##################################################################################
 GHS Rx frame found at index 59, frame size 61
##################################################################################
 Frame #3
Frame data:
02    01    B5    00    42    44    43    4D    
93    BD    80    80    84    00    00    00    
00    A0    56    17    41    3F    41    00    
12    2C    00    0D    30    00    2A    3F    
00    1E    7D    00    0D    1B    00    00    
21    00    1E    29    00    13    00    00    
3D    22    00    2B    69    4D    01    00    
00    00    C3    88    7D    
Decoding G.HS message CL
GHS version: 1
Country code: b500, Vendor ID: BDCM, Vendor-specific info: 93bd
Message segment index 0

80
Identification NPar1 descriptions:
		No information in octet 1

80
Identification SPar1 descriptions:
		No information in octet 1

Identification ends
84
Standard NPar1 descriptions:
	Silent period (Note 2)

00 00 00 00 a0
Standard SPar1 descriptions:
		No information in octet 1
		No information in octet 2
		No information in octet 3
		No information in octet 4
	G.993.2

SPar1 G.993.2
56
Standard NPar2 descriptions:
	Support of Downstream virtual noise
	Lineprobe
	Support of PSD shaping in US0


17 41
SPar1 G.993.2
SPar2 active settings:
	Profiles
	Bands Upstream (NOTE 1)
	Bands Downstream (NOTE 1)
	Initial IDFT size (2N)
	Annex A US0

G.993.2 --> Profiles:  3f 41
	8a
	8b
	8c
	8d
	12a
	12b
	17a


G.993.2 --> Bands Upstream (NOTE 1):  00 12 2c 00 0d 30 00 2a 3f 00 1e 7d
	Upstream band 0:  880 to 1196
	Upstream band 1: 1981 to 2751

G.993.2 --> Bands Downstream (NOTE 1):  00 0d 1b 00 00 21 00 1e 29 00 13 00 00 3d 22 00 2b 69
	Downstream band 0:   33 to  859
	Downstream band 1: 1216 to 1961
	Downstream band 2: 2793 to 3938


G.993.2 --> Initial IDFT size (2N):  4d
	IDFT size 2N = 8192

G.993.2 --> Annex A US0:  01 00 00 00 c3
	EU-32
		No information in octet 2
		No information in octet 3
		No information in octet 4
	US0 supported in profile 12b
	US0 supported in profile 17a


Standard ends

Segmented messages are all parsed

##################################################################################
 GHS Tx frame found at index 123, frame size 4
##################################################################################
 Frame #4
Frame data:
10    03    4D    A8    
Decoding G.HS message ACK(1)

##################################################################################
 GHS Rx frame found at index 129, frame size 1
##################################################################################
 Frame #5
Frame data:
Decoding G.HS KICK message
This is a virtual received message, please ignore this!

Decoding G.HS message ACK(1)

##################################################################################
 GHS Tx frame found at index 130, frame size 4
##################################################################################
 Frame #6
Frame data:
01    03    04    24    
Decoding G.HS message MR

##################################################################################
 GHS Rx frame found at index 136, frame size 22
##################################################################################
 Frame #7
Frame data:
00    01    80    80    80    00    00    00    
00    A0    40    01    41    00    41    01    
00    00    00    C0    20    DD    
Decoding G.HS message MS
GHS version: 1
Message segment index 0

80
Identification NPar1 descriptions:
		No information in octet 1

80
Identification SPar1 descriptions:
		No information in octet 1

Identification ends
80
Standard NPar1 descriptions:
		No information in octet 1

00 00 00 00 a0
Standard SPar1 descriptions:
		No information in octet 1
		No information in octet 2
		No information in octet 3
		No information in octet 4
	G.993.2

SPar1 G.993.2
40
Standard NPar2 descriptions:
		No information in octet 1


01 41
SPar1 G.993.2
SPar2 active settings:
	Profiles
	Annex A US0

G.993.2 --> Profiles:  00 41
		No information in octet 1
	17a


G.993.2 --> Annex A US0:  01 00 00 00 c0
	EU-32
		No information in octet 2
		No information in octet 3
		No information in octet 4
		No information in octet 5


Standard ends

Segmented messages are all parsed

##################################################################################
 GHS Tx frame found at index 161, frame size 4
##################################################################################
 Frame #8
Frame data:
10    03    4D    A8    
Decoding G.HS message ACK(1)

##################################################################################
 Rx frame found at index 167, frame size 183
##################################################################################
 Frame #9
Frame data:
01    11    01    03    35    B0    21    7A    
94    C0    F6    2A    E9    03    02    00    
07    4A    C3    70    AB    F7    BD    14    
1B    30    01    1B    30    20    35    70    
21    40    B0    41    40    B1    00    3A    
71    78    39    82    00    38    73    33    
35    53    5B    1B    33    5C    1B    34    
BF    35    F4    C0    37    54    DD    37    
57    A9    1B    37    AA    1B    3A    E8    
34    3A    E9    34    3F    62    1B    3F    
63    1B    3F    FF    0E    1B    30    01    
1B    30    06    41    F0    07    41    F0    
20    1B    30    21    1B    33    6F    39    
33    70    39    34    AC    1B    34    AD    
1B    37    BC    38    47    BD    38    4A    
BF    1B    3A    C0    1B    3F    FF    09    
33    40    21    35    B0    28    35    B3    
39    33    23    5B    33    C4    C0    35    
24    DD    35    27    A9    32    0A    E9    
32    0F    62    01    FA    00    91    02    
00    07    D0    00    07    D0    30    D6    
FF    FF    00    3C    80    01    00    01    
0A    00    00    00    94    A0    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 01,Message type:  01
Decoding O-Signature
Message segmantation:  1/ 1
Supported sub-carriers in DS(# of Bands descriptor): 3
	Band # 1, Start   33, End  859
	Band # 2, Start 1216, End 1961
	Band # 3, Start 2793, End 3938

Supported sub-carriers in US(# of bands descriptor): 3
	Band # 1, Start    7, End   32
	Band # 2, Start  880, End 1196
	Band # 3, Start 1981, End 2751

Downstream transmit PSD mask (# of breakpoint being described): 20
	Break point # 1, bin:    1, Level: -96.50 dBm/Hz
	Break point # 2, bin:   32, Level: -96.50 dBm/Hz
	Break point # 3, bin:   33, Level: -54.50 dBm/Hz
	Break point # 4, bin:   65, Level: -36.50 dBm/Hz
	Break point # 5, bin:  256, Level: -36.50 dBm/Hz
	Break point # 6, bin:  376, Level: -46.50 dBm/Hz
	Break point # 7, bin:  512, Level: -48.00 dBm/Hz
	Break point # 8, bin:  819, Level: -49.70 dBm/Hz
	Break point # 9, bin:  859, Level: -54.70 dBm/Hz
	Break point #10, bin:  860, Level: -96.50 dBm/Hz
	Break point #11, bin: 1215, Level: -96.50 dBm/Hz
	Break point #12, bin: 1216, Level: -53.70 dBm/Hz
	Break point #13, bin: 1245, Level: -51.50 dBm/Hz
	Break point #14, bin: 1961, Level: -51.50 dBm/Hz
	Break point #15, bin: 1962, Level: -96.50 dBm/Hz
	Break point #16, bin: 2792, Level: -96.50 dBm/Hz
	Break point #17, bin: 2793, Level: -56.50 dBm/Hz
	Break point #18, bin: 3938, Level: -56.50 dBm/Hz
	Break point #19, bin: 3939, Level: -96.50 dBm/Hz
	Break point #20, bin: 4095, Level: -96.50 dBm/Hz

Upstream transmit PSD mask (# of breakpoint being described): 14
	Break point # 1, bin:    1, Level: -96.50 dBm/Hz
	Break point # 2, bin:    6, Level: -96.50 dBm/Hz
	Break point # 3, bin:    7, Level: -34.50 dBm/Hz
	Break point # 4, bin:   32, Level: -34.50 dBm/Hz
	Break point # 5, bin:   33, Level: -96.50 dBm/Hz
	Break point # 6, bin:  879, Level: -96.50 dBm/Hz
	Break point # 7, bin:  880, Level: -48.50 dBm/Hz
	Break point # 8, bin: 1196, Level: -48.50 dBm/Hz
	Break point # 9, bin: 1197, Level: -96.50 dBm/Hz
	Break point #10, bin: 1980, Level: -96.50 dBm/Hz
	Break point #11, bin: 1981, Level: -50.00 dBm/Hz
	Break point #12, bin: 2751, Level: -50.00 dBm/Hz
	Break point #13, bin: 2752, Level: -96.50 dBm/Hz
	Break point #14, bin: 4095, Level: -96.50 dBm/Hz

Channel discovery downstream PSD (# of breakpoint being described): 9
	Break point # 1, bin:   33, Level: -58.00 dBm/Hz
	Break point # 2, bin:   40, Level: -54.10 dBm/Hz
	Break point # 3, bin:  825, Level: -54.10 dBm/Hz
	Break point # 4, bin:  859, Level: -58.20 dBm/Hz
	Break point # 5, bin: 1216, Level: -57.20 dBm/Hz
	Break point # 6, bin: 1245, Level: -55.00 dBm/Hz
	Break point # 7, bin: 1961, Level: -55.00 dBm/Hz
	Break point # 8, bin: 2793, Level: -60.00 dBm/Hz
	Break point # 9, bin: 3938, Level: -60.00 dBm/Hz

Initial Downstream PSD ceiling: -50.60 dBm/Hz
Downstream nominal maximum aggregate transmit power: 14.50 dBm

Parameters fo UPBO reference PSD (# of US bands): 2
	US1, value of a': 60.00, value of b': 0.00
	US2, value of a': 60.00, value of b': 0.00

Maximum target total data rate: 100016 kbps
Downstream maximum SNR margin: 6553.50 dB
Downstream target SNR margin: 6.00 dB
Downstream transmit window length:  128
Downstream cyclic prefix length:  256
Initial value of timing advance (0x7FFF means VTU-R decides): 0x010A

Downstream transmitter referred virtual noise PSD(# of breakpoints): 0
SNRM_MODE, value:  0, SNRM_MODE selected:  1

Upstream transmitter referred virtual noise PSD(# of breakpoints): 0

##################################################################################
 Rx frame found at index 350, frame size 183
##################################################################################
 Frame #10
Frame data:
01    11    01    03    35    B0    21    7A    
94    C0    F6    2A    E9    03    02    00    
07    4A    C3    70    AB    F7    BD    14    
1B    30    01    1B    30    20    35    70    
21    40    B0    41    40    B1    00    3A    
71    78    39    82    00    38    73    33    
35    53    5B    1B    33    5C    1B    34    
BF    35    F4    C0    37    54    DD    37    
57    A9    1B    37    AA    1B    3A    E8    
34    3A    E9    34    3F    62    1B    3F    
63    1B    3F    FF    0E    1B    30    01    
1B    30    06    41    F0    07    41    F0    
20    1B    30    21    1B    33    6F    39    
33    70    39    34    AC    1B    34    AD    
1B    37    BC    38    47    BD    38    4A    
BF    1B    3A    C0    1B    3F    FF    09    
33    40    21    35    B0    28    35    B3    
39    33    23    5B    33    C4    C0    35    
24    DD    35    27    A9    32    0A    E9    
32    0F    62    01    FA    00    91    02    
00    07    D0    00    07    D0    30    D6    
FF    FF    00    3C    80    01    00    01    
0A    00    00    00    94    A0    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 01,Message type:  01
Decoding O-Signature
Message segmantation:  1/ 1
Supported sub-carriers in DS(# of Bands descriptor): 3
	Band # 1, Start   33, End  859
	Band # 2, Start 1216, End 1961
	Band # 3, Start 2793, End 3938

Supported sub-carriers in US(# of bands descriptor): 3
	Band # 1, Start    7, End   32
	Band # 2, Start  880, End 1196
	Band # 3, Start 1981, End 2751

Downstream transmit PSD mask (# of breakpoint being described): 20
	Break point # 1, bin:    1, Level: -96.50 dBm/Hz
	Break point # 2, bin:   32, Level: -96.50 dBm/Hz
	Break point # 3, bin:   33, Level: -54.50 dBm/Hz
	Break point # 4, bin:   65, Level: -36.50 dBm/Hz
	Break point # 5, bin:  256, Level: -36.50 dBm/Hz
	Break point # 6, bin:  376, Level: -46.50 dBm/Hz
	Break point # 7, bin:  512, Level: -48.00 dBm/Hz
	Break point # 8, bin:  819, Level: -49.70 dBm/Hz
	Break point # 9, bin:  859, Level: -54.70 dBm/Hz
	Break point #10, bin:  860, Level: -96.50 dBm/Hz
	Break point #11, bin: 1215, Level: -96.50 dBm/Hz
	Break point #12, bin: 1216, Level: -53.70 dBm/Hz
	Break point #13, bin: 1245, Level: -51.50 dBm/Hz
	Break point #14, bin: 1961, Level: -51.50 dBm/Hz
	Break point #15, bin: 1962, Level: -96.50 dBm/Hz
	Break point #16, bin: 2792, Level: -96.50 dBm/Hz
	Break point #17, bin: 2793, Level: -56.50 dBm/Hz
	Break point #18, bin: 3938, Level: -56.50 dBm/Hz
	Break point #19, bin: 3939, Level: -96.50 dBm/Hz
	Break point #20, bin: 4095, Level: -96.50 dBm/Hz

Upstream transmit PSD mask (# of breakpoint being described): 14
	Break point # 1, bin:    1, Level: -96.50 dBm/Hz
	Break point # 2, bin:    6, Level: -96.50 dBm/Hz
	Break point # 3, bin:    7, Level: -34.50 dBm/Hz
	Break point # 4, bin:   32, Level: -34.50 dBm/Hz
	Break point # 5, bin:   33, Level: -96.50 dBm/Hz
	Break point # 6, bin:  879, Level: -96.50 dBm/Hz
	Break point # 7, bin:  880, Level: -48.50 dBm/Hz
	Break point # 8, bin: 1196, Level: -48.50 dBm/Hz
	Break point # 9, bin: 1197, Level: -96.50 dBm/Hz
	Break point #10, bin: 1980, Level: -96.50 dBm/Hz
	Break point #11, bin: 1981, Level: -50.00 dBm/Hz
	Break point #12, bin: 2751, Level: -50.00 dBm/Hz
	Break point #13, bin: 2752, Level: -96.50 dBm/Hz
	Break point #14, bin: 4095, Level: -96.50 dBm/Hz

Channel discovery downstream PSD (# of breakpoint being described): 9
	Break point # 1, bin:   33, Level: -58.00 dBm/Hz
	Break point # 2, bin:   40, Level: -54.10 dBm/Hz
	Break point # 3, bin:  825, Level: -54.10 dBm/Hz
	Break point # 4, bin:  859, Level: -58.20 dBm/Hz
	Break point # 5, bin: 1216, Level: -57.20 dBm/Hz
	Break point # 6, bin: 1245, Level: -55.00 dBm/Hz
	Break point # 7, bin: 1961, Level: -55.00 dBm/Hz
	Break point # 8, bin: 2793, Level: -60.00 dBm/Hz
	Break point # 9, bin: 3938, Level: -60.00 dBm/Hz

Initial Downstream PSD ceiling: -50.60 dBm/Hz
Downstream nominal maximum aggregate transmit power: 14.50 dBm

Parameters fo UPBO reference PSD (# of US bands): 2
	US1, value of a': 60.00, value of b': 0.00
	US2, value of a': 60.00, value of b': 0.00

Maximum target total data rate: 100016 kbps
Downstream maximum SNR margin: 6553.50 dB
Downstream target SNR margin: 6.00 dB
Downstream transmit window length:  128
Downstream cyclic prefix length:  256
Initial value of timing advance (0x7FFF means VTU-R decides): 0x010A

Downstream transmitter referred virtual noise PSD(# of breakpoints): 0
SNRM_MODE, value:  0, SNRM_MODE selected:  1

Upstream transmitter referred virtual noise PSD(# of breakpoints): 0

##################################################################################
 Tx frame found at index 533, frame size 39
##################################################################################
 Frame #11
Frame data:
01    11    81    00    00    01    59    06    
32    00    07    32    00    20    34    43    
70    34    84    AC    35    17    BD    35    
AA    BF    01    00    02    00    00    B0    
E0    80    01    80    50    17    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 01,Message type:  81
Decoding R-MSG1
Message segmantation:  1/ 1
Estimated electrical length (in dB at 1MHz): 0.00
Initial Upstream PSD ceiling: -34.50 dBm/Hz

Channel discovery upstream PSD (# of breakpoint being described): 6
	Break point # 1, bin:    7, Level: -60.00 dBm/Hz
	Break point # 2, bin:   32, Level: -60.00 dBm/Hz
	Break point # 3, bin:  880, Level: -56.40 dBm/Hz
	Break point # 4, bin: 1196, Level: -56.00 dBm/Hz
	Break point # 5, bin: 1981, Level: -55.10 dBm/Hz
	Break point # 6, bin: 2751, Level: -54.20 dBm/Hz

Number of pilot tones: 1
	Pilot #1: bin 0
	Pilot #2: bin 512

Timing advance: 176

O-P-PILOT settings: 0xE0
	O-P-PILOT1: on
	O-P-PILOT2: on
	O-P-PILOT3: on

Upstream transmit window length:  128
Upstream cyclic prefix length:  384

##################################################################################
 Rx frame found at index 573, frame size 17
##################################################################################
 Frame #12
Frame data:
02    11    02    00    12    10    00    0A    
BF    03    70    00    FF    44    35    D6    

Escaped bytes:    0, Errored escape bytes:    0
Message index: 02,Message type:  02
Decoding O-Update
Message segmantation:  1/ 1
Final electrical length (in dB at 1MHz): 1.80
Updated upstream PSD ceiling. 0x1000 -->special value  indicates no limit.
Higest allowed upstream sub-carrier: 2751
Lowest allowed upstream sub-carrier: 880
Blackout set of upstream sub-carriers (# of break points): 0
Timing advance correction: -188

##################################################################################
 Tx frame found at index 590, frame size 13
##################################################################################
 Frame #13
Frame data:
02    11    82    10    00    0F    62    00    
21    00    05    2E    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 02,Message type:  82
Decoding R-UPDATE
Message segmantation:  1/ 1

Updated downstream PSD ceiling: 0x1000-->special value, no limit
Proposed higest downstream sub-carrier: 3938
Proposed lowest downstream sub-carrier: 33

Blackout set of downstream sub-carriers (# of break points): 0

Suggested cyclic extension length. Value m is 0x05, assuming a total of 4096 bins, CE length is 640

##################################################################################
 Rx frame found at index 604, frame size 69
##################################################################################
 Frame #14
Frame data:
03    11    04    09    33    40    21    35    
A0    28    35    A3    3A    33    23    5B    
33    C4    C0    35    24    DD    35    27    
A9    32    0A    E9    32    0F    62    03    
35    B0    21    7A    94    C0    F6    2A    
E9    05    01    00    80    0D    00    10    
00    00    05    02    60    21    00    00    
28    00    03    3A    02    83    5B    02    
73    7B    CE    3D    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 03,Message type:  04
Decoding O-PRM
Message segmantation:  1/ 1

Downstream MEDLEY reference PSD (# of breakpoint being described): 9
	Break point # 1, bin:   33, Level: -58.00 dBm/Hz
	Break point # 2, bin:   40, Level: -54.20 dBm/Hz
	Break point # 3, bin:  826, Level: -54.20 dBm/Hz
	Break point # 4, bin:  859, Level: -58.20 dBm/Hz
	Break point # 5, bin: 1216, Level: -57.20 dBm/Hz
	Break point # 6, bin: 1245, Level: -55.00 dBm/Hz
	Break point # 7, bin: 1961, Level: -55.00 dBm/Hz
	Break point # 8, bin: 2793, Level: -60.00 dBm/Hz
	Break point # 9, bin: 3938, Level: -60.00 dBm/Hz

Downstream MEDLEY set (# of Bands descriptor): 3
	Band # 1, Start   33, End  859
	Band # 2, Start 1216, End 1961
	Band # 3, Start 2793, End 3938

Cyclic extension length. Value m is 0x05, assuming a total of 4096 bins, CE length is 640
Dowstream cyclic prefix length: 256
Downstream transmit window length:  128
VTU-O IDFT size. value is 0x0D, size is 8192
VTU-O EC training period: 0
Requested VTU-O TEQ training period: 1024
Requested VTU-R TEQ training period: 0
Requested minimum duration of the periodic signal: 0
Downstream frequency-domain spectrum shaping (# of break points): 5
	Break point # 1, bin:   33, log_tssi value: -3.80 dB
	Break point # 2, bin:   40, log_tssi value: -0.00 dB
	Break point # 3, bin:  826, log_tssi value: -0.00 dB
	Break point # 4, bin:  859, log_tssi value: -4.00 dB
	Break point # 5, bin:  891, log_tssi value: -3.90 dB

##################################################################################
 Tx frame found at index 673, frame size 35
##################################################################################
 Frame #15
Frame data:
03    11    84    04    34    43    70    34    
84    AC    35    17    BD    35    AA    BF    
02    4A    C3    70    AB    F7    BD    01    
80    80    0D    08    10    08    12    FA    
00    80    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 03,Message type:  84
Decoding R-PRM
Message segmantation:  1/ 1

Upstream MEDLEY reference PSD (# of breakpoint being described): 4
	Break point # 1, bin:  880, Level: -56.40 dBm/Hz
	Break point # 2, bin: 1196, Level: -56.00 dBm/Hz
	Break point # 3, bin: 1981, Level: -55.10 dBm/Hz
	Break point # 4, bin: 2751, Level: -54.20 dBm/Hz

Upstream MEDLEY set (# of Bands descriptor): 2
	Band # 1, Start  880, End 1196
	Band # 2, Start 1981, End 2751

Upstream cyclic prefix length:  384
Upstream transmit window length:  128
VTU-R IDFT size. value is 0x0D, size is 8192
VTU-R EC training period: 512
Requested VTU-R TEQ training period: 1024
Requested VTU-O TEQ training period: 512
Requested minimum duration of the periodic signal: 1152
Minimum duration of R-P-TRAINING1: 16000

Upstream frequency-domain spectrum shaping (# of break points): 0

##################################################################################
 Rx frame found at index 709, frame size 6
##################################################################################
 Frame #16
Frame data:
04    11    00    E4    29    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 04,Message type:  00
Decoding O-ACK


##################################################################################
 Tx frame found at index 715, frame size 13
##################################################################################
 Frame #17
Frame data:
04    11    85    FF    F4    00    00    1F    
FF    02    02    3C    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 04,Message type:  85
Decoding R-TA_UPDATE
Message segmantation:  1/ 1
Current timing advance: -12
Timing advance correction: 0
Maximum value of timing advance VTU-R can accomodate: 8191
Desired number of SOC bytes per DMT symbol in O-P-MEDLEY: 2
Desired number of SOC bytes per DMT symbol in R-P-MEDLEY: 2

##################################################################################
 Rx frame found at index 729, frame size 10
##################################################################################
 Frame #18
Frame data:
05    11    05    00    00    02    02    BE    
0C    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 05,Message type:  05
Decoding O-TA_UPDATE
Message segmantation:  1/ 1
Timing advance correction: 0
Desired number of SOC bytes per DMT symbol in O-P-MEDLEY: 2
Desired number of SOC bytes per DMT symbol in R-P-MEDLEY: 2

##################################################################################
 Tx frame found at index 739, frame size 5
##################################################################################
 Frame #19
Frame data:
05    11    80    30    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 05,Message type:  80
Decoding R-ACK


##################################################################################
 Rx frame found at index 745, frame size 50
##################################################################################
 Frame #20
Frame data:
06    11    03    00    3C    00    00    FF    
FF    02    01    04    04    20    20    00    
08    30    D6    00    08    08    80    00    
00    08    16    08    00    08    08    80    
00    00    00    0F    0F    7D    00    7D    
00    7D    00    7D    00    30    18    CE    
71    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 06,Message type:  03
Decoding O-MSG1
Message segmantation:  1/ 1
Downstream target SNR margin: 6.00 dB
Downstream minium SNR margin: 0.00 dB
Downstream maximum SNR margin: 6553.50 dB
RA-MODE (rate adaptive) for downstream: 2
VTU-O transport NTR (0:false, 1:true): 1
TPS-TC capabilities:


Maximum number of downstream TPS-TC of each type:
	Number of STM TPS-TCs: 0
	Number of ATM TPS-TCs: 0
	Number of PTM TPS-TCs: 1

Maximum number of upstream TPS-TC of each type:
	Number of STM TPS-TCs: 0
	Number of ATM TPS-TCs: 0
	Number of PTM TPS-TCs: 1

Supported combinations of downstream bearer channels and TPS-TCs:
	PTM can be supported on bearer channel 0

Supported combinations of upstream bearer channels and TPS-TCs:
	PTM can be supported on bearer channel 0

Downstream PTM-TC #1: 
	Minimum net data rate: 64 kbits/s
	Maximum net data rate: 100016 kbits/s
	Reserved net data rate (not used, should equal to min net data rate): 64 kbits/s
	Maximum interleaving delay (not used for O-MSG1): 8
	Impulse noise protection (not used for O-MSG1): 128
 	TPS-TC options for PTM: None

Upstream PTM-TC #1: 
	Minimum net data rate: 64 kbits/s
	Maximum net data rate: 45120 kbits/s
	Reserved net data rate (not used, should equal to min net data rate): 64 kbits/s
	Maximum interleaving delay (not used for O-MSG1): 8
	Impulse noise protection (not used for O-MSG1): 128
 	TPS-TC options for PTM: None

PMS-TC capabilities:

Downstream dynamic interleaver (should be 0: not supported): 0
Upstream dynamic interleaver (should be 0: not supported): 0
Downstream message overhead data rate: 16 kbit/s
Upstream message overhead data rate: 16 kbit/s
Max DS net data rate for latency path 0: 256000 kbit/s
Max US net data rate for latency path 0: 256000 kbit/s
Max DS net data rate for latency path 1: 256000 kbit/s
Max US net data rate for latency path 1: 256000 kbit/s
Max DS (1/S) value: 48
Max US (1/S) value: 24

##################################################################################
 Tx frame found at index 795, frame size 41
##################################################################################
 Frame #21
Frame data:
06    11    83    04    04    20    20    00    
20    61    A8    00    00    00    00    00    
00    20    61    A8    00    00    00    00    
00    00    00    03    03    75    30    75    
30    75    30    75    30    40    40    D7    

Escaped bytes:    0, Errored escape bytes:    0
Message index: 06,Message type:  83
Decoding R-MSG2
Message segmantation:  1/ 1
TPS-TC capabilities:

Maximum number of downstream TPS-TC of each type:
	Number of STM TPS-TCs: 0
	Number of ATM TPS-TCs: 0
	Number of PTM TPS-TCs: 1

Maximum number of upstream TPS-TC of each type:
	Number of STM TPS-TCs: 0
	Number of ATM TPS-TCs: 0
	Number of PTM TPS-TCs: 1

Supported combinations of downstream barer channels and TPS-TCs:
	PTM can be supported on bearer channel 0

Supported combinations of upstream barer channels and TPS-TCs:
	PTM can be supported on bearer channel 0

Downstream PTM-TC #1: 
	Minimum net data rate: 256 kbits/s
	Maximum net data rate: 200000 kbits/s
	Reserved net data rate (not used, should equal to min net data rate): 0 kbits/s
	Maximum interleaving delay (not used for R-MSG2): 0
	Impulse noise protection (not used for R-MSG2): 0
 	TPS-TC options for PTM: None

Upstream PTM-TC #1: 
	Minimum net data rate: 256 kbits/s
	Maximum net data rate: 200000 kbits/s
	Reserved net data rate (not used, should equal to min net data rate): 0 kbits/s
	Maximum interleaving delay (not used for O-MSG1): 0
	Impulse noise protection (not used for O-MSG1): 0
 	TPS-TC options for PTM: None

PMS-TC capabilities:

Downstream dynamic interleaver (should be 0: not supported): 0
Upstream dynamic interleaver (should be 0: not supported): 0
Downstream message overhead data rate: 4 kbit/s
Upstream message overhead data rate: 4 kbit/s
Max DS net data rate for latency path 0: 240000 kbit/s
Max US net data rate for latency path 0: 240000 kbit/s
Max DS net data rate for latency path 1: 240000 kbit/s
Max US net data rate for latency path 1: 240000 kbit/s
Max DS (1/S) value: 64
Max US (1/S) value: 64

##################################################################################
 Rx frame found at index 837, frame size 27
##################################################################################
 Frame #22
Frame data:
07    11    06    20    20    64    00    20    
30    D6    00    00    08    80    00    00    
20    16    08    00    00    08    80    00    
95    C2    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 07,Message type:  06
Decoding O-TPS
Message segmantation:  1/ 1

Downstream TPS-TC to bearer channel mapping:
	PTM-TC mapped to bearer channel 0
	Bearer channel 1 inactive

Upstream TPS-TC to bearer channel mapping:
	PTM-TC mapped to bearer channel 0
	Bearer channel 1 inactive

Downstream rate adaption ratio (% of rate assigned to bearer channel 0): 100 %

Downstream TPS-TC #1: 
	Minimum net data rate: 256 kbits/s
	Maximum net data rate: 100016 kbits/s
	Reserved net data rate (not used, should equal to min net data rate): 0 kbits/s
	Maximum interleaving delay (not used for O-MSG1): 8
	Impulse noise protection (not used for O-MSG1): 128
 	TPS-TC options for PTM: None

Upstream TPS-TC #1: 
	Minimum net data rate: 256 kbits/s
	Maximum net data rate: 45120 kbits/s
	Reserved net data rate (not used, should equal to min net data rate): 0 kbits/s
	Maximum interleaving delay (not used for O-MSG1): 8
	Impulse noise protection (not used for O-MSG1): 128
 	TPS-TC options for PTM: None

##################################################################################
 Tx frame found at index 864, frame size 5
##################################################################################
 Frame #23
Frame data:
07    11    86    BE    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 07,Message type:  86
Decoding R-TPS-ACK
Message segmantation:  1/ 1

##################################################################################
 Rx frame found at index 870, frame size 36
##################################################################################
 Frame #24
Frame data:
08    11    07    00    0F    EF    00    40    
17    FF    01    2C    4D    00    78    00    
01    01    00    00    01    00    00    00    
00    00    01    01    80    00    FF    FF    
FF    B7    7E    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 08,Message type:  07
Decoding O-PMS
Message segmantation:  1/ 1
OH frames of type 1 (message overhead) is assigned to latency path 0

Upstream bearer channels to latency paths mapping:
	Bearer channel 0 is carried by latency path 0
	Bearer channel 1 is disabled
Upstream number of octets per MDF for bearer channel 0 (Bx0): 239
Upstream number of octets per MDF for bearer channel 1 (Bx1): 0

Framing parameters for latency path 0
	T,Nummber of MDFs in an OH sub-frame: 64
	G,Total nummber of overhead octets in an OH sub-frame: 23
	F,Nummber of OH frames in the OH superframe: 255
	M,Nummber of MDFs in an RS codeword (valid value 1,2,4,8 and 16): 1
	L: 11341, R:    0, I:  120, D:    1

Framing parameters for latency path 1
	T,Nummber of MDFs in an OH sub-frame: 1
	G,Total nummber of overhead octets in an OH sub-frame: 0
	F,Nummber of OH frames in the OH superframe: 0
	M,Nummber of MDFs in an RS codeword (valid value 1,2,4,8 and 16): 1
	L:    0, R:    0, I:    0, D:    1

MaxD0, Maximum downstream interleaver delay for latency path 0 in bytes: 98304
MaxD1: 0xFFFFFF-->VTU-R shall autonomouslt partition MaxD0

##################################################################################
 Tx frame found at index 906, frame size 31
##################################################################################
 Frame #25
Frame data:
08    11    87    00    0F    EE    00    16    
03    0A    01    68    3E    10    FF    00    
D1    00    00    00    00    00    00    00    
00    00    00    00    38    EA    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 08,Message type:  87
Decoding R-PMS
Message segmantation:  1/ 1
OH frames of type 1 (message overhead) is assigned to latency path 0

Upstream bearer channels to latency paths mapping:
	Bearer channel 0 is carried by latency path 0
	Bearer channel 1 is disabled
Upstream number of octets per MDF for bearer channel 0 (Bx0): 238
Upstream number of octets per MDF for bearer channel 1 (Bx1): 0

Framing parameters for latency path 0
	T,Nummber of MDFs in an OH sub-frame: 22
	G,Total nummber of overhead octets in an OH sub-frame: 3
	F,Nummber of OH frames in the OH superframe: 10
	M,Nummber of MDFs in an RS codeword (valid value 1,2,4,8 and 16): 1
	L: 26686, R:   16, I:  255, D:  209

Framing parameters for latency path 1
	T,Nummber of MDFs in an OH sub-frame: 0
	G,Total nummber of overhead octets in an OH sub-frame: 0
	F,Nummber of OH frames in the OH superframe: 0
	M,Nummber of MDFs in an RS codeword (valid value 1,2,4,8 and 16): 0
	L:    0, R:    0, I:    0, D:    0
VTU-R erasure decoding:
	Erasure decoding is not used for latency path 0
	Erasure decoding is not used for latency path 1

##################################################################################
 Rx frame found at index 938, frame size 1029
##################################################################################
 Frame #26
Frame data:
09    41    08    01    B1    EE    B1    EE    
B1    EE    B1    EE    B1    EE    B1    EE    
B1    EE    B1    EE    B1    EE    B1    EE    
B1    EE    B1    EE    B1    EE    B1    EE    
B1    EE    B1    EE    B1    EE    B1    EE    
B1    EE    B1    EE    B1    EE    B1    EE    
B1    EE    B1    EE    B1    EE    B1    EE    
B1    EE    B1    EE    B1    EE    B1    EE    
B1    EE    B1    EE    B1    EE    B1    EE    
B1    EE    B1    EE    B1    EE    B1    EE    
B1    EE    B1    EE    B1    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    00    00    00    00    
00    00    00    00    
Escaped bytes:    0, Errored escape bytes:    0
Message index: 09,Message type:  08
Decoding O-PMD
Message segmantation:  1/ 4
