ModemStatus DEBUG 2 #modem status # 1 #0
BinSelect DEBUG 0 #Debug tone selection # 1 #0
IntCrcErrsD METANOIA 0 #Receive CRC counter # 1 #1
nO_DsFastPathRate DEBUG 0 #Data rate ( unit is 64 kbps ) # 1 #0
nO_UsFastPathRate DEBUG 0 #Data rate ( unit is 64 kbps ) # 1 #0
VisibleUsPb0FirstTone BANDPLAN 0 # # 1 #0
VisibleUsPb0LastTone BANDPLAN 0 # # 1 #0
VisibleUsPb1FirstTone BANDPLAN 0 # # 1 #0
VisibleUsPb1LastTone BANDPLAN 0 # # 1 #0
VisibleUsPb2FirstTone BANDPLAN 0 # # 1 #0
VisibleUsPb2LastTone BANDPLAN 0 # # 1 #0
VisibleUsPb3FirstTone BANDPLAN 0 # # 1 #0
VisibleUsPb3LastTone BANDPLAN 0 # # 1 #0
VisibleUsPb4FirstTone BANDPLAN 0 # # 1 #0
VisibleUsPb4LastTone BANDPLAN 0 # # 1 #0
VisibleUsPb0Tones BANDPLAN 0 # # 1 #0
VisibleUsPb1Tones BANDPLAN 0 # # 1 #0
VisibleUsPb2Tones BANDPLAN 0 # # 1 #0
VisibleUsPb3Tones BANDPLAN 0 # # 1 #0
VisibleUsTones BANDPLAN 0 # # 1 #0
VisibleUsPbs BANDPLAN 0 # # 1 #0
VisibleDsPb0LastTone BANDPLAN 0 # # 1 #0
VisibleDsPb1FirstTone BANDPLAN 0 # # 1 #0
VisibleDsPb1LastTone BANDPLAN 0 # # 1 #0
VisibleDsPb2FirstTone BANDPLAN 0 # # 1 #0
VisibleDsPb2LastTone BANDPLAN 0 # # 1 #0
VisibleDsPb3FirstTone BANDPLAN 0 # # 1 #0
VisibleDsPb3LastTone BANDPLAN 0 # # 1 #0
VisibleDsPb0Tones BANDPLAN 0 # # 1 #0
VisibleDsPb1Tones BANDPLAN 0 # # 1 #0
VisibleDsPb2Tones BANDPLAN 0 # # 1 #0
VisibleDsPb3Tones BANDPLAN 0 # # 1 #0
VisibleDsTones BANDPLAN 0 # # 1 #0
VisibleDsPbs BANDPLAN 0 # # 1 #0
ElectricLen DEBUG 0 #estimated line length # 1 #0
AocMinMarg1 DEBUG 0 #minmal snr Bin's snr # 1 #0
AocMinMarg2 DEBUG 0 #second minmal snr Bin's snr # 1 #0
RxPktCntr METANOIA 0 # send packet counter to switch# 1 #1
TxPktCntr METANOIA 0 # receive packet counter from switch p# 1 #1
xdsl2LineStatusAttainableRateDs METANOIA 0 # DS attainable data rate # 1 #1
xdsl2LineStatusAttainableRateUs METANOIA 0 # US attainable data rate # 1 #1
xdsl2LineStatusActAtpDs METANOIA 0 # DS actual power # 1 #1
xdsl2LineStatusActAtpUs METANOIA 0 # US actual power # 1 #1
xdsl2LineStatusActProfile METANOIA 0 # actual profile # 1 #1
xdsl2LineStatusElectricalLength METANOIA 0 # 1K electrical length * 14.4 ft # 1 #1
xdsl2LineBandStatusLnAtten9 METANOIA 0 # US all band line atten # 1 #1
xdsl2LineBandStatusSigAtten9 METANOIA 0 # US all band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin9 METANOIA 0 #Current SNR US # 1 #1
xdsl2LineBandStatusLnAtten10 METANOIA 0 # DS all band ling atten # 1 #1
xdsl2LineBandStatusSigAtten10 METANOIA 0 # DS all band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin10 METANOIA 0 #Current SNR DS # 1 #1
xdsl2LineBandStatusLnAtten0 DEBUG 0 # us0 band line atten # 1 #1
xdsl2LineBandStatusSigAtten0 DEBUG 0 # us0 band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin0 DEBUG 0 # us0 Current SNR # 1 #1
xdsl2LineBandStatusLnAtten1 DEBUG 0 # us1 band line atten # 1 #1
xdsl2LineBandStatusSigAtten1 DEBUG 0 # us1 band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin1 DEBUG 0 #Current SNR us1 # 1 #1
xdsl2LineBandStatusLnAtten2 DEBUG 0 # us2 band line atten # 1 #1
xdsl2LineBandStatusSigAtten2 DEBUG 0 # us2 band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin2 DEBUG 0 #Current SNR us2 # 1 #1
xdsl2LineBandStatusLnAtten3 DEBUG 0 # us3 band line atten # 1 #1
xdsl2LineBandStatusSigAtten3 DEBUG 0 # us3 band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin3 DEBUG 0 #Current SNR us3 # 1 #1
xdsl2LineBandStatusLnAtten4 DEBUG 0 # us4 band line atten # 1 #1
xdsl2LineBandStatusSigAtten4 DEBUG 0 # us4 band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin4 DEBUG 0 #Current SNR us4 # 1 #1
xdsl2LineBandStatusLnAtten5 DEBUG 0 # ds1 band line atten # 1 #1
xdsl2LineBandStatusSigAtten5 DEBUG 0 # ds1 band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin5 DEBUG 0 #Current SNR ds1 # 1 #1
xdsl2LineBandStatusLnAtten6 DEBUG 0 # ds2 band line atten # 1 #1
xdsl2LineBandStatusSigAtten6 DEBUG 0 # ds2 band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin6 DEBUG 0 #Current SNR ds2 # 1 #1
xdsl2LineBandStatusLnAtten7 DEBUG 0 # ds3 band line atten # 1 #1
xdsl2LineBandStatusSigAtten7 DEBUG 0 # ds3 band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin7 DEBUG 0 #Current SNR ds3 # 1 #1
xdsl2LineBandStatusLnAtten8 DEBUG 0 # ds4 band line atten # 1 #1
xdsl2LineBandStatusSigAtten8 DEBUG 0 # ds4 band signal atten # 1 #1
xdsl2LineBandStatusSnrMargin8 DEBUG 0 #Current SNR ds4 # 1 #1
xdsl2ChStatusActDataRate0 METANOIA 0 #US actual data rate # 1 #1
xdsl2ChStatusPrevDataRate0 METANOIA 0 # # 1 #1
xdsl2ChStatusActDelay0 METANOIA 0 #US actual delay # 1 #1
xdsl2ChStatusActInp0 METANOIA 0 #US actual INP # 1 #1
xdsl2ChStatusActDataRate2 METANOIA 0 #DS actual data rate # 1 #1
xdsl2ChStatusPrevDataRate2 METANOIA 0 # # 1 #1
xdsl2ChStatusActDelay2 METANOIA 0 #DS actual delay # 1 #1
xdsl2ChStatusActInp2 METANOIA 0 #DS actual INP # 1 #1
xdsl2LConfProfVdsl2CarMask BANDPLAN 2 #Conf band plan # 1 #0
xdsl2LConfProfTargetSnrmDs METANOIA 0 #DS target SNR margin # 1 #1
xdsl2LConfProfTargetSnrmUs METANOIA 0 #US target SNR margin # 1 #1
xdsl2LConfProfProfiles METANOIA 0 #Conf active profile # 1 #1
xdsl2LConfProfPsdMaskDs BANDPLAN 2 #Conf DS PSD mask # 1 #0
xdsl2LConfProfPsdMaskUs BANDPLAN 2 #Conf US PSD mask # 1 #0
xdsl2ChConfProfMinDataRateDs0 METANOIA 0 # config min data rate DS # 1 #1
xdsl2ChConfProfMinDataRateUs0 METANOIA 0 # config min data rate US # 1 #1
xdsl2ChConfProfMaxDataRateDs0 METANOIA 0 #Conf DS max data rate # 1 #1
xdsl2ChConfProfMaxDataRateUs0 METANOIA 0 #Conf US max data rate # 1 #1
xdsl2ChConfProfMaxDelayDs0 METANOIA 0 #Conf DS max network delay # 1 #1
xdsl2ChConfProfMaxDelayUs0 METANOIA 0 #Conf US max network delay # 1 #1
xdsl2ChConfProfMinProtectionDs0 METANOIA 0 #Conf DS INP in non-30a # 1 #1
xdsl2ChConfProfMinProtectionUs0 METANOIA 0 #Conf US INP in non-30a # 1 #1
xdsl2ChConfProfMinProtection8Ds0 METANOIA 0 #Conf DS INP in 30a # 1 #1
xdsl2ChConfProfMinProtection8Us0 METANOIA 0 #Conf US INP in 30a # 1 #1
xdsl2PMLInitCurr15MFullInits0 METANOIA 0 # Full init counter # 1 #1
xdsl2PMLInitCurr15MFailedFullInits0 METANOIA 0 # Fail init counter # 1 #1
xdsl2PMLInitCurr15MFullInits1 METANOIA 0 # Full init counter # 1 #1
xdsl2PMLHistInit15MFailedFullInits0 METANOIA 0 # Full init counter # 1 #1
xdsl2PMChCurr15MCodingViolations0 METANOIA 0 # CRC counter # 1 #1
xdsl2PMChCurr15MCorrectedBlocks0 METANOIA 0 # error correction counter # 1 #1
xdsl2PMChCurr15MCodingViolations2 METANOIA 0 # CRC counter # 1 #1
xdsl2PMChCurr15MCorrectedBlocks2 METANOIA 0 # error correction counter # 1 #1
vdslOtPhysCurrLineRate METANOIA 0 #Current UpStream linerate # 1 #1
vdslRtPhysCurrSnrMgn METANOIA 0 #Current DownStream Snr Mgn # 1 #1
vdslRtPhysCurrLineRate METANOIA 0 #Current DownStream linerate # 1 #1
vdslOtIntlvChanCurrTxSlowBurstProtect DEBUG 0 #unit of us, impulse noise protect of downstream, ~InterleaveDelay*(R/2N),R=16,N=160 # 1 #0
vdslRtIntlvChanCurrTxSlowBurstProtect DEBUG 0 #unit of us, impulse noise protect of upstream, ~InterleaveDelay*(R/2N),R=16,N=160 # 1 #0
vdslOtPerfDataESs DEBUG 0 #UpStream Error second # 1 #0
vdslOtPerfDataInits METANOIA 0 #connection success counter # 1 #1
vdslRtPerfDataESs DEBUG 0 #DownStream Error second # 1 #0
vdslRtPerfDataInits METANOIA 0 #connection success counter # 1 #1
vdslFirmwareVer METANOIA 2 #Firmware version # 1 #1
vdslFirmwareDate METANOIA 2 #Firmware date # 1 #1
vdslFirmwareTime METANOIA 2 #Firmware time # 1 #1
vdslLineDiagInitD DEBUG 2 # # 1 #0
vdslLineDiagInitDD DEBUG 2 # # 1 #0
vdslLineDiagTrnD DEBUG 2 # # 1 #0
vdslLineDiagTrnDD DEBUG 2 # # 1 #0
vdslLineDiagStD DEBUG 2 # # 1 #0
vdslLineDiagStDD DEBUG 2 # # 1 #0
vdslLineTime250ms DEBUG 2 # # 1 #0
vdslLineTime250msD DEBUG 2 # # 1 #0
vdslLineTime250msDD DEBUG 2 # # 1 #0
vdslLinePauseFrmCntr DEBUG 0 #802.3 pause frame counter # 1 #0
vdslLineDiagSt2 DEBUG 2 # # 1 #0
vdslLineDiagSt2D DEBUG 2 # # 1 #0
vdslLineDiagSt2DD DEBUG 2 # # 1 #0
vdslTwConfig METANOIA 2 #bit 4: report packet activities in LED 0 # 1 #1
xdslGhsConfCarrierSet DEBUG 0 # # 1 #0
vdslMetanoiaUsDataRatio DEBUG 0 #unit of %, ~DataRate/LineRata # 1 #0
vdslMetanoiaRtVcxo DEBUG 2 #RT clock setting reference # 1 #0
SecondCnt DEBUG 0 #when showtime, the value is seconds from showtime start # 1 #0
SecondIntlvCntST DEBUG 0 #total seconds of showtime # 1 #0
FeVendorFlag METANOIA 2 #IOP vendor ID and version # 1 #1
nGhsCLRChipVendor1 DEBUG 0 # # 1 #0
nGhsCLRChipVendor2 DEBUG 0 # # 1 #0
FeVendorFlag DEBUG 2 #IOP vendor ID and version # 1 #1
xdsl2LInvG994VendorId0 DEBUG 0 # # 1 #0
xdsl2LInvSystemVendorId0 DEBUG 0 # # 1 #0
xdsl2LInvG994VendorId1 DEBUG 0 # # 1 #0
xdsl2LInvSystemVendorId1 DEBUG 0 # # 1 #0
xdslGhsConfOtVendorId DEBUG 0 # # 1 #0
xdslGhsConfRtVendorId DEBUG 0 # # 1 #0
xdslGhsOtVendorId DEBUG 0 # # 1 #0
xdslGhsRtVendorId DEBUG 0 # # 1 #0
