MIBName ViewGroup DisplayFormat # MIBDescription #ShowLog#LastSave#MIBGrpup

BinSelect DEBUG 0 #Debug tone selection # 1 #0

nO_DsFastPathRate DEBUG 0 #Data rate ( unit is 64 kbps ) # 1 #0
nO_UsFastPathRate DEBUG 0 #Data rate ( unit is 64 kbps ) # 1 #0
ElectricLen DEBUG 0 #estimated line length # 1 #0
AocMinMarg1 DEBUG 0 #minmal snr Bin's snr # 1 #0
AocMinMarg2 DEBUG 0 #second minmal snr Bin's snr # 1 #0
RxPktCntr METANOIA 0 # send packet counter to switch# 1 #1
TxPktCntr METANOIA 0 # receive packet counter from switch p# 1 #1
xdsl2PMLHistInit15MFailedFullInits0 METANOIA 0 # Full init counter # 1 #1
vdslOtPhysCurrLineRate METANOIA 0 #Current UpStream linerate # 1 #1

vdslRtPhysCurrLineRate METANOIA 0 #Current DownStream linerate # 1 #1
vdslOtIntlvChanCurrTxSlowBurstProtect DEBUG 0 #unit of us, impulse noise protect of downstream, ~InterleaveDelay*(R/2N),R=16,N=160 # 1 #0
vdslRtIntlvChanCurrTxSlowBurstProtect DEBUG 0 #unit of us, impulse noise protect of upstream, ~InterleaveDelay*(R/2N),R=16,N=160 # 1 #0
vdslOtPerfDataESs DEBUG 0 #UpStream Error second # 1 #0

vdslRtPerfDataESs DEBUG 0 #DownStream Error second # 1 #0
vdslRtPerfDataInits METANOIA 0 #connection success counter # 1 #1
vdslFirmwareVer METANOIA 2 #Firmware version # 1 #1
vdslFirmwareDate METANOIA 2 #Firmware date # 1 #1
vdslFirmwareTime METANOIA 2 #Firmware time # 1 #1
vdslLineDiagInitD DEBUG 2 # # 1 #0
vdslLineDiagInitDD DEBUG 2 # # 1 #0
vdslLineDiagTrnD DEBUG 2 # # 1 #0
vdslLineDiagTrnDD DEBUG 2 # # 1 #0
vdslLineDiagStD DEBUG 2 # # 1 #0
vdslLineDiagStDD DEBUG 2 # # 1 #0
vdslLineTime250ms DEBUG 2 # # 1 #0
vdslLineTime250msD DEBUG 2 # # 1 #0
vdslLineTime250msDD DEBUG 2 # # 1 #0
vdslLinePauseFrmCntr DEBUG 0 #802.3 pause frame counter # 1 #0
vdslLineDiagSt2 DEBUG 2 # # 1 #0
vdslLineDiagSt2D DEBUG 2 # # 1 #0
vdslLineDiagSt2DD DEBUG 2 # # 1 #0

xdslGhsConfCarrierSet DEBUG 0 # # 1 #0
vdslMetanoiaUsDataRatio DEBUG 0 #unit of %, ~DataRate/LineRata # 1 #0
vdslMetanoiaRtVcxo DEBUG 2 #RT clock setting reference # 1 #0
SecondCnt DEBUG 0 #when showtime, the value is seconds from showtime start # 1 #0
SecondIntlvCntST DEBUG 0 #total seconds of showtime # 1 #0
FeVendorFlag METANOIA 2 #IOP vendor ID and version # 1 #1
nGhsCLRChipVendor1 DEBUG 0 # # 1 #0
nGhsCLRChipVendor2 DEBUG 0 # # 1 #0
FeVendorFlag DEBUG 2 #IOP vendor ID and version # 1 #1
xdslGhsConfOtVendorId DEBUG 0 # # 1 #0
xdslGhsConfRtVendorId DEBUG 0 # # 1 #0
ModemStatus METANOIA 2 #modem status # 1 #0
xdslMetanoiaOtCorrectedBlocks0 METANOIA 0 # US error correction counter this showtime# 1 #0
xdslMetanoiaRtCorrectedBlocks0 METANOIA 0 #  DS error correction counter this showtime # 1 #0



------------------------      Line      ------------------------

xdsl2LineStatusPwrMngState DEFAULT 0 # 4-No power management # 0 # 0 #Line
xdsl2LineStatusInitResult DEFAULT 0 # Indicates the result of the last full initialization performed on the line{noFail(0), configError(1),configNotFeasible(2), commFail(3), noPeerAtu(4),otherCause(5)} # 1 #0 #Line
xdsl2LineStatusLastStateDs DEFAULT 0 # The last successful transmitted initialization state in the downstream direction in the last full initialization performed on the line # 1 #0 #Line
xdsl2LineStatusLastStateUs DEFAULT 0 # The last successful transmitted initialization state in the upstream direction in the last full initialization performed on the line # 1 #0 #Line
xdsl2LineStatusXtur DEFAULT 0 # Indicates current state (existing failures) of the xTU-C # 1 #0 #Line
xdsl2LineStatusXtuc DEFAULT 0 # Indicates current state (existing failures) of the xTU-R # 1 #0 #Line
xdsl2LineStatusAttainableRateDs METANOIA 0 # Downstream attainable date rate(kbps) # 1 #1#Line
xdsl2LineStatusAttainableRateUs METANOIA 0 # Uownstream attainable date rate(kbps) # 1 #1#Line
xdsl2LineStatusActPsdDs DEFAULT 0 # Actual Power Spectrum Density (PSD) Downstream(0.1dB) # 1 #0 #Line
xdsl2LineStatusActPsdUs DEFAULT 0 # Actual Power Spectrum Density (PSD) Upstream(0.1dB) # 1 #0 #Line
xdsl2LineStatusActAtpDs METANOIA 0 # Actual Aggregate Transmit Power Downstream(0.1dB) # 1 #1#Line
xdsl2LineStatusActAtpUs METANOIA 0 # Actual Aggregate Transmit Power Upstream(0.1dB) # 1 #1#Line
xdsl2LineStatusActProfile METANOIA 0 # The G.993.2 profile in use{profile8a(0),profile8b(1),profile8c(2),profile8d(3),profile12a(4),profile12b(5),profile17a(6),profile30a(7)} # 1 #1#Line
xdsl2LineStatusActLimitMask DEFAULT 0 # The Limit PSD mask and band plan in use # 1 #0 #Line
xdsl2LineStatusActUs0Mask DEFAULT 0 # The US0 PSD mask in use # 1 #0 #Line
xdsl2LineStatusActSnrModeDs DEFAULT 0 # Downstream no virtual noise # 1 #0 #Line
xdsl2LineStatusActSnrModeUs DEFAULT 0 # Upstream no virtual noise # 1 #0 #Line
xdsl2LineStatusElectricalLength METANOIA 0 # Electric length (0.1dB),about 14.4ft # 1 #1#Line
xdsl2LineStatusTssiDs DEFAULT 0 # The transmit spectrum shaping (TSSi) breakpoints expressed as the set of breakpoints exchanged during G.994.1 # 1 #0 #Line
xdsl2LineStatusTssiUs DEFAULT 0 # The transmit spectrum shaping (TSSi) breakpoints expressed as the set of breakpoints exchanged during G.994.1 # 1 #0 #Line
xdsl2LineStatusMrefPsdDs DEFAULT 0 # The MEDLEY Reference PSD status parameters in the downstreasm # 1 #0 #Line
xdsl2LineStatusMrefPsdUs DEFAULT 0 # The MEDLEY Reference PSD status parameters in the upstreasm # 1 #0 #Line
xdsl2LineStatusTrellisDs DEFAULT 0 # This parameter reports whether trellis coding is in use in the downstream direction # 1 #0 #Line
xdsl2LineStatusTrellisUs DEFAULT 0 # This parameter reports whether trellis coding is in use in the upstream direction # 1 #0 #Line
xdsl2LineStatusActualCe DEFAULT 0 # This parameter reports the cyclic extension used on the line # 1 #0 #Line
xdsl2LineCnfgTemplate DEFAULT 0 # # 1 #0 #Line
xdsl2LineCnfgFallbackTemplate DEFAULT 0 # # 1 #0 #Line
xdsl2LineAlarmCnfgTemplate DEFAULT 0 # # 1 #0 #Line
xdsl2LineCmndConfPmsf DEFAULT 0 # # 1 #0 #Line
xdsl2LineCmndConfLdsf DEFAULT 0 # # 1 #0 #Line
xdsl2LineCmndConfLdsfFailReason DEFAULT 0 # # 1 #0 #Line
xdsl2LineCmndConfBpsc DEFAULT 0 # # 1 #0 #Line
xdsl2LineCmndConfBpscFailReason DEFAULT 0 # # 1 #0 #Line
xdsl2LineCmndConfBpscReqCount DEFAULT 0 # # 1 #0 #Line
xdsl2LineCmndAutomodeColdStart DEFAULT 0 # # 1 #0 #Line
xdsl2LineCmndConfReset DEFAULT 0 # # 1 #0 #Line
xdsl2LineStatusActTemplate DEFAULT 0 # # 1 #0 #Line
xdsl2LineStatusXtuTransSys DEFAULT 0 # # 1 #0 #Line


------------------------      LineBand      ------------------------

xdsl2LineBand0 DEFAULT 0 # us0 # 1 #0 #LineBand
xdsl2LineBand1 DEFAULT 0 # us1 # 1 #0 #LineBand
xdsl2LineBand2 DEFAULT 0 # us2 # 1 #0 #LineBand
xdsl2LineBand3 DEFAULT 0 # us3 # 1 #0 #LineBand
xdsl2LineBand4 DEFAULT 0 # us4 # 1 #0 #LineBand
xdsl2LineBand5 DEFAULT 0 # ds1 # 1 #0 #LineBand
xdsl2LineBand6 DEFAULT 0 # ds2 # 1 #0 #LineBand
xdsl2LineBand7 DEFAULT 0 # ds3 # 1 #0 #LineBand
xdsl2LineBand8 DEFAULT 0 # ds4 # 1 #0 #LineBand
xdsl2LineBand9 DEFAULT 0 # # 1 #0 #LineBand
xdsl2LineBand10 DEFAULT 0 # # 1 #0 #LineBand
xdsl2LineBandStatusLnAtten0 DEBUG 0 # us0 band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten1 DEBUG 0 # us1 band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten2 DEBUG 0 # us2 band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten3 DEBUG 0 # us3 band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten4 DEBUG 0 # us4 band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten5 DEBUG 0 # ds1 band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten6 DEBUG 0 # ds2 band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten7 DEBUG 0 # ds3 band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten8 DEBUG 0 # ds4 band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten9 METANOIA 0 # US all band line atten # 1 #1#LineBand
xdsl2LineBandStatusLnAtten10 METANOIA 0 # DS all band ling atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten0 DEBUG 0 # us0 band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten1 DEBUG 0 # us1 band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten2 DEBUG 0 # us2 band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten3 DEBUG 0 # us3 band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten4 DEBUG 0 # us4 band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten5 DEBUG 0 # ds1 band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten6 DEBUG 0 # ds2 band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten7 DEBUG 0 # ds3 band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten8 DEBUG 0 # ds4 band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten9 METANOIA 0 # US all band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSigAtten10 METANOIA 0 # DS all band signal atten # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin0 DEBUG 0 #Current SNR us0 # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin1 DEBUG 0 #Current SNR us1 # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin2 DEBUG 0 #Current SNR us2 # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin3 DEBUG 0 #Current SNR us3 # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin4 DEBUG 0 #Current SNR us4 # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin5 DEBUG 0 #Current SNR ds1 # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin6 DEBUG 0 #Current SNR ds2 # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin7 DEBUG 0 #Current SNR ds3 # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin8 DEBUG 0 #Current SNR ds4 # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin9 METANOIA 0 #Current SNR US # 1 #1#LineBand
xdsl2LineBandStatusSnrMargin10 METANOIA 0 #Current SNR DS # 1 #1#LineBand


------------------------      ChannelStatus      ------------------------

xdsl2ChStatusUnit0 DEFAULT 0 # The termination unit xtuc(1) or xtur(2) # 1 #0 #ChannelStatus
xdsl2ChStatusUnit1 DEFAULT 0 # The termination unit xtuc(1) or xtur(2) # 1 #0 #ChannelStatus
xdsl2ChStatusUnit2 DEFAULT 0 # The termination unit xtuc(1) or xtur(2) # 1 #0 #ChannelStatus
xdsl2ChStatusUnit3 DEFAULT 0 # The termination unit xtuc(1) or xtur(2) # 1 #0 #ChannelStatus
xdsl2ChStatusActDataRate0 METANOIA 0 #US actual data rate # 1 #1#ChannelStatus
xdsl2ChStatusActDataRate1 METANOIA 0 # # 1 #1#ChannelStatus
xdsl2ChStatusActDataRate2 METANOIA 0 #DS, actual data rate # 1 #1#ChannelStatus
xdsl2ChStatusActDataRate3 METANOIA 0 # # 1 #1#ChannelStatus
xdsl2ChStatusPrevDataRate0 METANOIA 0 #US, previous net data rate(kbps) # 1 #1#ChannelStatus
xdsl2ChStatusPrevDataRate1 METANOIA 0 # # 1 #1#ChannelStatus
xdsl2ChStatusPrevDataRate2 METANOIA 0 #DS, previous net data rate(kbps) # 1 #1#ChannelStatus
xdsl2ChStatusPrevDataRate3 METANOIA 0 # # 1 #1#ChannelStatus
xdsl2ChStatusActDelay0 METANOIA 0 #US, actual delay # 1 #1#ChannelStatus
xdsl2ChStatusActDelay1 METANOIA 0 # # 1 #1#ChannelStatus
xdsl2ChStatusActDelay2 METANOIA 0 #DS, actual delay # 1 #1#ChannelStatus
xdsl2ChStatusActDelay3 METANOIA 0 # # 1 #1#ChannelStatus
xdsl2ChStatusActInp0 METANOIA 0 #US, actual INP # 1 #1#ChannelStatus
xdsl2ChStatusActInp1 METANOIA 0 # # 1 #1#ChannelStatus
xdsl2ChStatusActInp0 METANOIA 0 #DS, actual INP # 1 #1#ChannelStatus
xdsl2ChStatusActInp3 METANOIA 0 # # 1 #1ChannelStatus
xdsl2ChStatusInpReport0 DEFAULT 0 #Us, Impulse noise protection reporting mode(1-inpComputedUsingFormula) # 1 #0 #ChannelStatus
xdsl2ChStatusInpReport1 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusInpReport2 DEFAULT 0 #Ds, Impulse noise protection reporting mode(1-inpComputedUsingFormula) # 1 #0 #ChannelStatus
xdsl2ChStatusInpReport3 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusNFec0 DEFAULT 0 #Us, Actual size of Reed-Solomon codeword # 1 #0 #ChannelStatus
xdsl2ChStatusNFec1 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusNFec2 DEFAULT 0 #Ds, Actual size of Reed-Solomon codeword # 1 #0 #ChannelStatus
xdsl2ChStatusNFec3 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusRFec0 DEFAULT 0 #Us, Actual number of Reed-Solomon redundancy bytes # 1 #0 #ChannelStatus
xdsl2ChStatusRFec1 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusRFec2 DEFAULT 0 #Ds, Actual number of Reed-Solomon redundancy bytes # 1 #0 #ChannelStatus
xdsl2ChStatusRFec3 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusLSymb0 DEFAULT 0 #Us, Actual number of bits per symbol # 1 #0 #ChannelStatus
xdsl2ChStatusLSymb1 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusLSymb2 DEFAULT 0 #Ds, Actual number of bits per symbol # 1 #0 #ChannelStatus
xdsl2ChStatusLSymb3 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusIntlvDepth0 DEFAULT 0 #Us, Actual interleaving depth # 1 #0 #ChannelStatus
xdsl2ChStatusIntlvDepth1 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusIntlvDepth2 DEFAULT 0 #Ds, Actual interleaving depth # 1 #0 #ChannelStatus
xdsl2ChStatusIntlvDepth3 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusIntlvBlock0 DEFAULT 0 #Us, Actual interleaving block length # 1 #0 #ChannelStatus
xdsl2ChStatusIntlvBlock1 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusIntlvBlock2 DEFAULT 0 #Ds, Actual interleaving block length # 1 #0 #ChannelStatus
xdsl2ChStatusIntlvBlock3 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusLPath0 DEFAULT 0 #Us, Actual latency path # 1 #0 #ChannelStatus
xdsl2ChStatusLPath1 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusLPath2 DEFAULT 0 #Ds, Actual latency path # 1 #0 #ChannelStatus
xdsl2ChStatusLPath3 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusAtmStatus0 DEFAULT 0 #Us, not ATM # 1 #0 #ChannelStatus
xdsl2ChStatusAtmStatus1 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusAtmStatus2 DEFAULT 0 #Ds, not ATM # 1 #0 #ChannelStatus
xdsl2ChStatusAtmStatus3 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusPtmStatus0 DEFAULT 0 #Us, PTM status(noDefect) # 1 #0 #ChannelStatus
xdsl2ChStatusPtmStatus1 DEFAULT 0 # # 1 #0 #ChannelStatus
xdsl2ChStatusPtmStatus2 DEFAULT 0 #Ds, PTM status(noDefect) # 1 #0 #ChannelStatus
xdsl2ChStatusPtmStatus3 DEFAULT 0 # # 1 #0 #ChannelStatus



------------------------      SCStatus      ------------------------

xdsl2SCStatusDirection0 DEFAULT 0 #The direction of the subcarrier either upstream or downstream{upstream(1),downstream(2)} # 1 #0 #SCStatus
xdsl2SCStatusDirection1 DEFAULT 0 #The direction of the subcarrier either upstream or downstream{upstream(1),downstream(2)} # 1 #0 #SCStatus
xdsl2SCStatusLinScale0 DEFAULT 0 #Us, scale factor to be applied to the H(f) linear representation values # 1 #0 #SCStatus
xdsl2SCStatusLinScale1 DEFAULT 0 #Ds, scale factor to be applied to the H(f) linear representation values # 1 #0 #SCStatus
xdsl2SCStatusLinScGroupSize0 DEFAULT 0 #Us, Number of subcarriers per group # 1 #0 #SCStatus
xdsl2SCStatusLinScGroupSize1 DEFAULT 0 #Ds, Number of subcarriers per group # 1 #0 #SCStatus
xdsl2SCStatusLogMt0 DEFAULT 0 #Us, the number of symbols used to measure the Hlog(f) values # 1 #0 #SCStatus
xdsl2SCStatusLogMt1 DEFAULT 0 #Ds, the number of symbols used to measure the Hlog(f) values # 1 #0 #SCStatus
xdsl2SCStatusLogMt0 DEFAULT 0 #Us, Number of subcarriers per group used to report the H(f) logarithmic representation values # 1 #0 #SCStatus
xdsl2SCStatusLogMt1 DEFAULT 0 #Ds, Number of subcarriers per group used to report the H(f) logarithmic representation values # 1 #0 #SCStatus
xdsl2SCStatusQlnMt0 DEFAULT 0 #Us, number of symbols used to measure the QLN(f) values # 1 #0 #SCStatus
xdsl2SCStatusQlnMt1 DEFAULT 0 #Ds, number of symbols used to measure the QLN(f) values # 1 #0 #SCStatus
xdsl2SCStatusQlnScGroupSize0 DEFAULT 0 #Us, Number of subcarriers per group # 1 #0 #SCStatus
xdsl2SCStatusQlnScGroupSize1 DEFAULT 0 #Ds, Number of subcarriers per group # 1 #0 #SCStatus
xdsl2SCStatusSnrMtime0 DEFAULT 0 #Us, the number of symbols used to measure the SNR(f) values # 1 #0 #SCStatus
xdsl2SCStatusSnrMtime1 DEFAULT 0 #Ds, the number of symbols used to measure the SNR(f) values # 1 #0 #SCStatus
xdsl2SCStatusSnrScGroupSize0 DEFAULT 0 #Us, Number of subcarriers per group used to report the SNR values # 1 #0 #SCStatus
xdsl2SCStatusSnrScGroupSize1 DEFAULT 0 #Ds, Number of subcarriers per group used to report the SNR values # 1 #0 #SCStatus
xdsl2SCStatusRowStatus0 DEFAULT 0 #Us, Row Status # 1 #0 #SCStatus
xdsl2SCStatusRowStatus1 DEFAULT 0 #Ds, Row Status # 1 #0 #SCStatus
xdsl2SCStatusAttainableRate0 DEFAULT 0 # # 1 #0 #SCStatus
xdsl2SCStatusAttainableRate1 DEFAULT 0 # # 1 #0 #SCStatus



------------------------      SCStatusBand      ------------------------

xdsl2SCStatusBand0 DEFAULT 0 #Us0 # 1 #0 #SCStatusBand
xdsl2SCStatusBand1 DEFAULT 0 #Us1 # 1 #0 #SCStatusBand
xdsl2SCStatusBand2 DEFAULT 0 #Us2 # 1 #0 #SCStatusBand
xdsl2SCStatusBand3 DEFAULT 0 #Us3 # 1 #0 #SCStatusBand
xdsl2SCStatusBand4 DEFAULT 0 #Us4 # 1 #0 #SCStatusBand
xdsl2SCStatusBand5 DEFAULT 0 #Ds1 # 1 #0 #SCStatusBand
xdsl2SCStatusBand6 DEFAULT 0 #Ds2 # 1 #0 #SCStatusBand
xdsl2SCStatusBand7 DEFAULT 0 #Ds3 # 1 #0 #SCStatusBand
xdsl2SCStatusBand8 DEFAULT 0 #Ds4 # 1 #0 #SCStatusBand
xdsl2SCStatusBand9 DEFAULT 0 #US all band # 1 #0 #SCStatusBand
xdsl2SCStatusBand10 DEFAULT 0 #dS all band # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten0 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten1 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten2 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten3 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten4 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten5 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten6 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten7 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten8 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten9 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandLnAtten10 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten0 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten1 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten2 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten3 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten4 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten5 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten6 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten7 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten8 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten9 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand
xdsl2SCStatusBandSigAtten10 DEFAULT 0 #measured difference in the total power transmitted by the xTU-C and the total power received by the xTU-R over all subcarriers during Showtime after the diagnostics mode # 1 #0 #SCStatusBand




------------------------      Linelnventory      ------------------------

xdsl2LInvUnit0 DEFAULT 0 #The termination unit xtuc{1} or xtur{2} # 1 #0 #Linelnventory
xdsl2LInvUnit1 DEFAULT 0 #The termination unit xtuc{1} or xtur{2} # 1 #0 #Linelnventory
xdsl2LInvG994VendorId0 DEBUG 0 #Us, G.994.1 Vendor ID # 1 #0#Linelnventory
xdsl2LInvG994VendorId1 DEBUG 0 #Ds, G.994.1 Vendor ID # 1 #0#Linelnventory
xdsl2LInvSystemVendorId0 DEBUG 0 #Us, ATU System Vendor ID # 1 #0#Linelnventory
xdsl2LInvSystemVendorId1 DEBUG 0 #Ds, ATU System Vendor ID # 1 #0#Linelnventory
xdsl2LInvVersionNumber0 DEFAULT 0 #Us, The xTU version number (vendor-specific information) # 1 #0 #Linelnventory
xdsl2LInvVersionNumber1 DEFAULT 0 #Ds, The xTU version number (vendor-specific information) # 1 #0 #Linelnventory
xdsl2LInvSerialNumber0 DEFAULT 0 #Us,The xTU serial number (vendor-specific information) # 1 #0 #Linelnventory
xdsl2LInvSerialNumber1 DEFAULT 0 #Ds,The xTU serial number (vendor-specific information) # 1 #0 #Linelnventory
xdsl2LInvSelfTestResult0 DEFAULT 0 #Us, xTU self-test result # 1 #0 #Linelnventory
xdsl2LInvSelfTestResult1 DEFAULT 0 #Ds, xTU self-test result # 1 #0 #Linelnventory
xdsl2LInvTransmissionCapabilities0 DEFAULT 0 #Us, xTU transmission system capability list of the different coding types # 1 #0 #Linelnventory
xdsl2LInvTransmissionCapabilities1 DEFAULT 0 #Ds, xTU transmission system capability list of the different coding types # 1 #0 #Linelnventory


------------------------      SCStatusSegment      ------------------------

xdsl2SCStatusSegment DEFAULT 0 # # 1 #0 #SCStatusSegment
xdsl2SCStatusSegmentLinReal DEFAULT 0 # # 1 #0 #SCStatusSegment
xdsl2SCStatusSegmentLinImg DEFAULT 0 # # 1 #0 #SCStatusSegment
xdsl2SCStatusSegmentLog DEFAULT 0 # # 1 #0 #SCStatusSegment
xdsl2SCStatusSegmentQln DEFAULT 0 # # 1 #0 #SCStatusSegment
xdsl2SCStatusSegmentSnr DEFAULT 0 # # 1 #0 #SCStatusSegment
xdsl2SCStatusSegmentBitsGainAlloc DEFAULT 0 # # 1 #0 #SCStatusSegment


------------------------      PMLineCurr      ------------------------

xdsl2PMLCurrUnit0 DEFAULT 0 #Us, The termination unit xtuc{1} or xtur{2} # 1 #0 #PMLineCurr
xdsl2PMLCurrUnit1 DEFAULT 0 #Ds, The termination unit xtuc{1} or xtur{2} # 1 #0 #PMLineCurr
xdsl2PMLCurr15MValidIntervals0 DEFAULT 0 #Us, Valid intervals # 1 #0 #PMLineCurr
xdsl2PMLCurr15MValidIntervals1 DEFAULT 0 #Ds, Valid intervals # 1 #0 #PMLineCurr
xdsl2PMLCurr15MInvalidIntervals0 DEFAULT 0 #Us, Invalid intervals # 1 #0 #PMLineCurr
xdsl2PMLCurr15MInvalidIntervals1 DEFAULT 0 #Ds, Invalid intervals # 1 #0 #PMLineCurr
xdsl2PMLCurr15MTimeElapsed0 DEFAULT 0 #Us, Total elapsed seconds in this interval # 1 #0 #PMLineCurr
xdsl2PMLCurr15MTimeElapsed1 DEFAULT 0 #Ds, Total elapsed seconds in this interval # 1 #0 #PMLineCurr
xdsl2PMLCurr15MFecs0 DEFAULT 0 #Us, Count of seconds during this interval that there was at least one FEC correction event # 1 #0 #PMLineCurr
xdsl2PMLCurr15MFecs1 DEFAULT 0 #Ds, Count of seconds during this interval that there was at least one FEC correction event # 1 #0 #PMLineCurr
xdsl2PMLCurr15MEs0 DEFAULT 0 #Us, Current 15M error second # 1 #0 #PMLineCurr
xdsl2PMLCurr15MEs1 DEFAULT 0 #Ds, Current 15M error second # 1 #0 #PMLineCurr
xdsl2PMLCurr15MSes0 DEFAULT 0 #Us, Current 15M SEs # 1 #0 #PMLineCurr
xdsl2PMLCurr15MSes1 DEFAULT 0 #Ds, Current 15M SEs # 1 #0 #PMLineCurr
xdsl2PMLCurr15MLoss0 DEFAULT 0 #Us, Current 15M LOSs # 1 #0 #PMLineCurr
xdsl2PMLCurr15MLoss1 DEFAULT 0 #Ds, Current 15M LOSs # 1 #0 #PMLineCurr
xdsl2PMLCurr15MUas0 DEFAULT 0 #Us, Current 15M Unavailability State # 1 #0 #PMLineCurr
xdsl2PMLCurr15MUas1 DEFAULT 0 #Ds, Current 15M Unavailability State # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayValidIntervals0 DEFAULT 0 #Us, Valid intervals # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayValidIntervals1 DEFAULT 0 #Ds, Valid intervals # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayInvalidIntervals0 DEFAULT 0 #Us, Invalid intervals # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayInvalidIntervals1 DEFAULT 0 #Ds, Invalid intervals # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayTimeElapsed0 DEFAULT 0 #Us, Total elapsed seconds in this interval # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayTimeElapsed1 DEFAULT 0 #Ds, Total elapsed seconds in this interval # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayFecs0 DEFAULT 0 #Us, 1 Day Fecs # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayFecs1 DEFAULT 0 #Ds, 1 Day Fecs # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayEs0 DEFAULT 0 #Us, 1 Day Es # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayEs1 DEFAULT 0 #Ds, 1 Day Es # 1 #0 #PMLineCurr
xdsl2PMLCurr1DaySes0 DEFAULT 0 #Us, 1 Day SEs # 1 #0 #PMLineCurr
xdsl2PMLCurr1DaySes1 DEFAULT 0 #Ds, 1 Day SEs # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayLoss0 DEFAULT 0 #Us, 1 Day LOSs # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayLoss1 DEFAULT 0 #Ds, 1 Day LOSs # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayUas0 DEFAULT 0 #Us, 1 Day Unavailability State # 1 #0 #PMLineCurr
xdsl2PMLCurr1DayUas1 DEFAULT 0 #Ds, 1 Day Unavailability State # 1 #0 #PMLineCurr



------------------------      PMLineInitCurr      ------------------------

xdsl2PMLInitCurr15MValidIntervals0 DEFAULT 0 #Us, Valid intervals # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MValidIntervals1 DEFAULT 0 #Ds, Valid intervals # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MInvalidIntervals0 DEFAULT 0 #Us, Invalid intervals # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MInvalidIntervals1 DEFAULT 0 #Ds, Invalid intervals # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MTimeElapsed0 DEFAULT 0 #Us, Total elapsed seconds in this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MTimeElapsed1 DEFAULT 0 #Ds, Total elapsed seconds in this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MFullInits0 METANOIA 0 #Us, Count of full initializations attempted on the line (successful and failed) during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MFullInits1 METANOIA 0 #Ds, Count of full initializations attempted on the line (successful and failed) during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MFailedFullInits0 METANOIA 0 #Us, Count of failed full initializations on the line during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MFailedFullInits1 METANOIA 0 #Ds, Count of failed full initializations on the line during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MShortInits0 DEFAULT 0 #Us, Count of short initializations attempted on the line (successful and failed) during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MShortInits1 DEFAULT 0 #Ds, Count of short initializations attempted on the line (successful and failed) during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MFailedShortInits0 DEFAULT 0 #Us, Count of failed short initializations on the line during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr15MFailedShortInits1 DEFAULT 0 #Ds, Count of failed short initializations on the line during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayValidIntervals0 DEFAULT 0 #Us, Valid intervals # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayValidIntervals1 DEFAULT 0 #Ds, Valid intervals # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayInvalidIntervals0 DEFAULT 0 #Us, Invalid intervals # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayInvalidIntervals1 DEFAULT 0 #Ds, Invalid intervals # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayTimeElapsed0 DEFAULT 0 #Us, Total elapsed seconds in this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayTimeElapsed1 DEFAULT 0 #Ds, Total elapsed seconds in this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayFullInits0 DEFAULT 0 #Us, Count of full initializations attempted on the line (successful and failed) during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayFullInits1 DEFAULT 0 #Ds, Count of full initializations attempted on the line (successful and failed) during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayFailedFullInits0 DEFAULT 0 #Us, Count of failed full initializations on the line during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayFailedFullInits1 DEFAULT 0 #Ds, Count of failed full initializations on the line during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayShortInits0 DEFAULT 0 #Us, Count of short initializations attempted on the line (successful and failed) during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayShortInits1 DEFAULT 0 #Ds, Count of short initializations attempted on the line (successful and failed) during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayFailedShortInits0 DEFAULT 0 #Us, Count of failed short initializations on the line during this interval # 1 #0 #PMLineInitCurr
xdsl2PMLInitCurr1DayFailedShortInits1 DEFAULT 0 #Ds, Count of failed short initializations on the line during this interval # 1 #0 #PMLineInitCurr


------------------------      PMChCurr      ------------------------

xdsl2PMChCurrUnit0 DEFAULT 0 #Us, The termination unit xtuc(1) or xtur(2) # 1 #0 #PMChCurr
xdsl2PMChCurrUnit1 DEFAULT 0 #The termination unit xtuc(1) or xtur(2) # 1 #0 #PMChCurr
xdsl2PMChCurrUnit2 DEFAULT 0 #Ds, The termination unit xtuc(1) or xtur(2) # 1 #0 #PMChCurr
xdsl2PMChCurrUnit3 DEFAULT 0 #The termination unit xtuc(1) or xtur(2) # 1 #0 #PMChCurr
xdsl2PMChCurr15MValidIntervals0 DEFAULT 0 #Us, Valid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr15MValidIntervals1 DEFAULT 0 #Valid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr15MValidIntervals2 DEFAULT 0 #Ds, Valid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr15MValidIntervals3 DEFAULT 0 #Valid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr15MInvalidIntervals0 DEFAULT 0 #Us, Invalid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr15MInvalidIntervals1 DEFAULT 0 #Invalid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr15MInvalidIntervals2 DEFAULT 0 #Ds, Invalid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr15MInvalidIntervals3 DEFAULT 0 #Invalid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr15MTimeElapsed0 DEFAULT 0 #Us, Total elapsed seconds in this interval # 1 #0 #PMChCurr
xdsl2PMChCurr15MTimeElapsed1 DEFAULT 0 #Total elapsed seconds in this interval # 1 #0 #PMChCurr
xdsl2PMChCurr15MTimeElapsed2 DEFAULT 0 #Ds, Total elapsed seconds in this interval # 1 #0 #PMChCurr
xdsl2PMChCurr15MTimeElapsed3 DEFAULT 0 #Total elapsed seconds in this interval # 1 #0 #PMChCurr
xdsl2PMChCurr15MCodingViolations0 METANOIA 0 #Us, CRC counter # 1 #1#PMChCurr
xdsl2PMChCurr15MCodingViolations1 METANOIA 0 # CRC counter # 1 #1#PMChCurr
xdsl2PMChCurr15MCodingViolations2 METANOIA 0 #Ds, CRC counter # 1 #1#PMChCurr
xdsl2PMChCurr15MCodingViolations3 METANOIA 0 # CRC counter # 1 #1#PMChCurr
xdsl2PMChCurr15MCorrectedBlocks0 METANOIA 0 #Us, error correction counter # 1 #1#PMChCurr
xdsl2PMChCurr15MCorrectedBlocks1 METANOIA 0 # error correction counter # 1 #1#PMChCurr
xdsl2PMChCurr15MCorrectedBlocks2 METANOIA 0 #Ds, error correction counter # 1 #1#PMChCurr
xdsl2PMChCurr15MCorrectedBlocks3 METANOIA 0 # error correction counter # 1 #1#PMChCurr
xdsl2PMChCurr1DayValidIntervals0 DEFAULT 0 #Us, Valid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr1DayValidIntervals1 DEFAULT 0 #Valid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr1DayValidIntervals2 DEFAULT 0 #Ds, Valid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr1DayValidIntervals3 DEFAULT 0 #Valid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr1DayInvalidIntervals0 DEFAULT 0 #Us, Invalid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr1DayInvalidIntervals1 DEFAULT 0 #Invalid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr1DayInvalidIntervals2 DEFAULT 0 #Ds, Invalid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr1DayInvalidIntervals3 DEFAULT 0 #Invalid intervals # 1 #0 #PMChCurr
xdsl2PMChCurr1DayTimeElapsed0 DEFAULT 0 #Us, Total elapsed seconds in this interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayTimeElapsed1 DEFAULT 0 #Total elapsed seconds in this interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayTimeElapsed2 DEFAULT 0 #Ds, Total elapsed seconds in this interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayTimeElapsed3 DEFAULT 0 #Total elapsed seconds in this interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayCodingViolations0 DEFAULT 0 #Us, Count of CRC-8 (FEBE for xTU-R) anomalies occurring in the channel during the interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayCodingViolations1 DEFAULT 0 #Count of CRC-8 (FEBE for xTU-R) anomalies occurring in the channel during the interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayCodingViolations2 DEFAULT 0 #Ds, Count of CRC-8 (FEBE for xTU-R) anomalies occurring in the channel during the interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayCodingViolations3 DEFAULT 0 #Count of CRC-8 (FEBE for xTU-R) anomalies occurring in the channel during the interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayCorrectedBlocks0 DEFAULT 0 #Us, Count of FEC (FFEC for xTU-R) anomalies (corrected code words) occurring in the channel during the interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayCorrectedBlocks1 DEFAULT 0 #Count of FEC (FFEC for xTU-R) anomalies (corrected code words) occurring in the channel during the interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayCorrectedBlocks2 DEFAULT 0 #Ds, Count of FEC (FFEC for xTU-R) anomalies (corrected code words) occurring in the channel during the interval # 1 #0 #PMChCurr
xdsl2PMChCurr1DayCorrectedBlocks3 DEFAULT 0 #Count of FEC (FFEC for xTU-R) anomalies (corrected code words) occurring in the channel during the interval # 1 #0 #PMChCurr






------------------------      LineConfProf      ------------------------

xdsl2LConfProfRaModeDs DEFAULT 0 #Us Ra mode { manual(1), raInit (2), dynamicRa(3) # 1 #0 #LineConfProf
xdsl2LConfProfRaModeUs DEFAULT 0 #Ds Ra mode { manual(1), raInit (2), dynamicRa(3) # 1 #0 #LineConfProf
xdsl2LConfProfRaUsNrmDs DEFAULT 0 #Downstream Up-Shift Noise Margin value(0.1dB) # 1 #0 #LineConfProf
xdsl2LConfProfRaUsNrmUs DEFAULT 0 #Upstream Up-Shift Noise Margin value(0.1dB) # 1 #0 #LineConfProf
xdsl2LConfProfRaUsTimeDs DEFAULT 0 #The Downstream Up-Shift Time Interval(second) # 1 #0 #LineConfProf
xdsl2LConfProfRaUsTimeUs DEFAULT 0 #The Upstream Up-Shift Time Interval(second) # 1 #0 #LineConfProf
xdsl2LConfProfRaDsNrmDs DEFAULT 0 #The Downstream Down-Shift Noise Margin value(0.1dB) # 1 #0 #LineConfProf
xdsl2LConfProfRaDsNrmUs DEFAULT 0 #The Upstream Down-Shift Noise Margin value(0.1dB) # 1 #0 #LineConfProf
xdsl2LConfProfRaDsTimeDs DEFAULT 0 #The Downstream Downshift Time Interval(second) # 1 #0 #LineConfProf
xdsl2LConfProfRaDsTimeUs DEFAULT 0 #The Upstream Downshift Time Interval(second) # 1 #0 #LineConfProf
xdsl2LConfProfTargetSnrmDs METANOIA 0 #DS target SNR margin # 1 #1 #LineConfProf
xdsl2LConfProfTargetSnrmUs METANOIA 0 #US target SNR margin # 1 #1 #LineConfProf
xdsl2LConfProfMaxSnrmDs DEFAULT 0 #The maximum Noise Margin the xTU-R receiver shall try to sustain(0.1dB) # 1 #0 #LineConfProf
xdsl2LConfProfMaxSnrmUs DEFAULT 0 #The maximum Noise Margin the xTU-C receiver shall try to sustain(0.1dB) # 1 #0 #LineConfProf
xdsl2LConfProfMinSnrmDs DEFAULT 0 #The minimum Noise Margin the xTU-R receiver shall tolerate(0.1dB) # 1 #0 #LineConfProf
xdsl2LConfProfMinSnrmUs DEFAULT 0 #The minimum Noise Margin the xTU-C receiver shall tolerate(0.1dB) # 1 #0 #LineConfProf
xdsl2LConfProfMsgMinUs DEFAULT 0 #Minimum Overhead Rate Upstream(kbits/second) # 1 #0 #LineConfProf
xdsl2LConfProfMsgMinDs DEFAULT 0 #Minimum Overhead Rate Downstream(kbits/second) # 1 #0 #LineConfProf
xdsl2LConfProfCeFlag DEFAULT 0 #This parameter is a bit that enables the use of the optional cyclic extension values{disable(0),enable(1)} # 1 #0 #LineConfProf
xdsl2LConfProfSnrModeDs DEFAULT 0 #This parameter enables the transmitter referred virtual noise in the downstream direction{disable(0),enable(1)} # 1 #0 #LineConfProf
xdsl2LConfProfSnrModeUs DEFAULT 0 #This parameter enables the transmitter referred virtual noise in the upstream direction{disable(0),enable(1)} # 1 #0 #LineConfProf
xdsl2LConfProfTxRefVnDs DEFAULT 0 #This configuration parameter defines the downstream transmitter referred virtual noise # 1 #0 #LineConfProf
xdsl2LConfProfTxRefVnUs DEFAULT 0 #This configuration parameter defines the upstream transmitter referred virtual noise # 1 #0 #LineConfProf
xdsl2LConfProfXtuTransSysEna DEFAULT 0 #This configuration parameter defines the upstream transmitter referred virtual noise # 1 #0 #LineConfProf
xdsl2LConfProfPmMode DEFAULT 0 #Power management state Enabling (PMMode){allowTransitionsToIdle(0),allowTransitionsToLowPower(1) # 1 #0 #LineConfProf
xdsl2LConfProfL0Time DEFAULT 0 #The minimum time (in seconds) between an Exit from the L2 state and the next Entry into the L2 state(second) # 1 #0 #LineConfProf
xdsl2LConfProfL2Time DEFAULT 0 #The minimum time (in seconds) between an Entry into the L2 state and the first Power Trim in the L2 state and between two consecutive Power Trims in the L2 State(second) # 1 #0 #LineConfProf
xdsl2LConfProfL2Atpr DEFAULT 0 #The maximum aggregate transmit power reduction (in dB) that can be performed at transition of L0 to L2 state # 1 #0 #LineConfProf
xdsl2LConfProfL2Atprt DEFAULT 0 #The total maximum aggregate transmit power reduction (in dB) that can be performed in an L2 state(dB) # 1 #0 #LineConfProf
xdsl2LConfProfProfiles METANOIA 0 #The configuration parameter contains the G.993.2 profiles to be allowed by the near-end xTU on this line # 1 #1 #LineConfProf
xdsl2LConfProfDpboEPsd DEFAULT 0 #This configuration parameter defines the PSD mask that is assumed to be permitted at the exchange # 1 #0 #LineConfProf
xdsl2LConfProfDpboEsEL DEFAULT 0 #This configuration parameter defines the assumed electrical length of cables(0.5dB) # 1 #0 #LineConfProf
xdsl2LConfProfDpboEsCableModelA DEFAULT 0 #The E-side Cable Model parameter A (DPBOESCMA) of the cable model (DPBOESCM) # 1 #0 #LineConfProf
xdsl2LConfProfDpboEsCableModelB DEFAULT 0 #The E-side Cable Model parameter B (DPBOESCMA) of the cable model (DPBOESCM) # 1 #0 #LineConfProf
xdsl2LConfProfDpboEsCableModelC DEFAULT 0 #The E-side Cable Model parameter C (DPBOESCMA) of the cable model (DPBOESCM) # 1 #0 #LineConfProf
xdsl2LConfProfDpboMus DEFAULT 0 #This configuration parameter defines the assumed Minimum Usable receive PSD mask (in dBm/Hz) # 1 #0 #LineConfProf
xdsl2LConfProfDpboFMin DEFAULT 0 #This configuration parameter defines the minimum frequency from which the DPBO shall be applied.(4.1234 kHz) # 1 #0 #LineConfProf
xdsl2LConfProfDpboFMax DEFAULT 0 #This configuration parameter defines the maximum frequency at which DPBO may be applied(4.3125kHz) # 1 #0 #LineConfProf
xdsl2LConfProfUpboKL DEFAULT 0 #This configuration parameter defines the electrical length expressed in dB at 1MHz(0.1dB) # 1 #0 #LineConfProf
xdsl2LConfProfUpboKLF DEFAULT 0 #Defines the upstream power backoff force mode.{auto(1), override(2),disableUpbo(3)} # 1 #0 #LineConfProf
xdsl2LConfProfUs0Mask DEFAULT 0 #US0 PSD masks to be allowed by the near-end xTU on the line # 1 #0 #LineConfProf
xdsl2LConfProfForceInp DEFAULT 0 #indicates that the framer settings of the bearer # 1 #0 #LineConfProf
xdsl2LConfProfRowStatus DEFAULT 0 #Row Status # 1 #0 #LineConfProf
xdsl2LConfProfVdsl2CarMask BANDPLAN 2 #Conf band plan # 1 #0 #LineConfProf
xdsl2LConfProfPsdMaskDs BANDPLAN 2 #Conf DS PSD mask # 1 #0 #LineConfProf
xdsl2LConfProfPsdMaskUs BANDPLAN 2 #Conf US PSD mask # 1 #0 #LineConfProf
xdsl2LConfProfVdsl2CarMask BANDPLAN 2 #Conf band plan # 1 #0 #LineConfProf
xdsl2LConfProfRfiBands DEFAULT 0 # # 1 #0 #LineConfProf



------------------------      CHConfProfile      ------------------------
xdsl2ChConfProfProfileName0 DEFAULT 0 # # 1 #0 #ChConfProfile
xdsl2ChConfProfMinDataRateDs0 METANOIA 0 # config min data rate DS # 1 #1 #ChConfProfile
xdsl2ChConfProfMinDataRateUs0 METANOIA 0 # config min data rate US # 1 #1 #ChConfProfile
xdsl2ChConfProfMinResDataRateDs0 DEFAULT 0 #Minimum Reserved Data Rate on Downstream direction(kbps) # 1 #0 #ChConfProfile
xdsl2ChConfProfMinResDataRateUs0 DEFAULT 0 #Minimum Reserved Data Rate on Upstream direction(kbps) # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxDataRateDs0 METANOIA 0 #Conf DS max data rate # 1 #1 #ChConfProfile
xdsl2ChConfProfMaxDataRateUs0 METANOIA 0 #Conf US max data rate # 1 #1 #ChConfProfile
xdsl2ChConfProfMinDataRateLowPwrDs0 DEFAULT 0 #minimum Downstream net data rate for the bearer channel as desired by the operator of the system during the low power state L1/L2(kbps) # 1 #0 #ChConfProfile
xdsl2ChConfProfMinDataRateLowPwrUs0 DEFAULT 0 #minimum Upstream net data rate for the bearer channel as desired by the operator of the system during the low power state L1/L2(kbps) # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxDelayDs0 METANOIA 0 #Conf DS max network delay(ms) # 1 #1 #ChConfProfile
xdsl2ChConfProfMaxDelayUs0 METANOIA 0 #Conf US max network delay(ms) # 1 #1 #ChConfProfile
xdsl2ChConfProfMinProtectionDs0 METANOIA 0 #Conf DS minimum impulse noise protection in 4.3125kHz(symbol), in 8a-17a # 1 #1 #ChConfProfile
xdsl2ChConfProfMinProtectionUs0 METANOIA 0 #Conf US minimum impulse noise protection in 4.3125kHz(symbol), in 8a-17a # 1 #1 #ChConfProfile
xdsl2ChConfProfMinProtection8Ds0 METANOIA 0 #Conf Ds minimum impulse noise protection in 8.625kHz(symbol), in 30a # 1 #1 #ChConfProfile
xdsl2ChConfProfMinProtection8Us0 METANOIA 0 #Conf Us minimum impulse noise protection in 8.625kHz(symbol), in 30a # 1 #1 #ChConfProfile
xdsl2ChConfProfMaxBerDs0 DEFAULT 0 #Maximum Bit Error Ratio on Downstream direction # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxBerUs0 DEFAULT 0 #Maximum Bit Error Ratio on Upstream direction # 1 #0 #ChConfProfile
xdsl2ChConfProfUsDataRateDs0 DEFAULT 0 #Data Rate Threshold Upshift for downstream direction(bps) # 1 #0 #ChConfProfile
xdsl2ChConfProfDsDataRateDs0 DEFAULT 0 #Data Rate Threshold Downshift for downstream direction(bps) # 1 #0 #ChConfProfile
xdsl2ChConfProfUsDataRateUs0 DEFAULT 0 #Data Rate Threshold Upshift for upstream direction(bps) # 1 #0 #ChConfProfile
xdsl2ChConfProfDsDataRateUs0 DEFAULT 0 #Data Rate Threshold Downshift for upstream direction(bps) # 1 #0 #ChConfProfile
xdsl2ChConfProfImaEnabled0 DEFAULT 0 #IMA Mode Enable # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxDelayVarDs0 DEFAULT 0 #Ds, aximum delay variation (DVMAX) # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxDelayVarUs0 DEFAULT 0 #Us, aximum delay variation (DVMAX) # 1 #0 #ChConfProfile
xdsl2ChConfProfInitPolicy0 DEFAULT 0 #Channel Initialization Policy Selection (CIPOLICY) # 1 #0 #ChConfProfile
xdsl2ChConfProfRowStatus0 DEFAULT 0 #Row Status # 1 #0 #ChConfProfile
xdsl2ChConfProfProfileName1 DEFAULT 0 # # 1 #0 #ChConfProfile
xdsl2ChConfProfMinDataRateDs1 METANOIA 0 # config min data rate DS # 1 #1 #ChConfProfile
xdsl2ChConfProfMinDataRateUs1 METANOIA 0 # config min data rate US # 1 #1 #ChConfProfile
xdsl2ChConfProfMinResDataRateDs1 DEFAULT 0 #Minimum Reserved Data Rate on Downstream direction(kbps) # 1 #0 #ChConfProfile
xdsl2ChConfProfMinResDataRateUs1 DEFAULT 0 #Minimum Reserved Data Rate on Upstream direction(kbps) # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxDataRateDs1 METANOIA 0 #Conf DS max data rate # 1 #1 #ChConfProfile
xdsl2ChConfProfMaxDataRateUs1 METANOIA 0 #Conf US max data rate # 1 #1 #ChConfProfile
xdsl2ChConfProfMinDataRateLowPwrDs1 DEFAULT 0 #minimum Downstream net data rate for the bearer channel as desired by the operator of the system during the low power state L1/L2(kbps) # 1 #0 #ChConfProfile
xdsl2ChConfProfMinDataRateLowPwrUs1 DEFAULT 0 #minimum Upstream net data rate for the bearer channel as desired by the operator of the system during the low power state L1/L2(kbps) # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxDelayDs1 METANOIA 0 #Conf DS max network delay(ms) # 1 #1 #ChConfProfile
xdsl2ChConfProfMaxDelayUs1 METANOIA 0 #Conf US max network delay(ms) # 1 #1 #ChConfProfile
xdsl2ChConfProfMinProtectionDs1 METANOIA 0 #Conf DS minimum impulse noise protection in 4.3125kHz(symbol), in 8a-17a # 1 #1 #ChConfProfile
xdsl2ChConfProfMinProtectionUs1 METANOIA 0 #Conf US minimum impulse noise protection in 4.3125kHz(symbol), in 8a-17a # 1 #1 #ChConfProfile
xdsl2ChConfProfMinProtection8Ds1 METANOIA 0 #Conf Ds minimum impulse noise protection in 8.625kHz(symbol), in 30a # 1 #1 #ChConfProfile
xdsl2ChConfProfMinProtection8Us1 METANOIA 0 #Conf Us minimum impulse noise protection in 8.625kHz(symbol), in 30a # 1 #1 #ChConfProfile
xdsl2ChConfProfMaxBerDs1 DEFAULT 0 #Maximum Bit Error Ratio on Downstream direction # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxBerUs1 DEFAULT 0 #Maximum Bit Error Ratio on Upstream direction # 1 #0 #ChConfProfile
xdsl2ChConfProfUsDataRateDs1 DEFAULT 0 #Data Rate Threshold Upshift for downstream direction(bps) # 1 #0 #ChConfProfile
xdsl2ChConfProfDsDataRateDs1 DEFAULT 0 #Data Rate Threshold Downshift for downstream direction(bps) # 1 #0 #ChConfProfile
xdsl2ChConfProfUsDataRateUs1 DEFAULT 0 #Data Rate Threshold Upshift for upstream direction(bps) # 1 #0 #ChConfProfile
xdsl2ChConfProfDsDataRateUs1 DEFAULT 0 #Data Rate Threshold Downshift for upstream direction(bps) # 1 #0 #ChConfProfile
xdsl2ChConfProfImaEnabled1 DEFAULT 0 #IMA Mode Enable # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxDelayVarDs1 DEFAULT 0 #Ds, aximum delay variation (DVMAX) # 1 #0 #ChConfProfile
xdsl2ChConfProfMaxDelayVarUs1 DEFAULT 0 #Us, aximum delay variation (DVMAX) # 1 #0 #ChConfProfile
xdsl2ChConfProfInitPolicy1 DEFAULT 0 #Channel Initialization Policy Selection (CIPOLICY) # 1 #0 #ChConfProfile
xdsl2ChConfProfRowStatUs1 DEFAULT 0 #Row Status # 1 #0 #ChConfProfile





------------------------      LineAlarmConfProfile      ------------------------

xdsl2LineAlarmConfProfileName DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXtucThresh15MinFecs DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXtucThresh15MinEs DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXtucThresh15MinSes DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXtucThresh15MinLoss DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXtucThresh15MinUas DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXturThresh15MinFecs DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXturThresh15MinEs DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXturThresh15MinSes DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXturThresh15MinLoss DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileXturThresh15MinUas DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileThresh15MinFailedFullInt DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileThresh15MinFailedShrtInt DEFAULT 0 # # 1 #0 #LineAlarmConfProfile
xdsl2LineAlarmConfProfileRowStatus DEFAULT 0 # # 1 #0 #LineAlarmConfProfile








------------------------      ChAlarmConfProfile      ------------------------


xdsl2ChAlarmConfProfileName DEFAULT 0 # # 1 #0 #ChAlarmConfProfile
xdsl2ChAlarmConfProfileXtucThresh15MinCodingViolations DEFAULT 0 #A threshold for the xdsl2PMChCurr15MCodingViolations Counter # 1 #0 #ChAlarmConfProfile
xdsl2ChAlarmConfProfileXtucThresh15MinCorrected DEFAULT 0 #A threshold for the xdsl2PMChCurr15MCorrectedBlocks Counter # 1 #0 #ChAlarmConfProfile
xdsl2ChAlarmConfProfileXturThresh15MinCodingViolations DEFAULT 0 #A threshold for the xdsl2PMChCurr15MCodingViolations Counter # 1 #0 #ChAlarmConfProfile
xdsl2ChAlarmConfProfileXturThresh15MinCorrected DEFAULT 0 #A threshold for the xdsl2PMChCurr15MCorrectedBlocks Counter # 1 #0 #ChAlarmConfProfile
xdsl2ChAlarmConfProfileRowStatus DEFAULT 0 #Row Status # 1 #0 #ChAlarmConfProfile





------------------------      Metanoia      ------------------------

xdslMetanoiaOtCurrLineRate DEFAULT 0 #UpStream line rate (kbps) # 1 #0 #Metanoia
xdslMetanoiaRtCurrLineRate DEFAULT 0 #DownStream line rate (kbps) # 1 #0 #Metanoia
xdslMetanoiaOtInits DEFAULT 0 #UpStream initial counter # 1 #0 #Metanoia
xdslMetanoiaRtInits DEFAULT 0 #DownStream initial counter # 1 #0 #Metanoia
xdslMetanoiaOtCodingViolations0 METANOIA 0 # US CRC counter this showtime # 1 #0#Metanoia
xdslMetanoiaRtCodingViolations0 METANOIA 0 # DS CRC counter this showtime # 1 #0#Metanoia
xdslTwConfig DEFAULT 0 #Config setting # 1 #0 #Metanoia
VisibleDsPbs BANDPLAN 0 #DownStream target SNR setting(0.1dB) # 1 #0#Metanoia
VisibleUsPbs BANDPLAN 0 #UpStream target SNR setting(0.1dB) # 1 #0#Metanoia
VisibleDsTones BANDPLAN 0 #Current DsTones # 1 #0#Metanoia
VisibleUsTones BANDPLAN 0 #Current UsTones # 1 #0#Metanoia
VisibleDsPb0Tones BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb0FirstTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb0LastTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb1Tones BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb1FirstTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb1LastTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb2Tones BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb2FirstTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb2LastTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb3Tones BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb3FirstTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleDsPb3LastTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb0Tones BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb0FirstTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb0LastTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb1Tones BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb1FirstTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb1LastTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb2Tones BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb2FirstTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb2LastTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb3Tones BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb3FirstTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb3LastTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb4FirstTone BANDPLAN 0 # # 1 #0#Metanoia
VisibleUsPb4LastTone BANDPLAN 0 # # 1 #0#Metanoia
xdslGhsOtVendorId DEBUG 0 #CO vendor ID # 1 #0#Metanoia
xdslGhsRtVendorId DEBUG 0 #CPE vendor ID # 1 #0#Metanoia
xdslOtFirmwareVer DEFAULT 0 # # 1 #0 #Metanoia
xdslRtFirmwareVer DEFAULT 0 # # 1 #0 #Metanoia
DrsCwHist0AccCorr DEFAULT 0 #Receive path error corrected counter # 1 #0 #Metanoia
DrsCwHist1AccCorr DEFAULT 0 #Receive path error corrected counter # 1 #0 #Metanoia
DrsCwHist0AccUnCorr DEFAULT 0 #Receive path error not corrected counter # 1 #0 #Metanoia
DrsCwHist1AccUnCorr DEFAULT 0 #Receive path error not corrected counter # 1 #0 #Metanoia
IntCrcErrsD METANOIA 0 #Receive CRC counter # 1 #1 #Metanoia
vdslOtPerfDataInits METANOIA 0 #connection success counter # 1 #1#Metanoia
vdslRtPerfDataInits METANOIA 0 #connection success counter # 1 #1#Metanoia
vdslTwConfig METANOIA 2 #bit 4: report packet activities in LED 0 # 1 #1#Metanoia
vdslOtPhysCurrSnrMgn METANOIA 0 #Current DownStream Snr Mgn # 1 #1#Metanoia
vdslRtPhysCurrSnrMgn METANOIA 0 #Current DownStream Snr Mgn # 1 #1#Metanoia



